;------------------------------------------------------------------------
;   A88VidBB.inf
;
;       This file contains installation inforamtion for video capture 
;       driver of AVerMedia's TV tuner card.
;
;   Copyright and Disclaimer:
;       
;       This software is provided "as is" without warranty of any kind,
;       either expressed or implied, including but not limited to the
;       implied warranties of merchantability and/or fitness for a
;       particular purpose.
; 
;       Copyright (c) 2001-2004 AVerMedia Technologies, Inc.
;       All Rights Reserved.
;
;------------------------------------------------------------------------

[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider="AVerMedia"
DriverVer=03/03/2005,1.0.6.14
CatalogFile=A88VidBB.cat

[Manufacturer]
"AVerMedia"=AVerMedia

[SourceDisksNames]
1="AVerMedia M150 H/W MPEG Card Drivers",,,""

[SourceDisksFiles]
A88VidBB.sys=1
cxtvrate.dll=1

[AVerMedia]
;----------------------------------------------------------------------------------------
; M150 Series
;----------------------------------------------------------------------------------------
%CX23880.videoNTSC%        = CX23880.Blackbird,         PCI\VEN_14F1&DEV_8800&SUBSYS_C0111461 ;M150, NTSC
%CX23880.videoNTSC%        = CX23880.Blackbird,         PCI\VEN_14F1&DEV_8810&SUBSYS_C0111461 ;M150, NTSC
%CX23880.videoNTSC%        = CX23880.Blackbird,         PCI\VEN_14F1&DEV_8800&SUBSYS_C1111461 ;M150, FIC, NTSC
%CX23880.videoNTSC%        = CX23880.Blackbird,         PCI\VEN_14F1&DEV_8810&SUBSYS_C1111461 ;M150, FIC, NTSC
%CX23880.videoPAL%         = CX23880.Blackbird_Pal,     PCI\VEN_14F1&DEV_8800&SUBSYS_C00B1461 ;M150, Europe
%CX23880.videoPAL%         = CX23880.Blackbird_Pal,     PCI\VEN_14F1&DEV_8810&SUBSYS_C00B1461 ;M150, Europe
%CX23880.videoPAL%         = CX23880.Blackbird_Pal,     PCI\VEN_14F1&DEV_8800&SUBSYS_C10B1461 ;M150, FIC, Europe
%CX23880.videoRUS%         = CX23880.Blackbird_Rus,     PCI\VEN_14F1&DEV_8800&SUBSYS_C1151461 ;M150, FIC, Russia
%CX23880.videoJAPAN%       = CX23880.Blackbird_JAP,     PCI\VEN_14F1&DEV_8800&SUBSYS_C00E1461 ;M150, NTSC-J
%CX23880.videoJAPAN%       = CX23880.Blackbird_JAP,     PCI\VEN_14F1&DEV_8810&SUBSYS_C00E1461 ;M150, NTSC-J
%CX23880.videoJAPAN%       = CX23880.Blackbird_JAP_FIC, PCI\VEN_14F1&DEV_8800&SUBSYS_C1161461 ;M150, FIC, NTSC-J
%CX23880.videoJAPAN%       = CX23880.Blackbird_JAP_FIC, PCI\VEN_14F1&DEV_8810&SUBSYS_C1161461 ;M150, FIC, NTSC-J

;----------------------------------------------------------------------------------------
; M183 Series
;----------------------------------------------------------------------------------------
%CX23880.videoNTSC%        = CX23880.M183,              PCI\VEN_14F1&DEV_8800&SUBSYS_C2111461 ;M183, NTSC
%CX23880.videoNTSC%        = CX23880.M183,              PCI\VEN_14F1&DEV_8810&SUBSYS_C2111461 ;M183, NTSC
%CX23880.videoNTSC%        = CX23880.M183_JAP_A,        PCI\VEN_14F1&DEV_8800&SUBSYS_C2161461 ;M183, NTSC-J
%CX23880.videoNTSC%        = CX23880.M183_JAP_A,        PCI\VEN_14F1&DEV_8810&SUBSYS_C2161461 ;M183, NTSC-J
%CX23880.videoPAL%         = CX23880.M183_Pal,          PCI\VEN_14F1&DEV_8800&SUBSYS_C20B1461 ;M183, PAL
%CX23880.videoPAL%         = CX23880.M183_Pal,          PCI\VEN_14F1&DEV_8810&SUBSYS_C20B1461 ;M183, PAL

;----------------------------------------------------------------------------------------
; M15F Series
;----------------------------------------------------------------------------------------
%CX23880.videoJAPAN%       = CX23880.M15F_JAP,          PCI\VEN_14F1&DEV_8800&SUBSYS_C30C1461 ;M15F, Buffalo, Japan
%CX23880.videoJAPAN%       = CX23880.M15F_JAP,          PCI\VEN_14F1&DEV_8810&SUBSYS_C30C1461 ;M15F, Buffalo, Japan

;----------------------------------------------------------------------------------------
; Engineering Model
;----------------------------------------------------------------------------------------
;%CX23880.video%           = CX23880.Blackbird,     PCI\VEN_14F1&DEV_8800
;%CX23880.video%           = CX23880.Blackbird,     PCI\VEN_14F1&DEV_8810

[DestinationDirs]
CX23880.CopyDrivers=10,system32\drivers
CX23880.CopyFilters=11

[CX23880.CopyDrivers]
A88VidBB.sys

[CX23880.CopyFilters]
cxtvrate.dll

;------------------------------------------------------------------------
; NTSC System, Philips 1236MK3 Tuner
;------------------------------------------------------------------------
[CX23880.Blackbird]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration, KSCAPTUR.Registration.NT, MSPCLOCK.Installation
AddReg=     CX23880.AddReg, Blackbird_Common.AddReg, Blackbird.AddReg
CopyFiles=  CX23880.CopyDrivers, CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; Enable TvRating

[Blackbird.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
; Enable Macrovision Obfuscation
HKR,"DriverData","EncoderMVDRM",         0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Pll27",                0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","DisableAutoBlueScreen",0x00010001, 0x01, 0x00, 0x00, 0x00

HKR,"ENUM\Device1",pnpid,,"cxtune.VEN_14F1.PhilipsMK3"
HKR,"ENUM\Device2",pnpid,,"cx88xbar.VEN_14F1.cnxt"

[CX23880.Blackbird.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.Blackbird.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

;------------------------------------------------------------------------
; NTSC-J System, Philips 1286MK3 Tuner, for Japan
;------------------------------------------------------------------------
[CX23880.Blackbird_JAP]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
;AddReg=     CX23880.AddReg, Blackbird_Common.AddReg, PhilipsNTSCJ.AddReg
AddReg=     CX23880.AddReg, Blackbird_Common.AddReg, Blackbird_JAP.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; Enable TvRating

[Blackbird_JAP.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x02,0x00,0x00,0x00
; Country code is Japan = 81
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x51,0x00,0x00,0x00
; Enable Macrovision Obfuscation
HKR,"DriverData","EncoderMVDRM",         0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Pll27",                0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","DisableAutoBlueScreen",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","ColorKillEnable",      0x00010001, 0x01, 0x00, 0x00, 0x00 

HKR,"ENUM\Device1",pnpid,,"cxtune.VEN_14F1.PhilipsFI1286MK3"
HKR,"ENUM\Device2",pnpid,,"cx88xbar.VEN_14F1.cnxt"

[CX23880.Blackbird_JAP.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.Blackbird_JAP.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

;------------------------------------------------------------------------
; NTSC-J System, Philips 1236MK3 Tuner, for Japan
;------------------------------------------------------------------------
[CX23880.Blackbird_JAP_FIC]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg, Blackbird_Common.AddReg, Blackbird_JAP_FIC.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; Enable TvRating

[Blackbird_JAP_FIC.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x51,0x00,0x00,0x00
; Enable Macrovision Obfuscation
HKR,"DriverData","EncoderMVDRM",         0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Pll27",                0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","DisableAutoBlueScreen",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","ColorKillEnable",      0x00010001, 0x01, 0x00, 0x00, 0x00 

HKR,"ENUM\Device1",pnpid,,"cxtune.VEN_14F1.Philips_FM1236MK3_J"
HKR,"ENUM\Device2",pnpid,,"cx88xbar.VEN_14F1.cnxt"

[CX23880.Blackbird_JAP_FIC.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.Blackbird_JAP_FIC.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

;------------------------------------------------------------------------
; PAL System, Philips 1216MK3 Tuner
;------------------------------------------------------------------------
[CX23880.Blackbird_Pal]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration, KSCAPTUR.Registration.NT, MSPCLOCK.Installation
AddReg=     CX23880.AddReg, Blackbird_Common.AddReg, Blackbird_PAL.AddReg
CopyFiles=  CX23880.CopyDrivers, CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; Enable TvRating

[Blackbird_PAL.AddReg]
HKR,"DriverData","4in1Tuner",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
; Country code is Germany = 49
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x31,0x00,0x00,0x00
; Enable Macrovision Obfuscation
HKR,"DriverData","EncoderMVDRM",         0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Pll27",                0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","DisableAutoBlueScreen",0x00010001, 0x01, 0x00, 0x00, 0x00

HKR,"ENUM\Device1",pnpid,,"cxtune.VEN_14F1.philips4in1"
HKR,"ENUM\Device2",pnpid,,"cx88xbar.VEN_14F1.cnxt"

[CX23880.Blackbird_PAL.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.Blackbird_PAL.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

;------------------------------------------------------------------------
; Russia System, Philips 1256MK3 Tuner
;------------------------------------------------------------------------
[CX23880.Blackbird_RUS]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration, KSCAPTUR.Registration.NT, MSPCLOCK.Installation
AddReg=     CX23880.AddReg, Blackbird_Common.AddReg, Blackbird_RUS.AddReg
CopyFiles=  CX23880.CopyDrivers, CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; Enable TvRating

[Blackbird_RUS.AddReg]
HKR,"DriverData","4in1Tuner",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
; Country code is Russia = 7
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x07,0x00,0x00,0x00
; Enable Macrovision Obfuscation
HKR,"DriverData","EncoderMVDRM",         0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Pll27",                0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","DisableAutoBlueScreen",0x00010001, 0x01, 0x00, 0x00, 0x00

HKR,"ENUM\Device1",pnpid,,"A88Tune.VEN_1461.PhilipsFM1256MK3"
HKR,"ENUM\Device2",pnpid,,"cx88xbar.VEN_14F1.cnxt"

[CX23880.Blackbird_RUS.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.Blackbird_RUS.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

;------------------------------------------------------------------------
; M183 (Triple-Input Crossbar), NTSC
;------------------------------------------------------------------------
[CX23880.M183]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration, KSCAPTUR.Registration.NT, MSPCLOCK.Installation
AddReg=     CX23880.AddReg, Blackbird_Common.AddReg, M183.AddReg
CopyFiles=  CX23880.CopyDrivers, CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; Enable TvRating

[M183.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
; Disable Macrovision Obfuscation
HKR,"DriverData","EncoderMVDRM",         0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Pll27",                0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","DisableAutoBlueScreen",0x00010001, 0x01, 0x00, 0x00, 0x00

HKR,"ENUM\Device1",pnpid,,"cxtune.VEN_14F1.PhilipsMK3"
HKR,"ENUM\Device2",pnpid,,"cx88xbar.VEN_1461.TRI"

[CX23880.M183.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.M183.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

;------------------------------------------------------------------------
; M183 (Triple-Input Crossbar), NTSC-J (Philips 1236MK3 Tuner)
;------------------------------------------------------------------------
[CX23880.M183_JAP_A]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg, Blackbird_Common.AddReg, M183_JAP_A.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; Enable TvRating

[M183_JAP_A.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x02,0x00,0x00,0x00
; Country code is Japan = 81
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x51,0x00,0x00,0x00
; Disable Macrovision Obfuscation
HKR,"DriverData","EncoderMVDRM",         0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Pll27",                0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","DisableAutoBlueScreen",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","ColorKillEnable",      0x00010001, 0x01, 0x00, 0x00, 0x00 

HKR,"ENUM\Device1",pnpid,,"cxtune.VEN_14F1.Philips_FM1236MK3_J"
HKR,"ENUM\Device2",pnpid,,"cx88xbar.VEN_1461.TRI"

[CX23880.M183_JAP_A.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.M183_JAP_A.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

;------------------------------------------------------------------------
; M183 (Triple-Input Crossbar), PAL
;------------------------------------------------------------------------
[CX23880.M183_PAL]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration, KSCAPTUR.Registration.NT, MSPCLOCK.Installation
AddReg=     CX23880.AddReg, Blackbird_Common.AddReg, M183_PAL.AddReg
CopyFiles=  CX23880.CopyDrivers, CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; Enable TvRating

[M183_PAL.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
; Country code is Germany = 49
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x31,0x00,0x00,0x00
; Disable Macrovision Obfuscation
HKR,"DriverData","EncoderMVDRM",         0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Pll27",                0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","DisableAutoBlueScreen",0x00010001, 0x01, 0x00, 0x00, 0x00

HKR,"ENUM\Device1",pnpid,,"cxtune.VEN_14F1.philips4in1"
HKR,"ENUM\Device2",pnpid,,"cx88xbar.VEN_1461.TRI"

[CX23880.M183_PAL.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.M183_PAL.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

;------------------------------------------------------------------------
; M15F, Philips 1286MK2 Tuner (without FM)
;------------------------------------------------------------------------
[CX23880.M15F_JAP]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg, Blackbird_Common.AddReg, M15F_JAP.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; Enable TvRating

[M15F_JAP.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x51,0x00,0x00,0x00
; Disable Macrovision Obfuscation
HKR,"DriverData","EncoderMVDRM",         0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Pll27",                0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","DisableAutoBlueScreen",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","ColorKillEnable",      0x00010001, 0x01, 0x00, 0x00, 0x00 

HKR,"ENUM\Device1",pnpid,,"A88Tune.VEN_1461.PhilipsFI1286MK2"
HKR,"ENUM\Device2",pnpid,,"cx88xbar.VEN_1461.ONE"

[CX23880.M15F_JAP.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.M15F_JAP.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

;------------------------------------------------------------------------
; Common Sections
;------------------------------------------------------------------------
[TvRating.RegDLL]
11,,cxtvrate.dll,1

[CX23880.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,A88VidBB.sys
HKR,,OkToHibernate,3,01
HKR,,PageOutWhenUnopened,3,00
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKR,"DriverData","XBarInPin0",0x00010001, 0x03,0x00,0x00,0x00
HKR,"DriverData","XBarInPin1",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","XBarInPin2",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData","XBarInPin3",0x00010001, 0x00,0x10,0x00,0x00
HKR,"DriverData","XTal0",0x00010001, 0x1c, 0x00, 0x00, 0x00
HKR,"DriverData","XTal1",0x00010001, 0x23, 0x00, 0x00, 0x00
HKR,"DriverData","BobMode",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","VolumeLevelNegdB",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","UseExternalVPRES",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","UseI2SAsClock",0x00010001, 0x00, 0x00, 0x00, 0x00
HKLM,%MediaCategories%\%GUID.PINNAME_656_OUT%,Name,,%PinName.656_OUT%
HKLM,%MediaCategories%\%GUID.PINNAME_I2S_OUT%,Name,,%PinName.I2S_OUT%

[Blackbird_Common.AddReg]
HKR,"DriverData","VDelayOdd525",  0x00010001, 0x1C, 0x00, 0x00, 0x00
HKR,"DriverData","VDelayEven525", 0x00010001, 0x1C, 0x00, 0x00, 0x00
HKR,"DriverData","VActiveOdd525",  0x00010001, 0xe7, 0x01, 0x00, 0x00
HKR,"DriverData","VActiveEven525", 0x00010001, 0xe7, 0x01, 0x00, 0x00
HKR,"DriverData","Out656VDelayOdd525",  0x00010001, 0x26, 0x00, 0x00, 0x00
HKR,"DriverData","Out656VDelayEven525", 0x00010001, 0x26, 0x00, 0x00, 0x00

HKR,"DriverData","VDelayOdd625",  0x00010001, 0x26, 0x00, 0x00, 0x00
HKR,"DriverData","VDelayEven625", 0x00010001, 0x26, 0x00, 0x00, 0x00
HKR,"DriverData","VActiveOdd625",  0x00010001, 0x40, 0x02, 0x00, 0x00
HKR,"DriverData","VActiveEven625", 0x00010001, 0x40, 0x02, 0x00, 0x00
HKR,"DriverData","Out656VDelayOdd625",  0x00010001, 0x26, 0x00, 0x00, 0x00
HKR,"DriverData","Out656VDelayEven625", 0x00010001, 0x26, 0x00, 0x00, 0x00

HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
;Enable I2S out to encoder
HKR,"DriverData","WWAudioEnableI2SOut",0x00010001, 0x01,0x00,0x00,0x00
;I2S output format is Sony (1) 
HKR,"DriverData","WWAudioI2SOutFormat",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","WWAudioI2SFrequency",0x00010001, 0x80,0xBB,0x00,0x00
HKR,"DriverData","WWAudioMuteDACs"    ,0x00010001, 0x01,0x00,0x00,0x00

[VideoCapture]
AddReg=VideoCapture.AddReg

[VideoTvAudio]
AddReg=VideoTvAudio.AddReg

[VideoCapture.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%CX23880.friendly%

[VideoTvAudio.AddReg]
HKR,,CLSID,,{71F96462-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%CX23880.friendly2%

[CX23880.ServiceInstall]
DisplayName   = %CX23880.video%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_AUTO_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %10%\system32\drivers\A88VidBB.sys

[Strings]
CX23880.video            	= "AVerMedia AVerTV MPEG Video Capture (!)"
CX23880.videoNTSC        	= "AVerMedia AVerTV MPEG Video Capture"
CX23880.videoBlackbird   	= "AVerMedia AVerTV MPEG Video Capture (Blackbird)"
CX23880.videoJAPAN       	= "AVerMedia AVerTV MPEG Video Capture"
CX23880.videoPAL                = "AVerMedia AVerTV MPEG Video Capture"
CX23880.videoRUS                = "AVerMedia AVerTV MPEG Video Capture"
CX23880.null             	= "AVerMedia (unused device function)"
CX23880.friendly         	= "AVerMedia AVerTV MPEG Video Capture"
CX23880.friendly2        	= "AVerMedia AVerTV TvAudio"
;RunOnce                 	= "SOFTWARE\Microsoft\Windows\CurrentVersion\RunOnce"
SERVICE_KERNEL_DRIVER    	= 1
SERVICE_AUTO_START       	= 2
SERVICE_ERROR_NORMAL     	= 1

MediaCategories		 	= "SYSTEM\CurrentControlSet\Control\MediaCategories"
GUID.PINNAME_656_OUT     	= "{E2EEB283-EB84-4910-BABE-037FFBB03249}"
GUID.PINNAME_I2S_OUT     	= "{71A59578-46D2-4368-BEAF-062B0447565D}"
PinName.656_OUT          	= "MPEG Video"
PinName.I2S_OUT          	= "MPEG Audio"

