/*=============================================================================
   FILE:         ReadMe.txt
-------------------------------------------------------------------------------
   DESCRIPTION:  TerraTV WDM driver notes
   HISTORY:      25-Mar-2002
   NOTES:        
-------------------------------------------------------------------------------
   COPYRIGHT:    (c) 2000-02, TerraTec Electronic GmbH. All Rights Reserved.

                 Information in this file is the intellectual property of
                 TerraTec Electronic GmbH.
=============================================================================*/


NOTES:
--------
       

HISTORY:
--------
25-Mar-2002
    - Bugfix Tuner driver: augmented tuner range from 
      [55.25 MHz .. 801.250 MHz] to [48.25 MHz .. 855.25 MHz]
      This should fix the problem that stations above 800 MHz were not found during station scan
      (e.g. in Netherlands).

10-Feb-2002
    - Bugfix INF file: TerraTV was not found as VfW capture device

30-May-2001
    - Bugfix: PLL settings for TerraTV+ w/o EEPROM wer wrong
    - Added support for "TValue Radio"

13-Feb-2001 C.L.
    - Fixed Bug in bttuner.sys. Low Band was limited to 55.2 MHz 
      but ARD starts at 48.25 MHz

01-Feb-2001 C.L.
    - Added all functionality from Custom driver to Capture driver. Now we
      get rid of Custom driver and can use the same Driver Installation for all 
      Windows Plattforms
      
17-Jan-2001 C.L.
    - New Customproperty: Read/Write generic Register
    - Fixed: Driver crashes during W2K Installation
    - Fixed Bugs in BT848.INF
    - Crossbar & Tuner Filter could not be loaded on after installation 
      on clean system
    - Devices are shown twice in driver list

06-Nov-2000
    - Mute when driver is loaded
    - Added TerraTV audio functionality to BT848.sys
    - Modification to Crossbar device (BTXBAR.SYS):
         Two more audio inputs (CD,Radio), 
         Changed order of pins etc.
    - Simplified driver installation:
      Merged BTTUNER.INF and BTXBAR.INF into BT848.INF
    - Improved cropping for PAL

	





