; /****************************************************************************
; * Copyright 2006 Atheros Communications Inc., all rights reserved.          *
; * INF file for Atheros reference designs                                    *
; ****************************************************************************/

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHEROS%
LoutFiles   = layout.inf
CatalogFile = athrext.cat
DriverVer   = 04/27/2007,7.2.0.215


[Manufacturer]
%ATHEROS%     = Atheros, NTX86
%Gigabyte%     = GIGABYTE, NTX86

[ControlFlags]
ExcludeFromSelect = *


[Atheros.NTX86]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
;legacy HW Entries
%ATHR.DeviceDesc.1030%     = ATHR_DEV_1030.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1030168C
%ATHR.DeviceDesc.2030%     = ATHR_DEV_2030.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2030168C
%ATHR.DeviceDesc.1031%     = ATHR_DEV_1031.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1031168C
%ATHR.DeviceDesc.2031%     = ATHR_DEV_2031.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2031168C
%ATHR.DeviceDesc.1041%     = ATHR_DEV_1041.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1041168C
%ATHR.DeviceDesc.2041%     = ATHR_DEV_2041.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2041168C
%ATHR.DeviceDesc.1042%     = ATHR_DEV_1042.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1042168C
%ATHR.DeviceDesc.2042%     = ATHR_DEV_2042.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2042168C
%ATHR.DeviceDesc.1051%     = ATHR_DEV_1051.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1051168C
%ATHR.DeviceDesc.2051%     = ATHR_DEV_2051.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2051168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_1052.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_1052168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_2052.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_2052168C
%ATHR.DeviceDesc.1053%     = ATHR_DEV_1053.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1053168C
%ATHR.DeviceDesc.2053%     = ATHR_DEV_2053.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2053168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_1054.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_1054168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_2054.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_2054168C
%ATHR.DeviceDesc.1062%     = ATHR_DEV_1062.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_1062168C
%ATHR.DeviceDesc.2062%     = ATHR_DEV_2062.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_2062168C
%ATHR.DeviceDesc.001B%     = ATHR_DEV_1063.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_1063168C
%ATHR.DeviceDesc.001B%     = ATHR_DEV_2063.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_2063168C
%ATHR.DeviceDesc.3062%     = ATHR_DEV_2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_3062168c
%ATHR.DeviceDesc.3063%     = ATHR_DEV_2063.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_3063168c
%ATHR.DeviceDesc.3061%     = ATHR_DEV_2051.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_3061168c
%ATHR.DeviceDesc.3065%     = ATHR_DEV_2052.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_3065168c
%ATHR.DeviceDesc.2061%     = ATHR_DEV_2051.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_2061168c
%ATHR.DeviceDesc.1061%     = ATHR_DEV_1051.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_1061168c
%ATHR.DeviceDesc.2065%     = ATHR_DEV_2052.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_2065168c
%ATHR.DeviceDesc.1065%     = ATHR_DEV_1052.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_1065168c
%ATHR.DeviceDesc.3062%     = ATHR_DEV_2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_0086106B
%ATHR.DeviceDesc.0013%     = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_A527167D
%ATHR.DeviceDesc.001A%     = ATHR_DEV_001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7101144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7108144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7116144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7114144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7115144F
%ATHR.DeviceDesc.2041%     = ATHR_DEV_2041.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_7064144F
%ATHR.DeviceDesc.2042%     = ATHR_DEV_2042.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_7065144F
%ATHR.DeviceDesc.2051%     = ATHR_DEV_2051.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_7084144F
%ATHR.DeviceDesc.2051%     = ATHR_DEV_2051.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_7088144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_001B.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_7092144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_2054.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7094144F
%ATHR.DeviceDesc.3063%     = ATHR_DEV_2063.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7096144F
%ATHR.DeviceDesc.3065%     = ATHR_DEV_2052.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7106144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7128144f
%ATHR.DeviceDesc.3062%     = ATHR_DEV_2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7112144f
%ATHR.DeviceDesc.001A%     = ATHR_DEV_001A.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_04271468
%ATHR.DeviceDesc.001B%     = ATHR_DEV_001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_04251468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_04261468
%ATHR.DeviceDesc.1737_g%   = ATHR_DEV_001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_00531737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_001B.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_00431737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_00351731
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_00351737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_00171737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_00251737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0012&SUBSYS_1022168C 
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1026168C
%ATHR.DeviceDesc.1737_abg% = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_00361737
%ATHR.DeviceDesc.001B%     = ATHR_DEV_001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_0086106B
%ATHR.DeviceDesc.0013%     = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1025168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1026168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2026168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1031168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2031168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_46101385
%ATHR.DeviceDesc.0013%     = ATHR_DEV_F013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_123410CF
%ATHR.DeviceDesc.0013%     = ATHR_DEV_F013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_123510CF
%ATHR.DeviceDesc.10CF%     = ATHR_DEV_F013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_123610CF
%ATHR.DeviceDesc.001B%     = ATHR_DEV_F013.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_132910CF
%ATHR.DeviceDesc.10CF%     = ATHR_DEV_F013.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_134F10CF
%ATHR.DeviceDesc.3062%     = ATHR_DEV_F013.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_139C10CF
%ATHR.DeviceDesc.3067%     = ATHR_DEV_F01C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_142E10CF
%ATHR.DeviceDesc.3013%     = ATHR_DEV_3013.ndi,    PCI\VEN_168C&DEV_1014&SUBSYS_05891014
%ATHR.DeviceDesc.4013%     = ATHR_DEV_4013.ndi,    PCI\VEN_168C&DEV_1014&SUBSYS_058A1014
%ATHR.DeviceDesc.2013%     = ATHR_DEV_2013.ndi,    PCI\VEN_168C&DEV_1014&SUBSYS_057E1014
%ATHR.DeviceDesc.1013%     = ATHR_DEV_1013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_04081468
%ATHR.DeviceDesc.5013%     = ATHR_DEV_5013.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_0034168c
%ATHR.DeviceDesc.3062%     = ATHR_DEV_2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102010E9
%ATHR.DeviceDesc.3062%     = ATHR_DEV_2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_75191113
%ATHR.DeviceDesc.14B9_abg% = ATHR_DEV_1042.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_cb2114B9
%ATHR.DeviceDesc.14B9_abg% = ATHR_DEV_1042.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_cc2114B9
%ATHR.DeviceDesc.3067%     = ATHR_DEV_001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_3067168C
%ATHR.DeviceDesc.3067%     = ATHR_DEV_10261A3B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_10261A3B
%ATHR.DeviceDesc.3062%     = ATHR_DEV_04221468.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_04221468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_04221468.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_04171468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_04221468.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_04181468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_04221468.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_04201468
%ATHR.DeviceDesc.3067%     = ATHR_DEV_04281468.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_04281468
%ATHR.DeviceDesc.04231468%     = ATHR_DEV_E000105B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_E000105B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_001C.ndi,        PCI\VEN_168C&DEV_001C&SUBSYS_042A1468
%ATHR.DeviceDesc.3067%     = ATHR_DEV_01051A32.ndi,        PCI\VEN_168C&DEV_001C&SUBSYS_01051A32
%ATHR.DeviceDesc.4B001385%     = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_4B001385
%ATHR.DeviceDesc.4B001385%     = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_5B001385
%ATHR.DeviceDesc.5D001385%     = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_5D001385
%ATHR.DeviceDesc.4D001385%     = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_4D001385
%ATHR.DeviceDesc.4F001385%     = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_4F001385
%ATHR.DeviceDesc.04061468%     = ATHR_DEV_04061468.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_04061468
%ATHR.DeviceDesc.04071468%     = ATHR_DEV_04061468.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_04071468 
%ATHR.DeviceDesc.04231468%     = ATHR_DEV_04231468.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_04231468 
%ATHR.DeviceDesc.04231468%     = ATHR_DEV_04231468.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_0423168C 
%ATHR.DeviceDesc.2055%     = ATHR_DEV_1055.ndi,    PCI\VEN_168C&DEV_001D&SUBSYS_1055168C
%ATHR.DeviceDesc.2055%     = ATHR_DEV_2055.ndi,    PCI\VEN_168C&DEV_001D&SUBSYS_2055168C
%ATHR.DeviceDesc.3070%     = ATHR_DEV_1042.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_307002FA
%ATHR.DeviceDesc.3071%     = ATHR_DEV_1042.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_307102FA
; Belkin
%ATHR.DeviceDesc.001A%     = ATHR_DEV_001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_701D1799
%ATHR.DeviceDesc.001A%     = ATHR_DEV_001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_700D1799
%ATHR.DeviceDesc.F6D3000%  = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_30001799
%ATHR.DeviceDesc.F6D3000%  = ATHR_DEV_001B.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_30001799
; D-Link
%ATHR.DeviceDesc.G650%         = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_3A121186
%ATHR.DeviceDesc.G520X%        = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_32031186
%ATHR.DeviceDesc.G520%         = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_3A131186
%ATHR.DeviceDesc.AG520%        = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_3A081186
%ATHR.DeviceDesc.AG530%        = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_3A141186
%ATHR.DeviceDesc.G630%         = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_3A151186
%ATHR.DeviceDesc.G510%         = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_3A161186
%ATHR.DeviceDesc.AG650%        = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_3A071186
%ATHR.DeviceDesc.AG660%        = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_3A631186
%ATHR.DeviceDesc.G680%         = ATHR_DEV_3A171186.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_3A171186
%ATHR.DeviceDesc.G550%         = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_3A181186
%ATHR.DeviceDesc.AG660B%       = ATHR_DEV_3A171186.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_3A191186
%ATHR.DeviceDesc.AG530B%       = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_3A221186
%ATHR.DeviceDesc.G650P%        = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_3A241186
%ATHR.DeviceDesc.G520P%        = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_3A231186
%ATHR.DeviceDesc.WDA1320%      = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_3A1D1186
%ATHR.DeviceDesc.WDA2320%      = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_3A1B1186
%ATHR.DeviceDesc.DWA520%       = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_3A731186
%ATHR.DeviceDesc.DWA620%       = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_3A741186
%ATHR.DeviceDesc.CWNA2330%     = ATHR_DEV_3A171186.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_3A1A1186
%ATHR.DeviceDesc.CWNA1330%     = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_3A1C1186
%ATHR.DeviceDesc.CWNA1330%     = ATHR_DEV_3A171186.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_3A1C1186
%ATHR.DeviceDesc.CG650%        = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_32021186
%ATHR.DeviceDesc.CG630%        = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_3B081186
%ATHR.DeviceDesc.CG630%        = ATHR_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_3B081186
; QMI                            
%ATHR.DeviceDesc.3065%         = ATHR_DEV_01001A32.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_01001A32
%ATHR.DeviceDesc.3063%         = ATHR_DEV_01001A32.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_02001A32
%ATHR.DeviceDesc.3072%         = ATHR_DEV_01001A32.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_05021A32

;11n HW Entries
%ATHR.DeviceDesc.1071%    = ATHR_DEV_1071.ndi,    PCI\VEN_168C&DEV_0023&SUBSYS_1071168C
%ATHR.DeviceDesc.1071%    = ATHR_DEV_1071.ndi,    PCI\VEN_168C&DEV_0023&SUBSYS_2071168C
%ATHR.DeviceDesc.3072%    = ATHR_DEV_3072.ndi,    PCI\VEN_168C&DEV_0023&SUBSYS_1072168C
%ATHR.DeviceDesc.3072%    = ATHR_DEV_3072.ndi,    PCI\VEN_168C&DEV_0023&SUBSYS_2072168C
%ATHR.DeviceDesc.3072%    = ATHR_DEV_3072.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_3072168C

%ATHR.DeviceDesc.0032168c%  	= ATHR_DEV_0032168c.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_0032168c
%ATHR.DeviceDesc.0033168c%  	= ATHR_DEV_0033168c.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_0033168c
%ATHR.DeviceDesc.3072%  	= ATHR_DEV_13C010CF.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_13C010CF
%ATHR.DeviceDesc.3072%  	= ATHR_DEV_7125144F.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_7125144F
%ATHR.DeviceDesc.3072%  	= ATHR_DEV_7125144F.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_04291468
%ATHR.DeviceDesc.3072%          = ATHR_DEV_3072.ndi,        PCI\VEN_168C&DEV_0024&SUBSYS_04301468
%ATHR.DeviceDesc.3072%          = ATHR_DEV_3072.ndi,        PCI\VEN_168C&DEV_0024&SUBSYS_00000000
%ATHR.DeviceDesc.3072%          = ATHR_DEV_3072.ndi,        PCI\VEN_168C&DEV_0024&SUBSYS_0087106b
%ATHER.DeviceDesc.800118CB%     = ATHR_DEV_3072.ndi,        PCI\VEN_168C&DEV_0023&SUBSYS_800118CB
; Belkin 11n
%ATHR.DeviceDesc.80111799%  	= ATHR_DEV_80111799.ndi,    PCI\VEN_168C&DEV_0023&SUBSYS_80111799
; D-Link 11n
%ATHR.DeviceDesc.DWA642%        = ATHR_DEV_1186.ndi,        PCI\VEN_168C&DEV_0023&SUBSYS_3A6A1186
%ATHR.DeviceDesc.DWA645%  	    = ATHR_DEV_1186.ndi,        PCI\VEN_168C&DEV_0023&SUBSYS_3A0907D1
%ATHR.DeviceDesc.DWA645%  	    = ATHR_DEV_1186.ndi,        PCI\VEN_168C&DEV_0023&SUBSYS_3A761186
%ATHR.DeviceDesc.DWA542%  	    = ATHR_DEV_3A691186.ndi,    PCI\VEN_168C&DEV_0023&SUBSYS_3A691186
%ATHR.DeviceDesc.DWA547%  	    = ATHR_DEV_3A6D1186.ndi,    PCI\VEN_168C&DEV_0023&SUBSYS_3A6B1186
%ATHR.DeviceDesc.DWA652%  	    = ATHR_DEV_1186.ndi,        PCI\VEN_168C&DEV_0023&SUBSYS_3A6E1186
%ATHR.DeviceDesc.DWA552%  	    = ATHR_DEV_3A6D1186.ndi,    PCI\VEN_168C&DEV_0023&SUBSYS_3A6D1186
%ATHR.DeviceDesc.DWA643%  	    = ATHR_DEV_3A6F1186.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_3A6F1186
%ATHR.DeviceDesc.DWA556%  	    = ATHR_DEV_3A701186.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_3A701186
; NEC 
%ATHR.DeviceDesc.3062%     = ATHR_DEV_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102510E9
%ATHR.DeviceDesc.3072%     = ATHR_DEV_N3072.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102210E9
[Gigabyte.NTX86]
;11N
;CardBus
%GIGA.DeviceDesc.E815%  = GIGA_DEV_E914.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_E8151458
;(Mini)PCI
%GIGA.DeviceDesc.E914%  = GIGA_DEV_E914.ndi,    PCI\VEN_168C&DEV_0023&SUBSYS_E9141458
;Express PCI
%GIGA.DeviceDesc.E915%  = GIGA_DEV_E914.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_E9151458
;Express Mini PCI
%GIGA.DeviceDesc.E916%  = GIGA_DEV_E916.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_E9161458
;11G
;CardBus
%GIGA.DeviceDesc.E801%  = GIGA_DEV_E801.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_E8011458
%GIGA.DeviceDesc.E811%  = GIGA_DEV_E811.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_E8111458
%GIGA.DeviceDesc.E814%  = GIGA_DEV_E814.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_E8141458
;(Mini)PCI
%GIGA.DeviceDesc.0013%  = GIGA_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_E9011458
%GIGA.DeviceDesc.E901%  = GIGA_DEV_E901.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_E9011458
%GIGA.DeviceDesc.E911%  = GIGA_DEV_E911.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_E9111458
%GIGA.DeviceDesc.E912%  = GIGA_DEV_E912.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_E9121458
%GIGA.DeviceDesc.E913%  = GIGA_DEV_E913.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_E9131458
%GIGA.DeviceDesc.E917%  = GIGA_DEV_E917.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_E9171458

[GIGA_DEV_E801.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E801.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E811.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E811.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E814.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E814.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_0013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_0013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E901.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E901.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E911.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E911.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E912.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E912.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog


[GIGA_DEV_E913.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer_GigaByteLed1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E913.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog


[GIGA_DEV_E917.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer_GigaByteLed1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E917.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E914.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer_GigaByte.reg, customer_GigaByteLed0.reg, 5416.antennacontrols.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[GIGA_DEV_E914.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[GIGA_DEV_E916.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer_GigaByte.reg, customer_GigaByteLed1.reg, 5416.antennacontrols.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[GIGA_DEV_E916.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_0013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_0013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_001A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_001A.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_001B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_001B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_001C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_001C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1055.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, gpioled.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1055.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2055.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2055.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1030.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1030.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2030.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2030.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1031.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1031.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2031.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2031.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1041.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1041.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2041.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2041.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1042.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1042.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2042.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2042.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1051.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1051.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2051.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2051.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1052.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1052.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2052.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2052.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_01001A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer9Led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_01001A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1053.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1053.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2053.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2053.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1054.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1054.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2054.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2054.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1062.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1062.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2062.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2062.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1063.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1063.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2063.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2063.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1071.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_1071.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3072.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3072.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

;;Others Section

[ATHR_DEV_1013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer0LED.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_1013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_2013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer0LED.reg, customer0.reg, roamthreshA.reg, ignore11d.reg, bandselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_2013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer0LED1.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_3013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_4013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer0LED1.reg, customer0.reg, roamthreshA.reg, ignore11d.reg, bandselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_4013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_5013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer0LED2.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_5013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_F013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer1ani.reg, bandselect.reg, adhocchannelselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_F013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_F01C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer1ani.reg, adhocchannelselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_F01C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_04221468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer3.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_04221468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_E000105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer4b.reg, customer4a_ASPM.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf
Needs           = PciASPMOptIn

[ATHR_DEV_E000105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_04281468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer3a.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_04281468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_01051A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer3a.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_01051A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_04061468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer4.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_04061468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_04231468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer4a.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf
Needs           = PciASPMOptIn

[ATHR_DEV_04231468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_0032168c.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer0_11n.reg, 5416.antennacontrols.reg, 5416.bgnxb.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_0032168c.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_0033168c.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer0_11n.reg, 5416.antennacontrols.reg, 5416.bandselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_0033168c.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_13C010CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, 5416.bandselect.reg, 5416.antennacontrols.reg, customer1ani.reg, adhocchannelselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_13C010CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_7125144F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, 5416.antennacontrols.reg, radiointerval.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_7125144F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3A171186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer5Led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_3A171186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_10261A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer6Led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_10261A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_80111799.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer7Led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_80111799.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer5.11nLED.reg, ratecap.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3A691186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, pcibusconfig.reg, customer5.11nLED.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3A691186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3A6D1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, pcibusconfig.reg, customer5.3x3.reg, customer5.11nLED.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3A6D1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3A6F1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer5.PCIe11nLed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3A6F1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_3A701186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer5.3x3.reg, customer5.PCIe11nLed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_3A701186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_N2062.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer11Led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11

[ATHR_DEV_N2062.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHR_DEV_N3072.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros.reg, customer11Led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHR_DEV_N3072.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

;;End of Others Section

[atheros.reg]
HKR, Ndi,                           Service,    0, "athr"
HKR, Ndi\Interfaces,                UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,                LowerRange, 0, "wlan,ethernet"
HKR, Ndi\params\*ReceiveBuffers,    ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,    default,    0, "256"
HKR, Ndi\params\*ReceiveBuffers,    min,        0, "1"
HKR, Ndi\params\*ReceiveBuffers,    max,        0, "00000512"
HKR, Ndi\params\*ReceiveBuffers,    step,       0, "1"
HKR, Ndi\params\*ReceiveBuffers,    Base,       0, "10"
HKR, Ndi\params\*ReceiveBuffers,    type,       0, "int"
HKR, Ndi\params\*TransmitBuffers,   ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,   default,    0, "512"
HKR, Ndi\params\*TransmitBuffers,   min,        0, "1"
HKR, Ndi\params\*TransmitBuffers,   max,        0, "00000512"
HKR, Ndi\params\*TransmitBuffers,   step,       0, "1"
HKR, Ndi\params\*TransmitBuffers,   Base,       0, "10"
HKR, Ndi\params\*TransmitBuffers,   type,       0, "int"
HKR, Ndi\params\NetworkAddress,     ParamDesc,  0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,     default,    0,  ""
HKR, Ndi\params\NetworkAddress,     LimitText,  0,  "12"
HKR, Ndi\params\NetworkAddress,     UpperCase,  0,  "1"
HKR, Ndi\params\NetworkAddress,     optional,   0,  "1"
HKR, Ndi\params\NetworkAddress,     type,       0,  "edit"
HKR, Ndi\params\shortPreamble,      ParamDesc,  0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,      Base,       0,  "10"
HKR, Ndi\params\shortPreamble,      default,    0,  "1"
HKR, Ndi\params\shortPreamble,      type,       0,  "enum"
HKR, Ndi\params\shortPreamble\enum, "1",        0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0",        0,  %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,      ParamDesc,  0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,      default,    0,  "60"
HKR, Ndi\params\scanTimeValid,      min,        0,  "20"
HKR, Ndi\params\scanTimeValid,      max,        0,  "120"
HKR, Ndi\params\scanTimeValid,      step,       0,  "5"
HKR, Ndi\params\scanTimeValid,      base,       0,  "10"
HKR, Ndi\params\scanTimeValid,      type,       0,  "int"

;/* Enable these if VLAN or 802.1p is to be enabled */
;HKR, Ndi\Params\*PriorityVLANTag,  ParamDesc,  , %PriorityVLAN%
;HKR, Ndi\Params\*PriorityVLANTag,  default,    , "3"
;HKR, Ndi\Params\*PriorityVLANTag,  type,       , "enum"
;HKR, Ndi\Params\*PriorityVLANTag\enum, 0,      , %PriorityVLANDisabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 1,      , %PriorityEnabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 2,      , %VLANEnabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 3,      , %PriorityVLANEnabled%

[atheros.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,ccode
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin
HKR,Ndi\params,MapRegisters,0x2000
HKR,,MapRegisters
HKR,Ndi\params,radioEnable,0x2000
HKR,Ndi\params,sleepMode,0x2000
HKR,,sleepMode
HKR,,gpioFunc0ActHi
HKR,,gpioFunc1ActHi
HKR,,gpioLedCustom
HKR,,gpioPinFunc0
HKR,,gpioPinFunc1
HKR,,transmitRateMax

;;Customized Section

[pcibusconfig.reg]
HKR, ,                                  BusConfig,                 	0x00002,  "0"

[bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,        %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,        "10"
HKR, Ndi\params\NetBand,                default,                        0,        "1549"
HKR, Ndi\params\NetBand,                type,                           0,        "enum"
HKR, Ndi\params\NetBand\enum,           "1549",                         0,        "Auto"
HKR, Ndi\params\NetBand\enum,           "1537",                         0,        "5Ghz Only"
HKR, Ndi\params\NetBand\enum,           "12",                           0,        "2.4Ghz Only"

[roamthreshA.reg]
HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,        %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,        "15"
HKR, Ndi\params\roamRssiA,              min,                            0,        "1"
HKR, Ndi\params\roamRssiA,              max,                            0,        "95"
HKR, Ndi\params\roamRssiA,              step,                           0,        "1"
HKR, Ndi\params\roamRssiA,              base,                           0,        "10"
HKR, Ndi\params\roamRssiA,              type,                           0,        "int"

[ignore11d.reg]
HKR,NDI\params\ignore11dBeacon,         ParamDesc,,                               "11d Mode Switch"
HKR,NDI\params\ignore11dBeacon,         type,,                                    "enum"
HKR,NDI\params\ignore11dBeacon,         Default,,                                 "1"
HKR,NDI\params\ignore11dBeacon\enum,    0,,                                       "Enable"
HKR,NDI\params\ignore11dBeacon\enum,    1,,                                       "Disable"

;[radioswitch.reg]
;HKR, Ndi\params\radioEnable,            ParamDesc,                      0,        %radioEnable%
;HKR, Ndi\params\radioEnable,            Base,                           0,        "10"
;HKR, Ndi\params\radioEnable,            default,                        0,        "1"
;HKR, Ndi\params\radioEnable,            type,                           0,        "enum"
;HKR, Ndi\params\radioEnable\enum,       "1",                            0,        %radioEnableOn%
;HKR, Ndi\params\radioEnable\enum,       "0",                            0,        %radioEnableOff%

[adhocchannelselect.reg]
HKR, Ndi\params\defaultIbssChannel,     ParamDesc,                      0,        %adhocchannel%
HKR, Ndi\params\defaultIbssChannel,     default,                        0,        "10"
HKR, Ndi\params\defaultIbssChannel,     min,                            0,        "1"
HKR, Ndi\params\defaultIbssChannel,     max,                            0,        "11"
HKR, Ndi\params\defaultIbssChannel,     step,                           0,        "1"
HKR, Ndi\params\defaultIbssChannel,     base,                           0,        "10"
HKR, Ndi\params\defaultIbssChannel,     type,                           0,        "int"

[5416.bgnxb.reg]
HKR, ,                                  NetBand,                        0x00002,  "26636"
HKR, ,                                  wmodeselect,                    0x00002,  "26636"

[5416.bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "130573"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "130573",                       0,  "Auto"
HKR, Ndi\params\NetBand\enum,           "103937",                       0,  "5Ghz Only"
HKR, Ndi\params\NetBand\enum,           "26636",                        0,  "2.4Ghz Only"

[5416.antennacontrols.reg] 
HKR, ,                                  rxChainMask,                 	0x00002,  "7"
HKR, ,                                  txChainMaskLegacy,              0x00002,  "5"
HKR, ,                                  rxChainMaskLegacy,           	0x00002,  "7"
HKR, ,                                  rxChainDetect,                  0x00002,  "1"
HKR, ,                                  rxChainDetectRef,               0x00002,  "0"
HKR, ,                                  rxChainDetectThreshA,           0x00002,  "0"
HKR, ,                                  rxChainDetectThreshG,           0x00002,  "0"
HKR, ,                                  rxChainDetectDeltaA,            0x00002,  "20"
HKR, ,                                  rxChainDetectDeltaG,            0x00002,  "20"

[customer0.reg]
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,                                  scanTimePreSleep,               0x00002,  "60" 
HKR, ,                                  capLinkSp,                      0x00002,  "1" 
HKR, ,                                  pcieAspm,                       0x00002,  "2" 
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1" 
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer0LED.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "0"

[customer0LED1.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  halPcieClockReq,                0x00002,  "1"

[customer0LED2.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  halPcieClockReq,                0x00002,  "1"

[customer0_11n.reg]
;PCIe Related
HKR, ,                                  radioEnableInterval,            0x00002,  "5"
HKR, ,                                  pcieAspm,                 	0x00002,  "2"
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  forceWake,                 	0x00002,  "0"
HKR, ,                                  antennaSwitchSwap,              0x00002,  "1"
;LED Related
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
;General Customer0
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR,NDI\params\ignore11dBeacon,ParamDesc,,	"11d Mode Switch"
HKR,NDI\params\ignore11dBeacon,type,,		"enum"
HKR,NDI\params\ignore11dBeacon,Default,,	"1"
HKR,NDI\params\ignore11dBeacon\enum,0,,		"Enable"
HKR,NDI\params\ignore11dBeacon\enum,1,,		"Disable"

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,  %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,  "15"
HKR, Ndi\params\roamRssiA,              min,                            0,  "1"
HKR, Ndi\params\roamRssiA,              max,                            0,  "95"
HKR, Ndi\params\roamRssiA,           	step,                           0,  "1"
HKR, Ndi\params\roamRssiA,           	base,                           0,  "10"
HKR, Ndi\params\roamRssiA,           	type,                           0,  "int"

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

[customer1ani.reg]
HKR, Ndi\params\rssiThrHigh,            ParamDesc,                      0,        %rssiThrHigh%
HKR, Ndi\params\rssiThrHigh,            Base,                           0,        "10"
HKR, Ndi\params\rssiThrHigh,            default,                        0,        "40"
HKR, Ndi\params\rssiThrHigh,            type,                           0,        "enum"
HKR, Ndi\params\rssiThrHigh\enum,       "40",                           0,        %rssiThrHighNormal%
HKR, Ndi\params\rssiThrHigh\enum,       "32",                           0,        %rssiThrHighMin%

;[customer2.reg]
;HKR,,                                   linkLEDFunc,                    0,        "53"
;HKR,,                                   activityLEDFunc,                0,        "51"
;HKR,,                                   connectionLEDFunc,              0,        "55"

[customer3.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  LinkLEDFunc,                   0x00002,  "19"
HKR, ,                                  ActivityLEDFunc,                   0x00002,  "21"

[customer3a.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

;[customer3b.reg]
;HKR, ,                                  gpioPinFunc1,			0x00002,  "3"
;HKR, ,                                  overrideACstatus,		0x00002,  "1"
;HKR, ,                                  halPcieClockReq,		0x00002,  "1"
;HKR, ,                                  gpioLedCustom,			0x00002,  "4"
;HKR, ,                                  gpioFunc1ActHi,			0x00002,  "0"

[customer4.reg]
HKR, ,					gpioPinFunc0,        		0x00002,  "1"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4a.reg]
HKR, ,                                  gpioPinFunc0,        		0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,      		0x00002,  "0"
HKR, ,                                  halPcieClockReq,        	0x00002,  "1"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4b.reg]
HKR, ,					gpioPinFunc0,        		0x00002,  "3"
HKR, ,					gpioFunc0ActHi,      		0x00002,  "0"
HKR, ,					halPcieClockReq,        	0x00002,  "1"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4a_ASPM.reg]
HKR, ,                                  pcieAspm,                       0x00002,  "0"

;[customer5.reg]
;HKR,,                                   linkLEDFunc,                    0,        "49"
;HKR,,                                   activityLEDFunc,                0,        "51"
;HKR,,                                   connectionLEDFunc,              0,        "55"

[customer5Led.reg]
HKR, ,                                  softLEDEnable,                  0x00002,  "1"
HKR, ,                                  swapDefaultLED,                 0x00002,  "1"

[customer5.11nLED.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "1"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "2"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer5.PCIe11nLed.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[customer5.3x3.reg]
HKR, ,                                  txChainMask,                 	0x00002,  "7"
HKR, ,                                  rxChainMask,                 	0x00002,  "7"

[customer6Led.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[customer7Led.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "2"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "2"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "1"

[customer9Led.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[gpioled.reg]
HKR,,                                   linkLEDFunc,                    0,        "49"
HKR,,                                   activityLEDFunc,                0,        "51"
HKR,,                                   connectionLEDFunc,              0,        "55"

[ratecap.reg]
;HKR, ,                                  txCoalescingEnable,             0x00002,  "1"

[radiointerval.reg]
;PCIe Related
HKR, ,                                  radioEnableInterval,            0x00002,  "5"

[customer11Led.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[customer_GigaByte.reg]
HKR, ,                          txChainMask,          0x00002,  "5"

[customer_GigaByteLed0.reg]
HKR, ,                  		LinkLedFunc,       		0, "19"
HKR, ,                  		ActivityLedFunc,       	0, "21" 

[customer_GigaByteLed1.reg]
HKR, ,                  		LinkLedFunc,       		0, "03"
HKR, ,                  		ActivityLedFunc,       		0, "05"

;;End of Customized Section

[atheros.Service]
DisplayName     = %ATHR.Service.DispName%
ServiceType     = 1         ;SERVICE_KERNEL_DRIVER
StartType       = 3         ;SERVICE_DEMAND_START
ErrorControl    = 1         ;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\athr.sys
LoadOrderGroup  = NDIS

[atheros.EventLog]
AddReg = atheros.AddEventLog.reg

[atheros.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


[atheros.CopyFiles]
athr.sys,,,2

[SourceDisksNames]
1 = %DiskDescription%,athr.sys,,

[SourceDisksFiles]
athr.sys = 1,,

[DestinationDirs]
atheros.CopyFiles            = 12
DefaultDestDirs              = 11

[Strings]
Msft                         = "Microsoft"
Atheros                      = "Atheros Communications Inc."
Gigabyte                     = "Gigabyte Technology Corp."
ATHR.Service.DispName        = "Atheros Extensible Wireless LAN device driver"
DiskDescription              = "Atheros Sample Driver Disk 1"
TransmitBuffers              = "Transmit Buffers"
ReceiveBuffers               = "Receive Buffers"
NetworkAddress               = "Network Address"
scanTimeValid                = "Scan Valid Interval"
shortPreamble                = "802.11b Preamble"
shortPreambleEnable          = "Long and Short"
shortPreambleDisable         = "Long only"
rssiThrHigh                  = "RSSI Threshold"
rssiThrHighNormal            = "Normal"
rssiThrHighMin               = "Min"
;radioEnable                  = "Radio On/Off"
;radioEnableOn                = "On"
;radioEnableOff               = "Off"
scanTime                     = "Roam Time (sec)"
roamRssiA                    = "Roam Time Threshold (db)"
WirelessMode                 = "Wireless Mode Selection"
adhocchannel                 = "Adhoc channel Selection"
ATHR.DeviceDesc.0013         = "Atheros Wireless Network Adapter"
ATHR.DeviceDesc.001A         = "Atheros AR5005G Wireless Network Adapter"
ATHR.DeviceDesc.001B         = "Atheros AR5006X Wireless Network Adapter"
ATHR.DeviceDesc.1030         = "Atheros AR5002G Wireless Network Adapter"
ATHR.DeviceDesc.2030         = "Atheros AR5002G Wireless Network Adapter"
ATHR.DeviceDesc.1031         = "Atheros AR5002X Wireless Network Adapter"
ATHR.DeviceDesc.2031         = "Atheros AR5002X Wireless Network Adapter"
ATHR.DeviceDesc.1041         = "Atheros AR5004G Wireless Network Adapter"
ATHR.DeviceDesc.2041         = "Atheros AR5004G Wireless Network Adapter"
ATHR.DeviceDesc.1042         = "Atheros AR5004X Wireless Network Adapter"
ATHR.DeviceDesc.2042         = "Atheros AR5004X Wireless Network Adapter"
ATHR.DeviceDesc.1051         = "Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.2051         = "Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.1053         = "Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.2053         = "Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.1061         = "Atheros AR5006GS Wireless Network Adapter"
ATHR.DeviceDesc.2061         = "Atheros AR5006GS Wireless Network Adapter"
ATHR.DeviceDesc.1062         = "Atheros AR5006XS Wireless Network Adapter"
ATHR.DeviceDesc.2062         = "Atheros AR5006XS Wireless Network Adapter"
ATHR.DeviceDesc.1065         = "Atheros AR5006G Wireless Network Adapter"
ATHR.DeviceDesc.2065         = "Atheros AR5006G Wireless Network Adapter"
ATHR.DeviceDesc.3061         = "Atheros AR5006EGS Wireless Network Adapter"
ATHR.DeviceDesc.3062         = "Atheros AR5006EXS Wireless Network Adapter"
ATHR.DeviceDesc.3063         = "Atheros AR5006EX Wireless Network Adapter"
ATHR.DeviceDesc.3065         = "Atheros AR5006EG Wireless Network Adapter"
ATHR.DeviceDesc.2055         = "Atheros AR5007G Wireless Network Adapter"
ATHR.DeviceDesc.3067         = "Atheros AR5007EG Wireless Network Adapter"
ATHR.DeviceDesc.1071         = "Atheros AR5008 Wireless Network Adapter"
ATHR.DeviceDesc.3072         = "Atheros AR5008X Wireless Network Adapter"
ATHR.DeviceDesc.10CF         = "IEEE 802.11a/g Wireless LAN Adapter (A)"
ATHR.DeviceDesc.1737_g       = "Linksys Wireless-G Notebook Adapter"
ATHR.DeviceDesc.1737_bg      = "Linksys Wireless A+G Notebook Adapter"
ATHR.DeviceDesc.14B9_abg     = "Cisco Aironet 802.11a/b/g Wireless Adapter"
ATHR.DeviceDesc.1737_abg     = "Linksys Wireless A+G PCI Adapter"
ATHR.DeviceDesc.1013         = "11b/g Wireless LAN Mini PCI Adapter"
ATHR.DeviceDesc.2013         = "11a/b/g Wireless LAN Mini PCI Adapter II" 
ATHR.DeviceDesc.3013         = "11b/g Wireless LAN Mini PCI Express Adapter"
ATHR.DeviceDesc.4013         = "11a/b/g Wireless LAN Mini PCI Express Adapter"
ATHR.DeviceDesc.5013         = "11b/g Wireless LAN Mini PCI Express Adapter II"
ATHR.DeviceDesc.0032168c     = "11b/g/n Wireless LAN Mini-PCI Express Adapter"
ATHR.DeviceDesc.0033168c     = "11a/b/g/n Wireless LAN Mini-PCI Express Adapter"
ATHR.DeviceDesc.4B001385     = "NETGEAR 108 Mbps Wireless PC Card WG511T"
ATHR.DeviceDesc.5D001385     = "NETGEAR RangeMax(TM) Wireless PC Card WPN511"
ATHR.DeviceDesc.4D001385     = "NETGEAR 108 Mbps Wireless PCI Adapter WG311T"
ATHR.DeviceDesc.4F001385     = "NETGEAR Double 108 Mbps Wireless PC Card WG511U"
ATHR.DeviceDesc.04061468     = "LAN-Express AS IEEE 802.11g miniPCI Adapter"
ATHR.DeviceDesc.04071468     = "LAN-Express AS IEEE 802.11a/g miniPCI Adapter"
ATHR.DeviceDesc.04231468     = "LAN-Express AS IEEE 802.11g PCI-E Adapter"
ATHR.DeviceDesc.F6D3000      = "Belkin Wireless A/G Desktop Network Card"
ATHR.DeviceDesc.80111799     = "Belkin N1 Wireless Notebook Card"
ATHR.DeviceDesc.G650	     = "D-Link AirPlus DWL-G650 Wireless Cardbus Adapter(rev.C)"
ATHR.DeviceDesc.G520X	     = "D-Link AirPlus Xtreme G DWL-G520 Adapter"
ATHR.DeviceDesc.G520	     = "D-Link AirPlus DWL-G520 Wireless PCI Adapter(rev.B)"
ATHR.DeviceDesc.AG520	     = "D-Link AirXpert DWL-AG520 Wireless PCI Adapter"
ATHR.DeviceDesc.AG530	     = "D-Link AirPremier DWL-AG530 Wireless PCI Adapter"
ATHR.DeviceDesc.G630         = "D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter(rev.D)"
ATHR.DeviceDesc.G510	     = "D-Link AirPlus G DWL-G510 Wireless PCI Adapter(rev.B)"
ATHR.DeviceDesc.AG650	     = "D-Link AirXpert DWL-AG650 Wireless Cardbus Adapter"
ATHR.DeviceDesc.AG660	     = "D-Link AirPremier DWL-AG660 Wireless Cardbus Adapter"
ATHR.DeviceDesc.G680         = "D-Link AirPremier DWL-G680 Wireless Cardbus Adapter"
ATHR.DeviceDesc.G550	     = "D-Link AirPremier DWL-G550 Wireless PCI Adapter"
ATHR.DeviceDesc.AG660B	     = "D-Link AirPremier AG DWL-AG660 Wireless Cardbus Adapter"
ATHR.DeviceDesc.AG530B	     = "D-Link AirPremier AG DWL-AG530 Wireless PCI Adapter"
ATHR.DeviceDesc.G650P        = "D-Link AirPlus G DWL-G650+A Wireless Cardbus Adapter"
ATHR.DeviceDesc.G520P	     = "D-Link AirPlus G DWL-G520+A Wireless PCI Adapter"
ATHR.DeviceDesc.WDA1320      = "D-Link WDA-1320 Desktop Adapter"
ATHR.DeviceDesc.WDA2320	     = "D-Link WDA-2320 Desktop Adapter"
ATHR.DeviceDesc.DWA520	     = "D-Link Wireless 108G DWA-520 Desktop Adapter"
ATHR.DeviceDesc.DWA620	     = "D-Link Wireless 108G DWA-620 Notebook Adapter"
ATHR.DeviceDesc.CWNA2330     = "D-Link WNA-2330 Notebook Adapter"
ATHR.DeviceDesc.CWNA1330     = "D-Link WNA-1330 Notebook Adapter"
ATHR.DeviceDesc.CG650        = "D-Link AirPlus Xtreme G DWL-G650 Adapter"
ATHR.DeviceDesc.CG630        = "D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter"
ATHR.DeviceDesc.DWA642       = "D-Link DWA-642 RangeBooster N Notebook Adapter"
ATHR.DeviceDesc.DWA645       = "D-Link DWA-645 RangeBooster N650 Notebook Adapter"
ATHR.DeviceDesc.DWA542       = "D-Link DWA-542 RangeBooster N Desktop Adapter"
ATHR.DeviceDesc.DWA547       = "D-Link DWA-547 RangeBooster N650 Desktop Adapter"
ATHR.DeviceDesc.DWA652       = "D-Link DWA-652 XtremeN Notebook Adapter"
ATHR.DeviceDesc.DWA552       = "D-Link DWA-552 XtremeN Desktop Adapter"
ATHR.DeviceDesc.DWA643       = "D-Link DWA-643 Xtreme N ExpressCard Notebook Adapter"
ATHR.DeviceDesc.DWA556       = "D-Link DWA-556 Xtreme N PCIe Desktop Adapter"
ATHR.DeviceDesc.3070         = "Gigaset PC Card 108"
ATHR.DeviceDesc.3071         = "Speedport Gigaset 54 Mbit"
ATHER.DeviceDesc.800118CB    = "Gigaset PC Card 300"
GIGA.DeviceDesc.E914	     = "Gigabyte GN-WI03N (mini) PCI WLAN Card"
GIGA.DeviceDesc.E915	     = "Gigabyte GN-WP02N PCI Express WLAN Card"
GIGA.DeviceDesc.E916	     = "Gigabyte GN-WI06N (mini) PCI Express WLAN Card"
GIGA.DeviceDesc.E815	     = "Gigabyte GN-WM02N Express WLAN Card"
GIGA.DeviceDesc.E801         = "Gigabyte GN-WLMA102 Cardbus WLAN Card"
GIGA.DeviceDesc.E811         = "Gigabyte GN-WMAG Cardbus WLAN Card"
GIGA.DeviceDesc.E814         = "Gigabyte GN-WM01GT Cardbus WLAN Card"
GIGA.DeviceDesc.0013         = "Gigabyte GN-WIAH (mini) PCI WLAN Card"
GIGA.DeviceDesc.E901         = "Gigabyte GN-WI01HT (mini) PCI WLAN Card"
GIGA.DeviceDesc.E911         = "Gigabyte GN-WIAG/GN-WPEAG (mini) PCI WLAN Card"
GIGA.DeviceDesc.E912         = "Gigabyte GN-WP01GT (mini) PCI WLAN Card"
GIGA.DeviceDesc.E913         = "Gigabyte GN-WI01GT (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E917         = "Gigabyte GN-WI07HT (mini) PCI-E WLAN Card"

;/* Enable these if VLAN or 802.1p is to be enabled */
;PriorityVLAN                = "Priority & VLAN"
;PriorityVLANDisabled        = "Priority & VLAN Disabled"
;PriorityEnabled             = "Priority Enabled"
;VLANEnabled                 = "VLAN Enabled"
;PriorityVLANEnabled         = "Priority & VLAN Enabled"
