;/*++
;
;Copyright (c) 2006,2008 AuthenTec. Inc,  All rights reserved.
;
;Module Name:
;
;    ATSWPWDF.INF
;
;Abstract:
;    Driver INF file for installing Authentec Swipe
;    sensor WDF drivers on x86 and x64 platforms.
;
;    NOTE: Currently not supporting IA64 platforms.

;--*/

[Version]
Signature="$WINDOWS NT$"
Class=Biometric
ClassGUID={53D29EF7-377C-4D14-864B-EB3A85769359}
provider=%Authentec%
DriverVer=10/02/2008,8.1.2.37
CatalogFile.NTx86   = ATSwpWDF.cat
CatalogFile.NTamd64 = AtswpWDFAMD64.cat


; ================= Class section =====================

[ClassInstall32.NT]
Addreg=BiometricClassReg

[BiometricClassReg]
HKR,,,,%ClassName%
HKR,,NoInstallClass,,1
HKR,,Icon,,-30


; ================= Device Install section =====================

;
; Manufacturer section
;  This consists of [Manufacturer][Models] with the
;	supported OS platform decorations
;
;
[Manufacturer]
%MfgName%=AuthentecModels,NTx86,NTamd64

;-----------------------------------------------------------------
; Models for Win2K, x86 based machines
;
;These are the VID/PIDs reserved for AuthenTec reference boards.
;
[AuthentecModels]
%AES2550REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2550
%AES2810REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2810
%AES2500REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2500
%AES2501REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2501
%AES2502REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2502
%AES2503REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2503
%AES2504REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2504
%AES2505REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2505
%AES2506REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2506
%AES2507REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2507
%AES2508REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2508
%AES2509REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2509
%AES250AREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250A
%AES250BREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250B
%AES250CREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250C
%AES250DREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250D
%AES250EREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250E
%AES250FREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250F
%AES2580REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2580
%AES2588REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2588
%AES2589REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2589
%AES258AREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258A
%AES258BREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258B
%AES258CREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258C
%AES258DREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258D
%AES258EREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258E
%AES258FREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258F

;-----------------------------------------------------------------
; Models for XP or later, x86 based machines
;
[AuthentecModels.NTx86]
%AES2550REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2550
%AES2810REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2810
%AES2500REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2500
%AES2501REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2501
%AES2502REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2502
%AES2503REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2503
%AES2504REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2504
%AES2505REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2505
%AES2506REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2506
%AES2507REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2507
%AES2508REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2508
%AES2509REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2509
%AES250AREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250A
%AES250BREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250B
%AES250CREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250C
%AES250DREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250D
%AES250EREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250E
%AES250FREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250F
%AES2580REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2580
%AES2588REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2588
%AES2589REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2589
%AES258AREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258A
%AES258BREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258B
%AES258CREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258C
%AES258DREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258D
%AES258EREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258E
%AES258FREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258F

;-----------------------------------------------------------------
; Models for AMD64 (or Intel EM64T) based machines
;
[AuthentecModels.NTamd64]
%AES2550REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2550
%AES2810REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2810
%AES2500REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2500
%AES2501REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2501
%AES2502REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2502
%AES2503REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2503
%AES2504REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2504
%AES2505REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2505
%AES2506REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2506
%AES2507REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2507
%AES2508REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2508
%AES2509REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2509
%AES250AREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250A
%AES250BREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250B
%AES250CREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250C
%AES250DREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250D
%AES250EREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250E
%AES250FREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_250F
%AES2580REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2580
%AES2588REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2588
%AES2589REFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_2589
%AES258AREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258A
%AES258BREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258B
%AES258CREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258C
%AES258DREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258D
%AES258EREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258E
%AES258FREFBoard%=ATSwpWDF_Inst, USB\VID_08FF&PID_258F


; ================= File Copy section =====================

[ATSwpWDF_Inst]
CopyFiles=ATSwpWDFCopy

[ATSwpWDFCopy]
ATSwpWDF.sys

;[SourceDisksNames]
;1=%Disk_Description%,,,

[DestinationDirs]
DefaultDestDir = 12

[SourceDisksFiles]
ATSwpWDF.sys = 1

[SourceDisksNames.x86]
1=%Disk1Name%,,,\i386

[SourceDisksNames.amd64]
1=%Disk1Name%,,,\amd64

; ================= Service Installation section =====================

[ATSwpWDF_Inst.Services]
Addservice = ATSwpWDF, 0x00000002, ATSwpWDF.AddService

[ATSwpWDF.AddService]
DisplayName    = %ATSwpWDF.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\ATSwpWDF.sys
AddReg         = ATSwpWDF.AddReg
LoadOrderGroup = Base

[ATSwpWDF.AddReg]
HKR, Parameters\Wdf, VerboseOn,       0x00010001, 1
HKR, Parameters\Wdf, VerifierOn,      0x00010001, 1
HKR, Parameters\Wdf, DbgBreakOnError, 0x00010001, 1
HKR,,"DriverVersion",0,%DriverVersionInfo%


; ================= WDF Coinstaller Installation section =====================

[DestinationDirs]
CoInstaller_CopyFiles = 11

[ATSwpWDF_Inst.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[CoInstaller_CopyFiles]
WdfCoinstaller01005.dll

[SourceDisksFiles]
WdfCoinstaller01005.dll=1 ; make sure the number matches with SourceDisksNames

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "WdfCoinstaller01005.dll,WdfCoInstaller"

[ATSwpWDF_Inst.Wdf]
KmdfService = ATSwpWDF, ATSwpWDF_wdfsect

[ATSwpWDF_wdfsect]
KmdfLibraryVersion = 1.5

; ================= Strings section =====================

[Strings]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "Personal Identification Devices"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"

; Spanish (Spain)
[Strings.040A]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "Dispositivos de identificación personal"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"

; Spanish (Mexico)
[Strings.080A]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "Dispositivos de identificación personal"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"

; French
[Strings.040C]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "Dispositifs d'identification personnelle"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"

; Portugese (Brazil)
[Strings.0416]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "Dispositivos de identificação pessoal"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"

; German
[Strings.0407]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "Geräte zur Personenidentifizierung"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"

; Italian
[Strings.0410]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "Dispositivi di identificazione personale"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"

; Japanese
[Strings.0411]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "個人認証デバイス"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"

; Simplified Chinese
[Strings.0804]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "个人身份识别设备"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"

; Traditional Chinese
[Strings.0404]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "個人身份識別裝置"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"

; Traditional Korean
[Strings.0404]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "개인 식별 장치"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"

; Swedish (Finland)
[Strings.081D]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "Henkilökohtaiset todennuslaitteet"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"

; Danish
[Strings.0406]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "Enheder til personlig identifikation"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"

; Norwegian
[Strings.0414]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "Enheter for personlig identifikasjon"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"

; Dutch
[Strings.0413]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES2550REFBoard=" AuthenTec Inc. AES2550"
AES2810REFBoard=" AuthenTec Inc. AES2810"
AES2500REFBoard=" AuthenTec Inc. AES2501"
AES2501REFBoard=" AuthenTec Inc. AES2501"
AES2502REFBoard=" AuthenTec Inc. AES2501"
AES2503REFBoard=" AuthenTec Inc. AES2501"
AES2504REFBoard=" AuthenTec Inc. AES2501"
AES2505REFBoard=" AuthenTec Inc. AES2501"
AES2506REFBoard=" AuthenTec Inc. AES2501"
AES2507REFBoard=" AuthenTec Inc. AES2501"
AES2508REFBoard=" AuthenTec Inc. AES2501"
AES2509REFBoard=" AuthenTec Inc. AES2501"
AES250AREFBoard=" AuthenTec Inc. AES2501"
AES250BREFBoard=" AuthenTec Inc  AES2501"
AES250CREFBoard=" AuthenTec Inc. AES2501"
AES250DREFBoard=" AuthenTec Inc. AES2501"
AES250EREFBoard=" AuthenTec Inc. AES2501"
AES250FREFBoard=" AuthenTec Inc. AES2501"
AES2580REFBoard=" AuthenTec Inc. AES2501A"
AES2588REFBoard=" AuthenTec Inc. AES2501A"
AES2589REFBoard=" AuthenTec Inc. AES2501A"
AES258AREFBoard=" AuthenTec Inc. AES2501A"
AES258BREFBoard=" AuthenTec Inc. AES2501A"
AES258CREFBoard=" AuthenTec Inc. AES2501A"
AES258DREFBoard=" AuthenTec Inc. AES2501A"
AES258EREFBoard=" AuthenTec Inc. AES2501A"
AES258FREFBoard=" AuthenTec Inc. AES2501A"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB WDF Driver"
ClassName       = "Persoonlijke identificatieapparaten"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="8.1.2.37"
