
[Version]
Signature="$WINDOWS NT$"
Class=SCSIAdapter
ClassGuid={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%VIA%
DriverVer=12/23/2008,5.1.6000.0300

[DestinationDirs]
DefaultDestDir = 12

[SourceDisksNames]
1 = %DiskId1%,,,""

[SourceDisksFiles]
vcrdrx32.sys  = 1

;*****************************************
; VIA Card Reader Driver Install Section
; Host Controller : SD/MMC/MS/MS Pro/XD
;*****************************************

[Manufacturer]
%StdMfg%=Standard,NTx86

; For Win2K because it cannot parse decorated sections
[Standard]
%VIA.SD.MS.DeviceDesc%=VIACardReader, PCI\VEN_1106&DEV_9530

; For XP and later
[Standard.NTx86]
%VIA.SD.MS.DeviceDesc%=VIACardReader, PCI\VEN_1106&DEV_9530

[VIACardReader.NT]
CopyFiles=Drivers_Dir

[VIACardReader.NT.HW]
AddReg=VIACardReader.NT.AddReg

[VIACardReader.NT.AddReg]                            
HKR,,DeviceCharacteristics,0x10001,0x0100         ; Use same security checks on relative opens
HKR,,Security,,"D:P(A;;GA;;;BA)(A;;GA;;;SY)"      ; Allow generic-all access to Built-in administrators and Local system 

[Drivers_Dir]
vcrdrx32.sys

;-------------- Service installation
[VIACardReader.NT.Services]
AddService = vcrdrx32,%SPSVCINST_ASSOCSERVICE%, CardReader_Service_Inst

; -------------- dynambus driver install sections
[CardReader_Service_Inst]
DisplayName    = %VIACardReaderDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START 
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\vcrdrx32.sys
LoadOrderGroup = SCSI Miniport


[Strings]
SPSVCINST_ASSOCSERVICE= 0x00000002
VIA = "VIA Technologies, Inc"
StdMfg = "(VIA MSP Cardreader driver)"
DiskId1 = "VIA MSP Cardreader driver Installation Disk #1"
VIA.SD.MS.DeviceDesc = "VIA MSP Cardreader Host Controller"
VIACardReaderDESC = "VIA MSP Cardreader Host Controller"