;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;
; Fidtblt.inf
; Installation file (.inf) for the Touch Panel Device.
; (For the WindowsXP TabletPC Edition)
;
; (c) Copyright 2005-2006 Fujitsu Component Ltd. 
;
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;

[version]
signature="$WINDOWS NT$"
Class=HIDClass
ClassGuid={745a17a0-74d3-11d0-b6fe-00a0c90f57da}
Provider=%PFCL%
CatalogFile = Fidtblt.cat
DriverVer=08/18/2006,1.0.1.4

[ControlFlags]
ExcludeFromSelect=*

[DestinationDirs]
DefaultDestDir          =11     ;LDID_SYS
FCLPenInst.NT.Copy      =12     ;LDID_DRIVERS

; Drivers
;----------------------------------------------------------
[Manufacturer]
%FCL%=FCL

[FCL]
%FCLTablet.DeviceDesc%      =FCLPenInst,ACPI\LTS0001

[FCLPenInst.NT]
CopyFiles                   =FCLPenInst.NT.Copy, FCLHidPen.Copy

[FCLPenInst.NT.Copy]
Fidtblt.sys

[FCLHidPen.Copy]
Fidtbrv.exe
Fidtbrv.del
FCLTBLT.cpl
CalTBwin.exe
FTIMV.dll

[FCLPenInst.NT.HW]
AddReg                      =SerialInst.NT.HW.AddReg

[FCLPenInst.NT.Services]
AddService                  =FCLPen,0x00000002,FCLPenServiceInst,FCLEventLogInst
AddService                  =Serial,,SerialServiceInst, SerialEventLogInst

[FCLEventLogInst]
AddReg                      =FCLEventLogAddReg

[FCLEventLogAddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\Fidtblt.sys"
HKR,,TypesSupported,0x00010001,7

HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\FPENRMV,"DisplayName",,"FCL Serial Pen Tablet"
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\FPENRMV,"UninstallString",,"Fidtbrv.exe"


; -------------- FCL Pen Driver install section
[FCLPenServiceInst]
DisplayName    = %FCLPen.SVCDESC%
ServiceType    = 1       ; SERVICE_KERNEL_DRIVER
StartType      = 3       ;
ErrorControl   = 1       ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\Fidtblt.sys
LoadOrderGroup = Extended Base

[SerialInst.NT.HW.AddReg]
HKR,,"LowerFilters",0x00010000,"serial"
HKR,,"MultiportDevice",0x00010001,0

[SerialEventLogInst]
AddReg         = SerialEventLogAddReg

[SerialEventLogAddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\serial.sys"
HKR,,TypesSupported,0x00010001,7

; -------------- Serial Port Driver install sections
[SerialServiceInst]
DisplayName    = %Serial.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 0               ; SERVICE_ERROR_IGNORE
ServiceBinary  = %12%\serial.sys
LoadOrderGroup = Extended base

;--------------------------------------------------------------
; Source file information
;
[SourceDisksNames.x86]
1 = %DiskId1%,,,""

[SourceDisksFiles]
Fidtblt.sys   = 1,,
Fidtbrv.del   = 1,,
Fidtbrv.exe   = 1,,
FCLTBLT.cpl   = 1,,
CalTBwin.exe  = 1,,
FTIMV.dll     = 1,,

[Strings]
PFCL="Fujitsu Component Ltd."
FCL="FCL"
FCLTablet.DeviceDesc="FCL Serial Pen Tablet"
FCLPen.SVCDESC="FCL Serial Pen HID Driver"
Serial.SVCDESC="Serial Port Driver"
DiskId1="FCL Installation Disk #1"
