;*******************************************************
; Copyright 2000 ATMEL.
; AT76C503A based FastVNET USB 11M Network Adapter
; INF file for the NDIS driver
;
; Windows XP
;



[Version]
Signature  = "$Windows NT$"
Class      = Net
ClassGUID  = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider   = %ATMEL%
;CatalogFile = netvusbr.cat
DriverVer  = 12/10/2001,1.2.2.58

[Manufacturer]
%ATMEL%   = ATMEL

[ControlFlags]
ExcludeFromSelect = VID_03eb&PID_7605


[ATMEL]
%USBFVNETR.DeviceDesc% = USBFVNETR.Ndi,USB\VID_03eb&PID_7605

;*******************************************************************************
; Win XP main sections
;*******************************************************************************


[USBFVNETR.Ndi.NT]
Characteristics = 0x84  ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 15    ; USB
AddReg          = USBFVNETR.NT.Reg, USBFVNETR.Params
CopyFiles       = CopyFile.NT.Sys
DriverVer  = 12/10/2001,1.2.2.58

[USBFVNETR.Ndi.NT.Services]
AddService = USBFVNETR, 2, USBFVNETR.Service, Common.EventLog

;*******************************************************************************
; Driver parameters
;*******************************************************************************

[USBFVNETR.Params]
HKR, Ndi\params\Rate,               ParamDesc,          0, "Rate (Mbps)"
HKR, Ndi\params\Rate,           default,        0, "3"
HKR, Ndi\params\Rate,               type,           0, "enum"
HKR, Ndi\params\Rate\enum,      0,          0, "1"
HKR, Ndi\params\Rate\enum,      1,          0, "2"
HKR, Ndi\params\Rate\enum,      2,          0, "5.5"
HKR, Ndi\params\Rate\enum,      3,          0, "11"
HKR, Ndi\params\Rate\enum,      4,          0, "Auto"
HKR, ,                                  Rate,           0, "3"

HKR, Ndi\params\RTS_Threshold,          ParamDesc,          0, "RTS Threshold"
HKR, Ndi\params\RTS_Threshold,      default,        0, "2347"
HKR, Ndi\params\RTS_Threshold,          type,           0, "int"
HKR, Ndi\params\RTS_Threshold,      min,            0, "0"
HKR, Ndi\params\RTS_Threshold,      max,            0, "2347"
HKR, Ndi\params\RTS_Threshold,      step,           0, "1"
HKR, ,                                  RTS_Threshold,      0, "2347"

HKR, Ndi\params\Frag_Threshold,         ParamDesc,          0, "Fragmentation Threshold"
HKR, Ndi\params\Frag_Threshold,     default,        0, "2346"
HKR, Ndi\params\Frag_Threshold,         type,           0, "int"
HKR, Ndi\params\Frag_Threshold,     min,            0, "256"
HKR, Ndi\params\Frag_Threshold,     max,            0, "2346"
HKR, Ndi\params\Frag_Threshold,     step,           0, "1"
HKR, ,                                  Frag_Threshold,     0, "2346"

HKR, Ndi\params\PreambleType,           ParamDesc,          0, "Preamble Type"
HKR, Ndi\params\PreambleType,       default,        0, "0"
HKR, Ndi\params\PreambleType,           type,           0, "enum"
HKR, Ndi\params\PreambleType\enum,  0,          0, "Long"
HKR, Ndi\params\PreambleType\enum,  1,          0, "Short"
HKR, Ndi\params\PreambleType\enum,  2,          0, "Auto"
HKR, ,                                  PreambleType,       0, "2"



;*******************************************************************************
; Install section for Windows XP
;*******************************************************************************

[USBFVNETR.NT.Reg]
; Interfaces
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi,            Service,    0, "USBFVNETR"

[USBFVNETR.Service]
DisplayName    = %USBFVNETR.DisplayName%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\vnetusbr.sys
LoadOrderGroup = NDIS


[Common.EventLog]
AddReg = Common.AddEventLog.Reg

[Common.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll, %%SystemRoot%%\System32\drivers\vnetusbr.sys
HKR, , TypesSupported  , 0x00010001, 7


[CopyFile.NT.Sys]
vnetusbr.sys,,,2

;*******************************************************************************
; Destination directories
;*******************************************************************************

[DestinationDirs]
DefaultDestDir   = 12 ; Drivers directory
CopyFile.NT.Sys  = 12


[SourceDisksNames]
50=%DriverDisketteName%,,

[SourceDisksFiles]
vnetusbr.sys=50,.,vnetusbr.sys,10000

;*******************************************************************************
; Localizable strings
;*******************************************************************************

[Strings]
ATMEL = "ATMEL"
USBFVNETR.DeviceDesc = "ATMEL USB FastVNET (AR)"
USBFVNETR.DisplayName = "ATMEL USB FastVNET (AR)"
DriverDisketteName      = "ATMEL USB FastVNET (AR) Drivers Disk"
Help_Text = "VirtualNET lets you set up easily and operate a Wireless LAN compliant with 802.11 Standard. It operates in the license free 2.4 GHz ISM band and achieves a peak data rate of 11 Mbs."
