; netm4cx.inf created 22-Jun-2006
;
; D-Link DGE-5xx Gigabit Ethernet Adapter 
;
; (C)Copyright 2002-2006 Marvell(R).
; 
; All rights reserved.
;
; INF File for NDIS5.1 Miniport Driver for Windows XP and Server 2003 (x86) M4CXW2K3.sys v8.39.10.3

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4D36E972-E325-11CE-BFC1-08002BE10318}
Provider	= %D-Link%
CatalogFile	= m4cxw2k3.CAT
DriverVer=06/22/2006, 8.39.10.3

[Manufacturer]


%D-Link%	= D-Link, NT.5.1, NT.5.2, NT.6.0



[ControlFlags]

ExcludeFromSelect	= *


;-----------------------------------------------------------------------------
;
;       Windows 2000
;
;-----------------------------------------------------------------------------
[D-Link]
;Empty section

;-----------------------------------------------------------------------------
;
;       Windows XP
;
;-----------------------------------------------------------------------------
[D-Link.NT.5.1]
%Dlink.DeviceDesc4360%	= SLYuk2CopGig.ndi, PCI\VEN_1186&DEV_4B00&SUBSYS_4B001186
%Dlink.DeviceDesc4320%	= SLYukCopGig.ndi, PCI\VEN_1186&DEV_4C00&SUBSYS_4C001186
%Dlink.DeviceDesc4320%	= SLYukCopGig.ndi, PCI\VEN_1186&DEV_4B01&SUBSYS_4B011186
%Dlink.DeviceDesc4346%	= SLYuk2FibGig.ndi, PCI\VEN_1186&DEV_4B02&SUBSYS_4B021186
%Dlink.DeviceDesc550SX%	= SLYuk2FibGig.ndi, PCI\VEN_1186&DEV_4001&SUBSYS_40011186


;-----------------------------------------------------------------------------
;
;       Windows Server 2003
;
;-----------------------------------------------------------------------------
[D-Link.NT.5.2]
%Dlink.DeviceDesc4360%	= SLYuk2CopGig.ndi, PCI\VEN_1186&DEV_4B00&SUBSYS_4B001186
%Dlink.DeviceDesc4320%	= SLYukCopGig.ndi, PCI\VEN_1186&DEV_4C00&SUBSYS_4C001186
%Dlink.DeviceDesc4320%	= SLYukCopGig.ndi, PCI\VEN_1186&DEV_4B01&SUBSYS_4B011186
%Dlink.DeviceDesc4346%	= SLYuk2FibGig.ndi, PCI\VEN_1186&DEV_4B02&SUBSYS_4B021186
%Dlink.DeviceDesc550SX%	= SLYuk2FibGig.ndi, PCI\VEN_1186&DEV_4001&SUBSYS_40011186


;-----------------------------------------------------------------------------
;
;       Windows Longhorn
;
;-----------------------------------------------------------------------------
[D-Link.NT.6.0]
;Empty section


;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <single link Version 2.0 Copper>

[SLYukCopGig.ndi]
DelReg= m4cxw2k3.delreg
AddReg		= m4cxw2k3.reg, m4cxw2k3.params, m4cxw2k3.SingleLink.params, m4cxw2k3.SLSpeedDuplex.params.DLK , m4cxw2k3.TxRxBuff.params, m4cxw2k3.WoL.params, m4cxw2k3.GigFrSize.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= m4cxw2k3.CopyFiles

[SLYukCopGig.ndi.Services]
AddService	= m4cxw2k3, 2, m4cxw2k3.Service, common.EventLog
;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <single link Copper>

[SLYuk2CopGig.ndi]
DelReg= m4cxw2k3.delreg
AddReg		= m4cxw2k3.reg, m4cxw2k3.params, m4cxw2k3.SingleLink.params, m4cxw2k3.SLSpeedDuplex.params, m4cxw2k3.TxRxLE.params, m4cxw2k3.WoL.params, m4cxw2k3.GigFrSize.params, m4cxw2k3.TcpSegm.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= m4cxw2k3.CopyFiles

[SLYuk2CopGig.ndi.Services]
AddService	= m4cxw2k3, 2, m4cxw2k3.Service, common.EventLog

;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <single link Fiber>

[SLYuk2FibGig.ndi]
DelReg= m4cxw2k3.delreg
AddReg		= m4cxw2k3.reg, m4cxw2k3.params, m4cxw2k3.SingleLink.params, m4cxw2k3.TxRxLE.params, m4cxw2k3.GigFrSize.params, m4cxw2k3.TcpSegm.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= m4cxw2k3.CopyFiles

[SLYuk2FibGig.ndi.Services]
DelService = ___DELMRVLSERVICENAME__, 204
DelService = ___DELSKSERVICENAME__, 204
AddService	= m4cxw2k3, 2, m4cxw2k3.Service, common.EventLog


;-----------------------------------------------------------------------------
;
; General Driver Parameters
;
;-----------------------------------------------------------------------------
[m4cxw2k3.params]

HKR, Ndi\Params\HwChecksum,		ParamDesc,	0, %HwCsum%
HKR, Ndi\Params\HwChecksum,		Type,		0, "enum"
HKR, Ndi\Params\HwChecksum\enum,	"1",			0, %On%
HKR, Ndi\Params\HwChecksum\enum,	"0",			0, %Off%
HKR, Ndi\Params\HwChecksum,		Default,		0, "1"

HKR, Ndi\Params\MessageLog,		ParamDesc,	0, %LogMsg%
HKR, Ndi\Params\MessageLog,		Type,		0, "enum"
HKR, Ndi\Params\MessageLog\enum,	"4",			0, %Non%
HKR, Ndi\Params\MessageLog\enum,	"3",			0, %Err%
HKR, Ndi\Params\MessageLog\enum,	"2",			0, %Wrn%
HKR, Ndi\Params\MessageLog\enum,	"1",			0, %Sta%
HKR, Ndi\Params\MessageLog\enum,	"0",			0, %All%
HKR, Ndi\Params\MessageLog,		Default,		0, "1"

HKR, Ndi\Params\NetworkAddress,	ParamDesc,	0, %NetAddress%
HKR, Ndi\Params\NetworkAddress,	Type,		0, "edit"
HKR, Ndi\Params\NetworkAddress,	LimitText,	0, "18"
HKR, Ndi\Params\NetworkAddress,	UpperCase,	0, "1"
HKR, Ndi\Params\NetworkAddress,	Default,		0, ""
HKR, Ndi\Params\NetworkAddress,	Optional,		0, "1"

HKR, Ndi\Params\Moderate,		ParamDesc,	0, %IntMod%
HKR, Ndi\Params\Moderate,		Type,		0, "enum"
HKR, Ndi\Params\Moderate\enum,	"1",			0, %On%
HKR, Ndi\Params\Moderate\enum,	"0",			0, %Off%
HKR, Ndi\Params\Moderate,		Default,		0, "1"

HKR, Ndi\Params\FixedIntMod,	ParamDesc,	0, %MaxIrq%
HKR, Ndi\Params\FixedIntMod,	Type,		0, "int"
HKR, Ndi\Params\FixedIntMod,	Base,		0, "10"
HKR, Ndi\Params\FixedIntMod,	Min,			0, "1000"
HKR, Ndi\Params\FixedIntMod,	Max,			0, "30000"
HKR, Ndi\Params\FixedIntMod,	Step,		0, "1"
HKR, Ndi\Params\FixedIntMod,	Default,		0, "5000"


;-----------------------------------------------------------------------------
;
; Additional driver parameters for TX/RX buffers (V1 and V2)
;
;-----------------------------------------------------------------------------
[m4cxw2k3.TxRxBuff.params]



HKR, Ndi\Params\MaxReceives,	ParamDesc,	0, %NumRcv%
HKR, Ndi\Params\MaxReceives,	Type,		0, "int"
HKR, Ndi\Params\MaxReceives,	Base,		0, "10"
HKR, Ndi\Params\MaxReceives,	Min,			0, "3"
HKR, Ndi\Params\MaxReceives,	Max,			0, "500"
HKR, Ndi\Params\MaxReceives,	Step,		0, "1"
HKR, Ndi\Params\MaxReceives,	Default,		0, "50"

HKR, Ndi\Params\MaxTransmits,	ParamDesc,	0, %NumTx%
HKR, Ndi\Params\MaxTransmits,	Type,		0, "int"
HKR, Ndi\Params\MaxTransmits,	Base,		0, "10"
HKR, Ndi\Params\MaxTransmits,	Min,			0, "4"
HKR, Ndi\Params\MaxTransmits,	Max,			0, "200"
HKR, Ndi\Params\MaxTransmits,	Step,		0, "1"
HKR, Ndi\Params\MaxTransmits,	Default,		0, "50"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for TX/RX LE (Y2)
;
;-----------------------------------------------------------------------------
[m4cxw2k3.TxRxLE.params]


HKR, Ndi\Params\MaxReceives,	ParamDesc,	0, %NumRcv%
HKR, Ndi\Params\MaxReceives,	Type,		0, "int"
HKR, Ndi\Params\MaxReceives,	Base,		0, "10"
HKR, Ndi\Params\MaxReceives,	Min,			0, "256"
HKR, Ndi\Params\MaxReceives,	Max,			0, "512"
HKR, Ndi\Params\MaxReceives,	Step,		0, "128"
HKR, Ndi\Params\MaxReceives,	Default,		0, "256"

HKR, Ndi\Params\MaxTransmits,	ParamDesc,	0, %NumTx%
HKR, Ndi\Params\MaxTransmits,	Type,		0, "int"
HKR, Ndi\Params\MaxTransmits,	Base,		0, "10"
HKR, Ndi\Params\MaxTransmits,	Min,			0, "256"
HKR, Ndi\Params\MaxTransmits,	Max,			0, "512"
HKR, Ndi\Params\MaxTransmits,	Step,		0, "128"
HKR, Ndi\Params\MaxTransmits,	Default,		0, "256"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for Maximum Frame Size (10/100/1000 chip)
;
;-----------------------------------------------------------------------------
[m4cxw2k3.GigFrSize.params]


HKR, Ndi\Params\MaxFrameSize,           ParamDesc,      0, %MaxFrSize%
HKR, Ndi\Params\MaxFrameSize,           default,        0, "1514"
HKR, Ndi\Params\MaxFrameSize\Enum,      "1514",         0, %Disabled%
HKR, Ndi\Params\MaxFrameSize\Enum,      "4088",         0, %Bytes4088%
HKR, Ndi\Params\MaxFrameSize\Enum,      "9014",         0, %Bytes9014%
HKR, Ndi\Params\MaxFrameSize,           type,           0, "enum"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan
;
;-----------------------------------------------------------------------------
[m4cxw2k3.WoL.params]


HKR, Ndi\Params\WakeUpModeCap_A,		ParamDesc,	0, %WakeUpCaps%
HKR, Ndi\Params\WakeUpModeCap_A,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"0",		0, %Non%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"25",		0, %Magic Packet%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"26",		0, %Pattern Match%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"27",		0, %Mag Pack Patt Match%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"28",		0, %Link Change%
HKR, Ndi\Params\WakeUpModeCap_A,		Default,	0, "27"

HKR, Ndi\Params\WakeFromShutdown,		ParamDesc,	0, %WakeFromShut%
HKR, Ndi\Params\WakeFromShutdown,		Type,		0, "enum"
HKR, Ndi\Params\WakeFromShutdown\enum,	"1",		0, %On%
HKR, Ndi\Params\WakeFromShutdown\enum,	"0",		0, %Off%
HKR, Ndi\Params\WakeFromShutdown,		Default,	0, "0"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for TCP segmentation
;
;-----------------------------------------------------------------------------
[m4cxw2k3.TcpSegm.params]

HKR, Ndi\Params\TcpLargeSend,		ParamDesc,	0, %TcpSegmentation%
HKR, Ndi\Params\TcpLargeSend,		Type,		0, "enum"
HKR, Ndi\Params\TcpLargeSend\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\TcpLargeSend\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\TcpLargeSend,		Default,	0, "1"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for Single Link Adapters
;
;-----------------------------------------------------------------------------
[m4cxw2k3.SingleLink.params]

HKR, Ndi\Params\TagHeaderSupport_A,			ParamDesc,	0, %QoSSup%
HKR, Ndi\Params\TagHeaderSupport_A,			Type,		0, "enum"
HKR, Ndi\Params\TagHeaderSupport_A\enum,	"1",		0, %On%
HKR, Ndi\Params\TagHeaderSupport_A\enum,	"0",		0, %Off%
HKR, Ndi\Params\TagHeaderSupport_A,			Default,	0, "0"

HKR, Ndi\Params\FlowControl_A,		ParamDesc,	0, %FlowCtrl%
HKR, Ndi\Params\FlowControl_A,		Type,		0, "enum"
HKR, Ndi\Params\FlowControl_A\enum,	"3",		0, %On%
HKR, Ndi\Params\FlowControl_A\enum,	"0",		0, %Off%
HKR, Ndi\Params\FlowControl_A,		Default,	0, "3"



HKR,, MaxMulticast,,         "128"
HKR,, WaitForRxResources,,   "1"
HKR,, SGMapRegistersNeeded,, "64"

;-----------------------------------------------------------------------------
;
; Additional driver parameter to set the port speed and capabilities
;
;-----------------------------------------------------------------------------
[m4cxw2k3.SLSpeedDuplex.params]


HKR,Ndi\Params\ConnectionType_A,      ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\Params\ConnectionType_A,      Type,       0, "enum"
HKR,Ndi\Params\ConnectionType_A,      Default,    0, "0"
HKR,Ndi\Params\ConnectionType_A\enum, "0",        0, %Autosense%
HKR,Ndi\Params\ConnectionType_A\enum, "1",        0, %10MHD%
HKR,Ndi\Params\ConnectionType_A\enum, "2",        0, %10MFD%
HKR,Ndi\Params\ConnectionType_A\enum, "3",        0, %100MHD%
HKR,Ndi\Params\ConnectionType_A\enum, "4",        0, %100MFD%

;-----------------------------------------------------------------------------
;
; Additional driver parameter to set the port speed and capabilities
;
;-----------------------------------------------------------------------------
[m4cxw2k3.SLSpeedDuplex.params.DLK]


HKR,Ndi\Params\ConnectionType_A,      ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\Params\ConnectionType_A,      Type,       0, "enum"
HKR,Ndi\Params\ConnectionType_A,      Default,    0, "0"
HKR,Ndi\Params\ConnectionType_A\enum, "0",        0, %Autosense%
HKR,Ndi\Params\ConnectionType_A\enum, "1",        0, %10MHD%
HKR,Ndi\Params\ConnectionType_A\enum, "2",        0, %10MFD%
HKR,Ndi\Params\ConnectionType_A\enum, "3",        0, %100MHD%
HKR,Ndi\Params\ConnectionType_A\enum, "4",        0, %100MFD%
HKR,Ndi\Params\ConnectionType_A\enum, "5",        0, %1000MFD%

;-----------------------------------------------------------------------------
;
; General Registry Entries
;
;-----------------------------------------------------------------------------
[m4cxw2k3.reg]

HKR, Ndi\Interfaces, UpperRange,, "ndis5"

HKR, Ndi\Interfaces, LowerRange,, "ethernet"
HKR, Ndi, Service,, "m4cxw2k3"


;-----------------------------------------------------------------------------
;
; This section contain the keys which will be deleted. These are old keys 
; which are not any more supported in newest INF.
;
;-----------------------------------------------------------------------------
[m4cxw2k3.delreg]
; remove the "OS Controlled" (15) subkey from WakeUpModeCap_X
HKR, Ndi\Params\WakeUpModeCap_A\enum,15
HKR, Ndi\Params\WakeUpModeCap_B\enum,15
HKR, Ndi\Params\DuplexCapabilities_A
HKR, Ndi\Params\DuplexCapabilities_B
HKR, Ndi\Params\FlowControl_A
HKR, Ndi\Params\FlowControl_B
HKR, Ndi\Params\AutoNegotiation_A
HKR, Ndi\Params\AutoNegotiation_B
HKR, Ndi\Params\Role_A
HKR, Ndi\Params\Role_B
HKR, Ndi\Params\Speed_A
HKR, Ndi\Params\Speed_B
HKR, Ndi\Params\MaxFrameSize


;-----------------------------------------------------------------------------
;
; Service
;
;-----------------------------------------------------------------------------
[m4cxw2k3.Service]
DisplayName	= %m4cxw2k3.DriverDesc%
ServiceType	= 1
StartType = 3
ErrorControl = 1
ServiceBinary  = %12%\m4cxw2k3.sys
LoadOrderGroup = NDIS


;-----------------------------------------------------------------------------
;
;
;
;-----------------------------------------------------------------------------
[common.EventLog]
AddReg = common.AddEventLog.reg

;-----------------------------------------------------------------------------
;
;
;
;-----------------------------------------------------------------------------
[common.AddEventLog.reg]
HKR,, EventMessageFile,	0x00020000, "%%SystemRoot%%\System32\Drivers\m4cxw2k3.sys"
HKR,, TypesSupported,	0x00010001, 7


;-----------------------------------------------------------------------------
;
; Source Files
;
;-----------------------------------------------------------------------------
[SourceDisksNames]
1 = %DriverDisk%,,,

[SourceDisksFiles]
m4cxw2k3.sys	= 1,,

[m4cxw2k3.CopyFiles]
m4cxw2k3.sys,,,2


;-----------------------------------------------------------------------------
;
; Destination Directories
;
;-----------------------------------------------------------------------------
[DestinationDirs]

DefaultDestDir = 12
m4cxw2k3.CopyFiles	= 12

;-----------------------------------------------------------------------------
;
; Localizable Strings
;
;-----------------------------------------------------------------------------
[Strings]
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "Network Address"
HwCsum = "Hardware Checksumming"
WakeUpCaps   = "Wake Up Capabilities"
IntMod = "Interrupt Moderation"
MaxIrq = "Max IRQ per Sec"
LogMsg = "Log Status Messages"
NumRcv = "Number of Receive Buffers"
NumTx  = "Number of Transmit Buffers"
RLMT  = "RLMT Mode"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Preferred Port"
On = "On"
Off = "Off"
Enabled = "Enabled"
Disabled = "Disabled"
Non = "None"
Err = "Errors"
Wrn = "Warnings"
Sta = "Status Messages"
All = "All Messages"
A = "A"
B = "B"
Autosense = "Auto-Sense"
10MHD = "10Mbps Half Duplex"
10MFD = "10Mbps Full Duplex"
100MHD = "100Mbps Half Duplex"
100MFD = "100Mbps Full Duplex"
1000MFD = "1000Mbps Full Duplex"
Magic Packet = "Magic Packet"
Pattern Match = "Pattern Match"
Mag Pack Patt Match = "Magic Packet & Pattern Match"
Link Change = "Link Change"
SpeedDuplex = "Speed & Duplex"
SpeedDuplexA = "Speed & Duplex Port A"
SpeedDuplexB = "Speed & Duplex Port B"
FlowCtrl = "FlowControl"
FlowCtrlA = "FlowControl Port A"
FlowCtrlB = "FlowControl Port B"
QoSSup = "802.1p Support"
QoSSupA = "802.1p Support Port A"
QoSSupB = "802.1p Support Port B"
WakeFromShut = "Wake From Shutdown"
TcpSegmentation = "TCP Segmentation"
BatSpeed = "BatterySpeedSettings"
Fast = "SmartSpeedDown"
Gig = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
MaxFrSize    = "Jumbo Frames"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;-----------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk Installation Disk"

Dlink.DeviceDesc4360	= "DGE-560T Gigabit PCI Express Ethernet Adapter"
Dlink.DeviceDesc4320	= "D-Link DGE-530T Gigabit Ethernet Adapter"
Dlink.DeviceDesc4346	= "DGE-560SX Single fiber Gigabit Ethernet PCI-E Adapter V.A1"
Dlink.DeviceDesc550SX = "DGE-550SX Single fiber Gigabit Ethernet PCI-X Adapter"
m4cxw2k3.DriverDesc	= "NDIS5.1 Miniport Driver for D-Link PCI Express Ethernet Controller"


;-----------------------------------------------------------------------------

; Chinese (Taiwan)
[Strings.0404]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "網路位址"
HwCsum = "硬體檢查總和"
WakeUpCaps   = "喚醒功能"
IntMod = "中斷模式"
MaxIrq = "最大 IRQ數量"
LogMsg = "日誌狀態訊息"
NumRcv = "接收緩衝區數量"
NumTx  = "傳輸緩衝區數量"
RLMT  = "RLMT 模式"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "偏好埠"
On = "開啟"
Off = "關閉"
Enabled = "啟用"
Disabled = "禁用"
Non = "無"
Err = "錯誤"
Wrn = "警告"
Sta = "狀態訊息"
All = "所有訊息"
A = "A"
B = "B"
Autosense = "自動感應"
10MHD = "10Mbps 半雙工"
10MFD = "10Mbps 全雙工"
100MHD = "100Mbps 半雙工"
100MFD = "100Mbps 全雙工"
1000MFD = "1000Mbps 全雙工"
Magic Packet = "Magic Packet喚醒模式"
Pattern Match = "Pattern Match喚醒模式"
Mag Pack Patt Match = "Magic Packet & Pattern Match"
Link Change = "Link Change喚醒模式"
SpeedDuplex = "速度和雙工"
SpeedDuplexA = "端口A的速度和雙工"
SpeedDuplexB = "端口B的速度和雙工"
FlowCtrl = "流量控制"
FlowCtrlA = "流量控制 埠 A"
FlowCtrlB = "流量控制 埠 B"
QoSSup = "802.1p 支援"
QoSSupA = "802.1p 支援 埠 A"
QoSSupB = "802.1p 支援 埠 B"
WakeFromShut = "從關閉狀態下喚醒"
TcpSegmentation = "TCP分段"
BatSpeed = "電池狀態傳輸速度"
Fast = "智慧降速節能"
Gig = "全速"
BatLinkDet = "電池狀態鏈接偵測"
NoPwrSave = "無節能"
MaxPwrSave = "最大節能"
EnDetPwrSave = "EnergyDetect+™"
MaxFrSize    = "巨大封包"
Bytes4088 = "4088位元組"
Bytes9014 = "9014位元組";; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk"


Dlink.DeviceDesc4360	= "DGE-560T Gigabit PCI Express Ethernet Adapter"
Dlink.DeviceDesc4320	= "D-Link DGE-530T Gigabit Ethernet Adapter"
Dlink.DeviceDesc4346	= "DGE-560SX Single fiber Gigabit Ethernet PCI-E Adapter V.A1"
Dlink.DeviceDesc550SX = "DGE-550SX Single fiber Gigabit Ethernet PCI-X Adapter"
m4cxw2k3.DriverDesc	= "NDIS5.1 Miniport Driver for D-Link PCI Express Ethernet Controller"


; Chinese (PRC)
[Strings.0804]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "网络地址"
HwCsum = "硬件检查和"
WakeUpCaps   = "唤醒功能"
IntMod = "中断模式"
MaxIrq = "最大 IRQ数量"
LogMsg = "日志状态信息"
NumRcv = "接收缓存区数量"
NumTx  = "传送缓存区数量"
RLMT  = "RLMT 模式"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "首选端口"
On = "开"
Off = "关"
Enabled = "启用"
Disabled = "禁用"
Non = "无"
Err = "错误"
Wrn = "警告"
Sta = "状态信息"
All = "所有信息"
A = "A"
B = "B"
Autosense = "自动感应"
10MHD = "10Mbps 半双工"
10MFD = "10Mbps 全双工"
100MHD = "100Mbps 半双工"
100MFD = "100Mbps 全双工"
1000MFD = "1000Mbps 全双工"
Magic Packet = "Magic Packet唤醒模式"
Pattern Match = "Pattern Match唤醒模式"
Mag Pack Patt Match = "Magic Packet & Pattern Match"
Link Change = "Link Change唤醒模式"
SpeedDuplex = "速度和双工"
SpeedDuplexA = "端口A的速度和双工"
SpeedDuplexB = "端口B的速度和双工"
FlowCtrl = "流控制"
FlowCtrlA = "流控制端口 A"
FlowCtrlB = "流控制端口 B"
QoSSup = "801.1p 支持"
QoSSupA = "802.1p 支持端口 A"
QoSSupB = "802.1p 支持端口 B"
WakeFromShut = "从关闭状态下唤醒"
TcpSegmentation ="TCP分段"
BatSpeed = "电池状态传输速度"
Fast = "智慧降速节能"
Gig = "全速"
BatLinkDet = "电池状态链接侦测"
NoPwrSave = "无节能"
MaxPwrSave = "最大节能"
EnDetPwrSave = "EnergyDetect+™"
MaxFrSize    = "大帧"
Bytes4088 = "4088 个字节"
Bytes9014 = "9014 个字节"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk"


Dlink.DeviceDesc4360	= "DGE-560T Gigabit PCI Express Ethernet Adapter"
Dlink.DeviceDesc4320	= "D-Link DGE-530T Gigabit Ethernet Adapter"
Dlink.DeviceDesc4346	= "DGE-560SX Single fiber Gigabit Ethernet PCI-E Adapter V.A1"
Dlink.DeviceDesc550SX = "DGE-550SX Single fiber Gigabit Ethernet PCI-X Adapter"
m4cxw2k3.DriverDesc	= "NDIS5.1 Miniport Driver for D-Link PCI Express Ethernet Controller"
