2004/6/24 06:01¤U¤È;***********************************************************************
; PRISMA02.INF
;
;   IEEE 802.11g Wireless LAN CARDBUS/USB2.0 Adapters installation script.
;   Installs driver, network control panel app, coinstaller, advanced properties,
;   PRISM API, and PRISM server.
;   Supports Windows 2000 and XP.
;
;   Copyright 2004 IEEE 802.11g Wireless LAN.
;   All Rights Reserved
;***********************************************************************

[Version]
 DriverVer = 03/26/2004, 1.0.3
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
 ;CatalogFile         = PRISMA02.cat
 MillenniumPreferred = .ME

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = *

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]
 %A021_DESC_STR%     = PRISM_A021,        USB\VID_09AA&PID_1000
 %A022_DESC_STR%     = PRISM_A022,        USB\VID_0915&PID_2000
 
 %A001_DESC_STR%     = PRISM_A001,        PCI\VEN_1260&DEV_3890&SUBSYS_00001260
 %A002_DESC_STR%     = PRISM_A002,        PCI\VEN_1260&DEV_3886&SUBSYS_00001260
 %A002_DESC_STR%     = PRISM_A002,        PCI\VEN_1260&DEV_FFFF&SUBSYS_00001260

;==========
[PRISM_A021]       ; Win9x
 AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON_USB.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy

[PRISM_A021.ME]    ; WinMe
 AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON_USB.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_A021.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON_USB.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_A021.NT]    ; Win2k and WinXP
 AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON_USB.reg
 CopyFiles      = PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
 BusType        = 15 ; PNP (allows USB)
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_A021.NT.Services]
 AddService= "PRISM_A02", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog

[PRISM_A021.NT.CoInstallers]
 CopyFiles      = PRISM_COINSTALL.copy.NT
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_A021.reg]
 HKR,Ndi,DeviceID,0,"USB\VID_09AA&PID_1000"
; 0x3890 = 14480 0x2280 = 8832
 HKR,,PlatformID,0,14480
 HKR,,UsbVariant,0,8832
 HKR,,VendorDesc,0,%A021_DESC_STR%
 HKR,,FWFileName,0,"PRISMA02.arm"
 
;==========
[PRISM_A022]       ; Win9x
 AddReg         = PRISM_A022.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON_USB20.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy

[PRISM_A022.ME]    ; WinMe
 AddReg         = PRISM_A022.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON_USB20.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_A022.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_A022.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON_USB20.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_A022.NT]    ; Win2k
 AddReg         = PRISM_A022.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON_USB20.reg
 CopyFiles      = PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
 BusType        = 15 ; PNP (allows USB)
 Characteristics= 0x84

[PRISM_A022.NT.Services]
 AddService= "PRISM_A02", 2, PRISM_DRIVER_A03.Service, PRISM_DRIVER.EventLog

[PRISM_A022.NT.CoInstallers]
 CopyFiles      = PRISM_COINSTALL.copy.NT
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_A022.reg]
 HKR,Ndi,DeviceID,0,"USB\VID_0915&PID_2000"
; 0x3890 = 14480 0x3887 = 14471
 HKR,,PlatformID,0,14480
 HKR,,UsbVariant,0,14471
 HKR,,VendorDesc,0,%A022_DESC_STR%
 HKR,,FWFileName,0,"PRISMA02.arm"
 
;################################################################################################## 
 
 
;==========================================
[PRISM_A001]       ; Win9x
 AddReg         = PRISM_A001.reg, COMMON_A00.reg, COMMON_NDIS.reg, COMMON.reg
 DelReg         = COMMON_A00_DEL.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
 DelFiles       = PRISM_FWA00.del

[PRISM_A001.ME]    ; WinMe
 AddReg         = PRISM_A001.reg, COMMON_A00.reg, COMMON_NDIS.reg.ME, COMMON.reg
 DelReg         = COMMON_A00_DEL.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
 DelFiles       = PRISM_FWA00.del.ME

[PRISM_A001.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_A001.reg, COMMON_A00.reg, COMMON_NDIS.reg.ME, COMMON.reg
 DelReg         = COMMON_A00_DEL.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
 DelFiles       = PRISM_FWA00.del.ME

[PRISM_A001.NT]    ; Win2k and XP
 AddReg         = PRISM_A001.reg, COMMON_A00.reg, COMMON_NDIS.reg.NT, COMMON.reg
 DelReg         = COMMON_A00_DEL.reg
 CopyFiles      = PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
 ;DelFiles       = PRISM_FWA00.del.NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_A001.NT.Services]
 AddService     = "PRISM_A00", 2, PRISM_DRIVER_A00.Service, PRISM_DRIVER.EventLog

[PRISM_A001.NT.CoInstallers]
 CopyFiles      = PRISM_COINSTALL.copy.NT
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_A001.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_00001260"
; 0x3890 = 14480
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%A001_DESC_STR%

;==========================================
[PRISM_A002]       ; Win9x
 AddReg         = PRISM_A002.reg, COMMON_A00.reg, COMMON_NDIS.reg, COMMON.reg
 DelReg         = COMMON_A00_DEL.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
 DelFiles       = PRISM_FWA00.del

[PRISM_A002.ME]    ; WinMe
 AddReg         = PRISM_A002.reg, COMMON_A00.reg, COMMON_NDIS.reg.ME, COMMON.reg
 DelReg         = COMMON_A00_DEL.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
 DelFiles       = PRISM_FWA00.del.ME

[PRISM_A002.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_A002.reg, COMMON_A00.reg, COMMON_NDIS.reg.ME, COMMON.reg
 DelReg         = COMMON_A00_DEL.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
 DelFiles       = PRISM_FWA00.del.ME

[PRISM_A002.NT]    ; Win2k
 AddReg         = PRISM_A002.reg, COMMON_A00.reg, COMMON_NDIS.reg.NT, COMMON.reg
 DelReg         = COMMON_A00_DEL.reg
 CopyFiles      = PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
 ;DelFiles       = PRISM_FWA00.del.NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_A002.NT.Services]
 AddService     = "PRISM_A00", 2, PRISM_DRIVER_A00.Service, PRISM_DRIVER.EventLog

[PRISM_A002.NT.CoInstallers]
 CopyFiles      = PRISM_COINSTALL.copy.NT
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_A002.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3886&SUBSYS_00001260"
; 0x3886 = 14470, but same functions as 3890
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%A002_DESC_STR% 
 

;###############################################################################
[PRISM_COINSTALL.reg.NT]
 ;HKR,           ,CoInstallers32         ,0x00010000     ,"PRISMNDI.dll,NdiProc"

[PRISM_DRIVER_A02.Service]
 DisplayName    = %A02_SERVICE_STR%
 Description    = "%HelpText%"
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\PRISMA02.sys
 LoadOrderGroup = NDIS
 
 
[PRISM_DRIVER_A00.Service]
 DisplayName    = %A00_SERVICE_STR%
 Description    = "%HelpText%"
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\PRISMA00.sys
 LoadOrderGroup = NDIS


[PRISM_DRIVER_A03.Service]
 DisplayName    = %A03_SERVICE_STR%
 Description    = "%HelpText%"
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\PRISMA03.sys
 LoadOrderGroup = NDIS 

[PRISM_DRIVER.EventLog]
 AddReg         = PRISM_DRIVER.EventLog.reg

[PRISM_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################
[COMMON_A00.reg]
 HKR,NDI                ,Service                ,0      ,"PRISM_A00"
 HKR,                   ,BusType                    ,0  ,"5"

[COMMON_A00_DEL.reg]
 HKR,                   ,FWFileName

[COMMON_A02_DEL.reg]
 HKR,                   ,FWFileName

[COMMON_A02.reg]
  HKR,NDI                ,Service                ,0      ,"PRISM_A02"
 HKR,NDI                ,CardType               ,0      ,"USB"
 HKR,                   ,BusType                ,0      ,"0"  ; Inconsistency with earlier definition is needed.

[COMMON_NDIS.reg]
; Win9X
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,                   ,DeviceVxDs             ,0      ,"PRISMA00.sys"
 HKR,                   ,DeviceVxDs             ,0      ,"PRISMA02.sys"
 HKR,                   ,DeviceVxDs             ,0      ,"PRISMA03.sys" ;Cohiba
 HKR,NDI                ,NdiInstaller           ,0      ,"PRISMNDI.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,04
 HKR,NDIS               ,MinorNdisVersion       ,1      ,00

[COMMON_NDIS.reg.ME]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,                   ,DeviceVxDs             ,0      ,"PRISMA00.sys"
 HKR,                   ,DeviceVxDs             ,0      ,"PRISMA02.sys"
 HKR,NDI                ,NdiInstaller           ,0      ,"PRISMNDI.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,04
 HKR,NDIS               ,MinorNdisVersion       ,1      ,00

[COMMON_NDIS.reg.NT]
 HKR,Ndi	            ,HelpText				,0		,"%HelpText%"
 HKR,                   ,EnumPropPages32        ,0      ,"PRISMNDI.dll,NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

[COMMON.reg]
 HKR,                   ,SSID                   ,0      ,"ANY"
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts
 HKR,                    ,CardBusBridgeLatencyTimer  ,0  ,"32"
 HKR,                    ,CardBusBridgeCacheLineSize ,0  ,"8"
;Uncomment the above 2 lines to fix misconfigured CardBus bridges, not required for PCI

[COMMON_USB.reg]
 HKR,                   ,SSID                   ,0      ,"ANY"
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,,ConfigProfile,0,256
 HKR,NDI\params\ConfigProfile,default,0,256
 HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
 HKR,NDI\params\ConfigProfile,type,0,"enum"
 HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
 HKR,NDI\params\ConfigProfile,default,0,"256"
 HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
 HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
 HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
 HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
 HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
 HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
 HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
 HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
 HKR,NDI\params\ConfigProfile,optional,0,1

 HKR,,NitroMode,0,"1"
 HKR,NDI\params\NitroMode,default,0,1
 HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
 HKR,NDI\params\NitroMode,type,0,"enum"
 HKR,NDI\params\NitroMode,flag,1,30,00,00,00
 HKR,NDI\params\NitroMode,default,0,"1"
 HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
 HKR,NDI\params\NitroMode\enum,1,,%ON_STR%
 HKR,NDI\params\NitroMode,optional,0,1

 HKR,,PSMode,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,0,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,0,"enum"
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode,default,0,"1"
 HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
 HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
 HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
 HKR,NDI\params\PSMode,optional,0,1

; HKR,,11dMode,0,0  ; Default 11dMode to none.
 
 HKR,NDI\params\PpePdlpEnable,default,0,1
 HKR,NDI\params\PpePdlpEnable,ParamDesc,,%PPE_PDLP%
 HKR,NDI\params\PpePdlpEnable,type,,enum
 HKR,NDI\params\PpePdlpEnable,flag,1,30,00,00,00
 HKR,NDI\params\PpePdlpEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpePdlpEnable\enum,1,,%ON_STR%
 HKR,NDI\params\PpePdlpEnable,optional,0,1

 HKR,NDI\params\PpeCompressEnable,default,0,1
 HKR,NDI\params\PpeCompressEnable,ParamDesc,,%PPE_COMPRESS%
 HKR,NDI\params\PpeCompressEnable,type,,enum
 HKR,NDI\params\PpeCompressEnable,flag,1,30,00,00,00
 HKR,NDI\params\PpeCompressEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpeCompressEnable\enum,1,,%ON_STR%
 HKR,NDI\params\PpeCompressEnable,optional,0,1


 HKR,NDI\params\PpeConcatEnable,default,0,1
 HKR,NDI\params\PpeConcatEnable,ParamDesc,,%PPE_CONCAT%
 HKR,NDI\params\PpeConcatEnable,type,,enum
 HKR,NDI\params\PpeConcatEnable,flag,1,30,00,00,00
 HKR,NDI\params\PpeConcatEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpeConcatEnable\enum,1,,%ON_STR%
 HKR,NDI\params\PpeConcatEnable,optional,0,1

 HKR,NDI\params\PpePiggyBackEnable,default,0,1
 HKR,NDI\params\PpePiggyBackEnable,ParamDesc,,%PPE_PIGGYBACK%
 HKR,NDI\params\PpePiggyBackEnable,type,,enum
 HKR,NDI\params\PpePiggyBackEnable,flag,1,30,00,00,00
 HKR,NDI\params\PpePiggyBackEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpePiggyBackEnable\enum,1,,%ON_STR%
 HKR,NDI\params\PpePiggyBackEnable,optional,0,1

;###############################################################################
[COMMON_USB20.reg]
 HKR,                   ,SSID                   ,0      ,"ANY"
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,,PSMode,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,0,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,0,"enum"
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode,default,0,"1"
 HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
 HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
 HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
 HKR,NDI\params\PSMode,optional,0,1
 
 HKR,,ConfigProfile,0,256
 HKR,NDI\params\ConfigProfile,default,0,256
 HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
 HKR,NDI\params\ConfigProfile,type,0,"enum"
 HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
 HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
 HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
 HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
 HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
 HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
 HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
 HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
 HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
 HKR,NDI\params\ConfigProfile,optional,0,1

 HKR,,NitroMode,0,"1"
 HKR,NDI\params\NitroMode,default,0,1
 HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
 HKR,NDI\params\NitroMode,type,,enum
 HKR,NDI\params\NitroMode,flag,1,30,00,00,00
 HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
 HKR,NDI\params\NitroMode\enum,1,,%ON_STR%
 HKR,NDI\params\NitroMode,optional,0,1
 
 HKR,Ndi\params\RTSThresh,default,0,2347
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2347
 HKR,NDI\params\RTSThresh,step,0,1
 HKR,NDI\params\RTSThresh,optional,0,1

 HKR,Ndi\params\FragThresh,default,0,2346
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2346
 HKR,NDI\params\FragThresh,step,0,2
 HKR,NDI\params\FragThresh,optional,0,1
 
; HKR,,11dMode,0,0  ; Default 11dMode to none.

;###############################################################################






[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 PRISM_DRIVER.copy      = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.ME   = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.NT   = 12 ; Win2k=%windir%\system32\drivers
 PRISM_FWA00.del        = 11 ; Win9x=%windir%\system
 PRISM_FWA00.del.ME     = 11 ; Win9x=%windir%\system
 ;PRISM_FWA00.del.NT     = 12 ; Win2k=%windir%\system32\drivers
 

[PRISM_NDI.copy]
 ;PRISMNDI.dll
 ;PRISMAPI.dll
 ;PRISMSVR.exe

[PRISM_NDI.copy.ME]
 ;PRISMNDI.dll
 ;PRISMAPI.dll
 ;PRISMSVR.exe

[PRISM_COINSTALL.copy.NT]
 ;PRISMNDI.dll           ; Win2k CoInstaller
 ;PRISMAPI.dll
 ;PRISMSVR.exe

[PRISM_DRIVER.copy]
 PRISMA00.sys
 PRISMA02.sys
 PRISMA03.sys            ;Cohiba
 ;PRISMIOC.vxd           ; Win9x Ioctl interface

[PRISM_DRIVER.copy.ME]
 PRISMA00.sys
 PRISMA02.sys
 PRISMA03.sys            ;Cohiba 
 ;PRISMIOC.vxd           ; Win9x Ioctl interface

[PRISM_DRIVER.copy.NT]
 PRISMA00.sys
 PRISMA02.sys
 PRISMA03.sys            ;Cohiba 

[PRISM_APPLET.copy]

[PRISM_APPLET.copy.ME]

[PRISM_APPLET.copy.NT]

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
 PRISMA00.sys           = 1
 PRISMA02.sys           = 1
 ;PRISMIOC.vxd           = 1,win9x
 ;PRISMNDI.dll           = 1,win9x
 ;PRISMAPI.dll           = 1
 ;PRISMSVR.exe           = 1

[SourceDisksFiles.ME]   ; WinMe
 PRISMA00.sys           = 1
 PRISMA02.sys           = 1
 ;PRISMIOC.vxd           = 1,win9x
 ;PRISMNDI.dll           = 1,win9x
 ;PRISMAPI.dll           = 1
 ;PRISMSVR.exe           = 1

[SourceDisksFiles.X86]  ; Win2k/Xp
 PRISMA00.sys           = 1
 PRISMA02.sys           = 1
 PRISMNDI.dll           = 1
 ;PRISMAPI.dll           = 1
 ;PRISMSVR.exe           = 1

;###############################################################################
[Strings]
;String ID               = String Text
;---------                 -----------
 VER_VENDOR_STR          = "IEEE 802.11g"
 VER_VENDOR_NAME_STR     = "IEEE 802.11g"
 INSTALL_DISK_STR        = "IEEE 802.11g Wireless LAN Install Disk"

 A021_DESC_STR           = "IEEE 802.11g USB"
 A022_DESC_STR           = "IEEE 802.11g USB2.0"
 A02_SERVICE_STR         = "IEEE 802.11g USB Driver"
 A03_SERVICE_STR         = "IEEE 802.11g USB2.0 Driver"
 
 A001_DESC_STR           = "IEEE 802.11g Card Bus"
 A002_DESC_STR           = "IEEE 802.11g Card Bus"
 A00_SERVICE_STR         = "IEEE 802.11g Card Bus Driver"
 
 
 HelpText		         = "The IEEE 802.11g Adapter provides wireless local area networking."


 ON_STR                  = "On"
 OFF_STR                 = "Off"
 POWER_SAVE_STR          = "Power Save Mode"
 POWER_SAVE_OFF_STR      = "Disabled"
 POWER_SAVE_DYN_STR      = "Dynamic"
 POWER_SAVE_MAX_STR      = "Maximum"
 CONFIG_PROFILE          = "Configuration Profile"
 CONFIG_PROF_B_ONLY      = "B only"
 CONFIG_PROF_MIXED       = "Mixed"
 CONFIG_PROF_MIXED_LONG  = "Mixed Long"
 CONFIG_PROF_G_ONLY      = "G only"
 CONFIG_PROF_TEST        = "Test"
 CONFIG_PROF_B_WIFI      = "B WiFi"
 CONFIG_PROF_MIXED_SHORT = "Mixed Short"
 CONFIG_PROF_WIFI_SPEC   = "WiFi Spec"
 NITRO_MODE              = "Nitro Mode"
 PPE_PDLP                = "Direct Link"
 PPE_COMPRESS            = "Compression"
 PPE_CONCAT              = "Concatenation"
 PPE_PIGGYBACK           = "PiggyBack"

