;*******************************************************
; AWL300 Copyright 2000 BENQ.
; INF file for the NDIS driver
; Supported OS: Windows XP
; INF version for the 128-bit encryption cards
;*******************************************************

[Version]
Signature  = "$Windows NT$"
Class      = Net
ClassGUID  = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider   = %VENDOR%
;CatalogFile = netvusba.cat
DriverVer = 05/30/2002,1.3.4.124

[Manufacturer]
%VENDOR%   = BENQ

[ControlFlags]
ExcludeFromSelect = VID_04a5&PID_9000
ExcludeFromSelect = VID_03eb&PID_7603


[BENQ]
%USBFVNETA.DeviceDesc% = USBFVNETA.Ndi,USB\VID_04a5&PID_9000
%USBFVNETA.DeviceDesc% = USBFVNETA.Ndi,USB\VID_03eb&PID_7603

;*******************************************************************************
; Win XP main sections
;*******************************************************************************


[USBFVNETA.Ndi.NT]
Characteristics = 0x84  ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 15    ; USB
AddReg          = USBFVNETA.NT.Reg, USBFVNETA.Params
CopyFiles       = CopyFile.NT.Sys
DriverVer = 05/30/2002,1.3.4.124

[USBFVNETA.Ndi.NT.Services]
AddService = USBFVNETA, 2, USBFVNETA.Service, Common.EventLog

;*******************************************************************************
; Driver parameters
;*******************************************************************************

[USBFVNETA.Params]
HKR, Ndi\params\Rate,               ParamDesc,          0, "Rate (Mbps)"
HKR, Ndi\params\Rate,               default,            0, "3"
HKR, Ndi\params\Rate,               type,               0, "enum"
HKR, Ndi\params\Rate\enum,          0,                  0, "1"
HKR, Ndi\params\Rate\enum,          1,                  0, "2"
HKR, Ndi\params\Rate\enum,          2,                  0, "5.5"
HKR, Ndi\params\Rate\enum,          3,                  0, "11"
HKR, Ndi\params\Rate\enum,          4,                  0, "Auto"
HKR, ,                              Rate,               0, "3"

HKR, Ndi\params\RTS_Threshold,      ParamDesc,          0, "RTS Threshold"
HKR, Ndi\params\RTS_Threshold,      default,            0, "2347"
HKR, Ndi\params\RTS_Threshold,      type,               0, "int"
HKR, Ndi\params\RTS_Threshold,      min,                0, "0"
HKR, Ndi\params\RTS_Threshold,      max,                0, "2347"
HKR, Ndi\params\RTS_Threshold,      step,               0, "1"
HKR, ,                              RTS_Threshold,      0, "2347"

HKR, Ndi\params\Frag_Threshold,     ParamDesc,          0, "Fragmentation Threshold"
HKR, Ndi\params\Frag_Threshold,     default,            0, "2346"
HKR, Ndi\params\Frag_Threshold,     type,               0, "int"
HKR, Ndi\params\Frag_Threshold,     min,                0, "256"
HKR, Ndi\params\Frag_Threshold,     max,                0, "2346"
HKR, Ndi\params\Frag_Threshold,     step,               0, "1"
HKR, ,                              Frag_Threshold,     0, "2346"

HKR, Ndi\params\PreambleType,       ParamDesc,          0, "Preamble Type"
HKR, Ndi\params\PreambleType,       default,            0, "0"
HKR, Ndi\params\PreambleType,       type,               0, "enum"
HKR, Ndi\params\PreambleType\enum,  0,                  0, "Long"
HKR, Ndi\params\PreambleType\enum,  1,                  0, "Short"
HKR, Ndi\params\PreambleType\enum,  2,                  0, "Auto"
HKR, ,                              PreambleType,       0, "2"


;*******************************************************************************
; Install section for Windows XP
;*******************************************************************************

[USBFVNETA.NT.Reg]
; Interfaces
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi,            Service,    0, "USBFVNETA"

[USBFVNETA.Service]
DisplayName    = %USBFVNETA.DisplayName%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\vnetusba.sys
LoadOrderGroup = NDIS


[Common.EventLog]
AddReg = Common.AddEventLog.Reg

[Common.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll, %%SystemRoot%%\System32\drivers\vnetusba.sys
HKR, , TypesSupported  , 0x00010001, 7


[CopyFile.NT.Sys]
vnetusba.sys,,,2

;*******************************************************************************
; Destination directories
;*******************************************************************************

[DestinationDirs]
DefaultDestDir   = 12 ; Drivers directory
CopyFile.NT.Sys  = 12


[SourceDisksNames]
50=%DriverDisketteName%,,

[SourceDisksFiles]
vnetusba.sys=50,.,vnetusba.sys,10000

;*******************************************************************************
; Localizable strings
;*******************************************************************************

[Strings]
VENDOR = "BENQ"
USBFVNETA.DeviceDesc = "BENQ AWL300 Wireless LAN USB Adapter"
USBFVNETA.DisplayName = "BENQ AWL300 Wireless LAN USB Adapter"
DriverDisketteName      = "BENQ AWL300 Wireless LAN USB Adapter Drivers Disk"
Help_Text = "BENQ Wireless LAN lets you set up easily and operate a Wireless LAN compliant with 802.11 Standard. It operates in the license free 2.4 GHz ISM band and achieves a peak data rate of 11 Mbs."
