;****************************************************************************************
;
;    FILE:
;            Rt2500.inf
;
;    DESCRIPTION:
;            Linksys Wireless-G PCI Adapter
;            Copyright (C) 2005, Cisco System, Inc. All rights reserved.
;
;*******************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %VENDOR%
Compatible      = 1
DriverVer       = 04/21/2005, 3.00.03.0000
CatalogFile     = RT2500.CAT            

[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%MANUFACTURE%        = WMP54Gv4,   NT.5.1

[WMP54Gv4]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%PRODUCT_NAME%         = WMP54Gv4.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_00321737

[WMP54Gv4.NT.5.1]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%PRODUCT_NAME%         = WMP54Gv4_XP.ndi,        PCI\VEN_1814&DEV_0201&SUBSYS_00321737



;*******************************************************************************************
; Windows 9X specific entries
;*******************************************************************************************

[WMP54Gv4.ndi]
AddReg                  = Common.reg, WMP54Gv4.ndi.reg
CopyFiles               = win9x.CopyFiles

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[WMP54Gv4.ndi.NT]
AddReg                  = Common.reg, WMP54Gv4.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

; NT services sections
[WMP54Gv4.ndi.NT.Services]
AddService              = RT2500, 2, WMP54Gv4.Service, common.EventLog

;*******************************************************************************************
; Windows XP specific entries
;*******************************************************************************************
[WMP54Gv4_XP.ndi.NT]
AddReg                  = Common.reg, WMP54Gv4.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = XP.CopyFiles

; XP services sections
[WMP54Gv4_XP.ndi.NT.Services]
AddService              = RT2500, 2, WMP54Gv4.Service, common.EventLog

;*******************************************************************************************
; common regs for NT and W9x
;*******************************************************************************************

[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                    CurProfile,      0,""
HKR, Default,             CurProfile,      0,""

; add for User Interface
HKR, ,                           TxBurst,            0, "0"
HKR, NDI\params\TxBurst,         ParamDesc,          0, "TxBurst"
HKR, NDI\params\TxBurst,         type,               0, "enum"
HKR, NDI\params\TxBurst,         default,            0, "0"
HKR, NDI\params\TxBurst\enum,    0,                  0, "TxBurst Disable"
HKR, NDI\params\TxBurst\enum,    1,                  0, "TxBurst Enable"

HKR, ,                           TxPower,            0, "0"
HKR, NDI\params\TxPower,         ParamDesc,          0, "TxPower"
HKR, NDI\params\TxPower,         type,               0, "enum"
HKR, NDI\params\TxPower,         default,            0, "0"
HKR, NDI\params\TxPower\enum,    0,                  0, "Auto"
HKR, NDI\params\TxPower\enum,    1,                  0, "100%"
HKR, NDI\params\TxPower\enum,    2,                  0, "75%"
HKR, NDI\params\TxPower\enum,    3,                  0, "50%"
HKR, NDI\params\TxPower\enum,    4,                  0, "25%"
HKR, NDI\params\TxPower\enum,    5,                  0, "10%"
HKR, NDI\params\TxPower\enum,    6,                  0, "6%"


;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, "Radio On/Off"
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, "Disable"
HKR, NDI\params\Radio\enum,       0,               0, "Enable"

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,      0, "1"
HKR, NDI\params\AutoReconnect,          ParamDesc,          0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect,          type,               0, "enum"
HKR, NDI\params\AutoReconnect,          default,            0, "1"
HKR, NDI\params\AutoReconnect\enum,     0,                  0, "Disable"
HKR, NDI\params\AutoReconnect\enum,     1,                  0, "Enable"

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                                  ShowHiddenSSID,     0, "0"   ; 0=disable(default), 1=enable

;
; Country Region 
;
HKR, ,                                  CountryRegion,      0, "0"
;HKR, NDI\params\CountryRegion,         ParamDesc,          0, "Country Region"
;HKR, NDI\params\CountryRegion,         type,               0, "enum"
;HKR, NDI\params\CountryRegion,         default,            0, "0"
;HKR, NDI\params\CountryRegion\enum,    0,                  0, "FCC (Channel 1 - 11)"
;HKR, NDI\params\CountryRegion\enum,    1,                  0, "IC (Channel 1 - 11)"
;HKR, NDI\params\CountryRegion\enum,    2,                  0, "ETSI (Channel 1 - 13)"
;HKR, NDI\params\CountryRegion\enum,    3,                  0, "Spain (Channel 10 - 11)"
;HKR, NDI\params\CountryRegion\enum,    4,                  0, "France (Channel 10 - 13)"
;HKR, NDI\params\CountryRegion\enum,    5,                  0, "MKK (Channel 14)"
;HKR, NDI\params\CountryRegion\enum,    6,                  0, "MKK1 (Channel 1 - 14)"
;HKR, NDI\params\CountryRegion\enum,    7,                  0, "Israel (Channel 3 - 9)"

;*******************************************************************************************
; Advance Page

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "0"


;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "0"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "0"

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"

;
; CCX2 control
;
HKR, ,                            CCX2Control,     0x00010001, 0x00fa4600

;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%

;*******************************************************************************************
; Profile

;
; SSID
;
HKR, ,                            SSID,            0, %SSID_DEF_STR%
HKR, Default,                     SSID,            0, %SSID_DEF_STR%
HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
HKR, NDI\params\SSID,             type,            0, "edit"
HKR, NDI\params\SSID,             limitText,       0, "32"
HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType,      ParamDesc,       0, "Network Type"
HKR, NDI\params\NetworkType,      type,            0, "enum"
HKR, NDI\params\NetworkType,      default,         0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0,               0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1,               0, "Infrastructure"

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, "Power Saving Mode"
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum,      1,               0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum,      2,               0, "Fast_PSP (Power Save Mode)"

;
; CAM when AC Power
;
HKR, ,                            ACPowerCam,      0, "0"
HKR, Default,                     ACPowerCam,      0, "0"
HKR, NDI\params\ACPowerCam,       ParamDesc,       0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam,       type,            0, "enum"
HKR, NDI\params\ACPowerCam,       default,         0, "0"
HKR, NDI\params\ACPowerCam\enum,  0,               0, "Disable"
HKR, NDI\params\ACPowerCam\enum,  1,               0, "Enable"

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"
HKR, NDI\params\RTSThresh,        ParamDesc,       0, "RTS Threshold"
HKR, NDI\params\RTSThresh,        type,            0, "int"
HKR, Ndi\params\RTSThresh,        default,         0, "2347"
HKR, NDI\params\RTSThresh,        min,             0, "0"
HKR, NDI\params\RTSThresh,        max,             0, "2347"
HKR, NDI\params\RTSThresh,        step,            0, "32"
HKR, NDI\params\RTSThresh,        optional,        0, "0"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"
HKR, NDI\params\FragThresh,       ParamDesc,       0, "Fragment Threshold"
HKR, NDI\params\FragThresh,       type,            0, "int"
HKR, Ndi\params\FragThresh,       default,         0, "2346"
HKR, NDI\params\FragThresh,       min,             0, "256"
HKR, NDI\params\FragThresh,       max,             0, "2346"
HKR, NDI\params\FragThresh,       step,            0, "32"
HKR, NDI\params\FragThresh,       optional,        0, "0"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                AuthenType,      0, "0" ; Open System
HKR, Default,         AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                Encryption,      0, "1" ; Disable
HKR, Default,         Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                WEPKeyLen,       0, "0"
HKR, Default,         WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                WEPKeyUse,       0,"1"
HKR, Default,         WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                WEPKey1,         0,""
HKR, Default,         WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                WEPKey2,         0,""
HKR, Default,         WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                WEPKey3,         0,""
HKR, Default,         WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                WEPKey4,         0,""
HKR, Default,         WEPKey4,         0,""


;*******************************************************************************************
; APConfig use
;

;
; WPA Group-Key ReKey Interval
;
HKR, ,                RekeyInterval,   0, "60"

;
; WPA Group-Key ReKey Method
;
HKR, ,                RekeyMethod,     0, "0"


[WMP54Gv4.ndi.reg]
HKR, ,                            NTMPDriver,       0, RT25009x.sys
HKR, Ndi,                         DeviceID,         0, "PCI\VEN_1814&DEV_0201"

HKR, ,                            BusType,          0, 5
HKR, NDI,                         CardType,         0, "PCI"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "RT25009x.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "RT25009X"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
XP.CopyFiles            = 12    ; system32\drivers subdirectory on Windows XP
win9x.CopyFiles         = 11    ; system32 subdirectory on win9x

[NT.CopyFiles]
RT2500.sys                      ; NT Installation

[XP.CopyFiles]
RT2500.sys                      ; XP Installation

[win9x.CopyFiles]
RT25009x.sys                    ; Win9x Installation

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
RT2500.sys              = 1
RT25009x.sys            = 1


;*******************************************************************************************
; NT specific
;*******************************************************************************************
[WMP54Gv4.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "RT2500"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[WMP54Gv4.Service]
DisplayName                 = %WMP54Gv4.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\RT2500.sys"
HKR, , TypesSupported,   0x00010001, 7



;*******************************************************************************************
; Strings
;*******************************************************************************************
[Strings]
VENDOR                      = "Linksys"
MANUFACTURE                 = "Linksys, A Division of Cisco Systems, Inc."
PRODUCT_NAME                = "Linksys Wireless-G PCI Adapter"
INSTALL_DISK_STR            = "Linksys Wireless-G PCI Adapter Installation Disk"
WMP54Gv4.Service.DispName   = "Linksys Wireless-G PCI Adapter Driver"
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR	    = "Linksys Wireless-G PCI Adapter"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"

