;===========================================================================
; 
; Windows XP NDIS driver INF for D-Link AirPlus XtremeG Wireless Adapter
; Copyright (C) 2003 D-Link, Inc.
;
;=========================================================================== 
 
 
[Version] 
Signature = "$Windows NT$" 
Compatible  = 1
Class=Net
ClassGUID={4D36E972-E325-11CE-BFC1-08002BE10318} 
Provider=%MRVL% 
CatalogFile=mrv8knet.cat
DriverVer=1/09/2004,2.3.0.1

;===========================================================================
; Source Media Information Sections
;===========================================================================
[SourceDisksNames]
1 = "Marvell installation disk 1",,,

[SourceDisksFiles]
; On Marvell installation disk 1 
mrv8k51.sys =1 

[DestinationDirs]
W8100PCI.XP.CopyFiles  = 12 
DefaultDestDirs        = 11

[Manufacturer] 
%MRVL%=DLINK

[DLINK]
%W8100PCIXPCB.DeviceDesc1% = W8100PCIXP.ndi, PCI\VEN_11AB&DEV_1FA6


;===========================================================================
; ControlFlags section
;===========================================================================
; pnp cards should be excluded from select
[ControlFlags]
ExcludeFromSelect = *

;***************************************************************************
;**         
;**          Win XP DDInstall section
;**          
;***************************************************************************
;***************************************************************************
[W8100PCIXP.ndi]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI or CardBus
BusType         = 5 
AddReg          = W8100PCI.reg, W8100PCIXP.reg, W8100PCI.zerocfg
CopyFiles       = W8100PCI.XP.CopyFiles


;===========================================================================
; W8100 PCI WinXP registers
;===========================================================================
[W8100PCIXP.reg]
HKR, Ndi,            Service,    0, "W8100PCI"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"


[W8100PCI.XP.CopyFiles]
mrv8k51.sys,,,2 

[W8100PCIXP.ndi.Services]
AddService = W8100PCI, 2, W8100PCIXP.Service, CommonXP.EventLog

[W8100PCIXP.Service]
DisplayName    = %W8100PCIXP.Service.DispName%
ServiceType    = 1 ;%SERVICE_KERNEL_DRIVER%
StartType      = 3 ;%SERVICE_DEMAND_START%
ErrorControl   = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\mrv8k51.sys
LoadOrderGroup = NDIS

[CommonXP.EventLog]
AddReg = CommonXP.AddEventLog.reg

[CommonXP.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7



;===========================================================================
; W8100 PCI common, MIB can be defined here
;===========================================================================
[W8100PCI.reg]

HKR, Ndi\xparams\DesiredSSID,ParamDesc,,"%SSID%"
HKR, Ndi\xparams\DesiredSSID,default,,"default"
HKR, Ndi\xparams\DesiredSSID,type,,"edit" 
HKR, Ndi\xparams\DesiredSSID,LimitText,,"32"
HKR, Ndi\xparams\DesiredSSID,UpperCase,,"0" 
HKR, Ndi\xparams\DesiredSSID,Optional,,"1" 

HKR, Ndi\xparams\AuthMode,ParamDesc,,"%AuthMode%"
HKR, Ndi\xparams\AuthMode,default,,"0"
HKR, Ndi\xparams\AuthMode,type,,enum
HKR, Ndi\xparams\AuthMode\enum,"0",,"Open"
HKR, Ndi\xparams\AuthMode\enum,"1",,"Shared"

HKR, Ndi\xparams\NetworkMode,ParamDesc,,"%NetworkMode%"
HKR, Ndi\xparams\NetworkMode,default,,"1"
HKR, Ndi\xparams\NetworkMode,type,,enum
HKR, Ndi\xparams\NetworkMode\enum,"0",,"Ad Hoc"
HKR, Ndi\xparams\NetworkMode\enum,"1",,"Infrastructure"

;HKR, Ndi\xparams\Wireless,ParamDesc,,"%WirelessM%"
;HKR, Ndi\xparams\Wireless,default,,"0"
;HKR, Ndi\xparams\Wireless,type,,enum
;HKR, Ndi\xparams\Wireless\enum,"0",,"Auto"
;HKR, Ndi\xparams\Wireless\enum,"1",,"B rates only"
 
HKR, Ndi\xparams\FragThsd,  ParamDesc,0 , "%FragThsds%"
HKR, Ndi\xparams\FragThsd,  default, 0 , "2346"
HKR, Ndi\xparams\FragThsd,  min, 0 , "256"
HKR, Ndi\xparams\FragThsd,  max, 0 , "2346"
HKR, Ndi\xparams\FragThsd,  step, 0 , "1"
HKR, Ndi\xparams\FragThsd,  Base, 0 , "10"
HKR, Ndi\xparams\FragThsd,  type, 0 ,"dword"

HKR, Ndi\xparams\Channel,  ParamDesc,0 , "%Channel%"
HKR, Ndi\xparams\Channel,  default, 0 , "6"
HKR, Ndi\xparams\Channel,  min, 0 , "0"
HKR, Ndi\xparams\Channel,  max, 0 , "14"
HKR, Ndi\xparams\Channel,  step, 0 , "1"
HKR, Ndi\xparams\Channel,  Base, 0 , "16"
HKR, Ndi\xparams\Channel,  type, 0 ,"dword"

HKR, Ndi\xparams\TxAntenna,  ParamDesc,0 , "%TxAntennaStr%"
HKR, Ndi\xparams\TxAntenna,  default, 0 , "2"
HKR, Ndi\xparams\TxAntenna,  min, 0 , "1"
HKR, Ndi\xparams\TxAntenna,  max, 0 , "ffff"
HKR, Ndi\xparams\TxAntenna,  step, 0 , "1"
HKR, Ndi\xparams\TxAntenna,  Base, 0 , "16"
HKR, Ndi\xparams\TxAntenna,  type, 0 ,"dword"

HKR, Ndi\xparams\RxAntenna,  ParamDesc,0 , "%RxAntennaStr%"
HKR, Ndi\xparams\RxAntenna,  default, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna,  min, 0 , "1"
HKR, Ndi\xparams\RxAntenna,  max, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna,  step, 0 , "1"
HKR, Ndi\xparams\RxAntenna,  Base, 0 , "16"
HKR, Ndi\xparams\RxAntenna,  type, 0 ,"dword"

HKR, Ndi\xparams\RTSThsd,  ParamDesc, 0, "%RTSThsds%"
HKR, Ndi\xparams\RTSThsd,  default, 0, "2346"
HKR, Ndi\xparams\RTSThsd,  min, 0, "0"
HKR, Ndi\xparams\RTSThsd,  max, 0, "2346"
HKR, Ndi\xparams\RTSThsd,  step, 0, "1"
HKR, Ndi\xparams\RTSThsd,  Base, 0, "10"
HKR, Ndi\xparams\RTSThsd,  type, 0, "dword"

;HKR, Ndi\xparams\PowerMode,ParamDesc,,"%PowerMode%"
;HKR, Ndi\xparams\PowerMode,default,,"0"
;HKR, Ndi\xparams\PowerMode,type,,enum
;HKR, Ndi\xparams\PowerMode\enum,"0",,"CAM-Constantly Awake Mode"
;HKR, Ndi\xparams\PowerMode\enum,"1",,"MaxPSP-Max Power Savings"
;HKR, Ndi\xparams\PowerMode\enum,"2",,"FastPSP-Fast Power Savings"

HKR, Ndi\xparams\DataRate,ParamDesc,,"%DataRate%"
HKR, Ndi\xparams\DataRate,default,,"FF"
HKR, Ndi\xparams\DataRate,type,,enum
HKR, Ndi\xparams\DataRate\enum,"FF",,"Auto"
HKR, Ndi\xparams\DataRate\enum,"2",,"1 Mbps"
HKR, Ndi\xparams\DataRate\enum,"4",,"2 Mbps"
HKR, Ndi\xparams\DataRate\enum,"b",,"5.5 Mbps"
HKR, Ndi\xparams\DataRate\enum,"16",,"11 Mbps"
;HKR, Ndi\xparams\DataRate\enum,"2C",,"22 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"C",,"6 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"12",,"9 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"18",,"12 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"24",,"18 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"30",,"24 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"48",,"36 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"60",,"48 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"6C",,"54 Mbps"

HKR, Ndi\xparams\WepStatus,ParamDesc,,"%WepStatus%"
HKR, Ndi\xparams\WepStatus,default,,"1"
HKR, Ndi\xparams\WepStatus,type,,enum
HKR, Ndi\xparams\WepStatus\enum,"0",,"Enabled"
HKR, Ndi\xparams\WepStatus\enum,"1",,"Disabled"


HKR, Ndi\xparams\Preamble,ParamDesc,,"%PreambleStr%"
HKR, Ndi\xparams\Preamble,default,,"3"
HKR, Ndi\xparams\Preamble,type,,enum 
HKR, Ndi\xparams\Preamble\enum,"1",,"Auto"
HKR, Ndi\xparams\Preamble\enum,"2",,"Short Preamble" 
HKR, Ndi\xparams\Preamble\enum,"3",,"Long Preamble"

HKR,, TxWepKey, 2, "" 
HKR,, WepKey1, 2, "" 
HKR,, WepKey2, 2, "" 
HKR,, WepKey3, 2, "" 
HKR,, WepKey4, 2, "" 


;Special for Driver on WinXP OS.
;[W8100PCI.zerocfg]
 
;===========================================================================
; Strings section
;===========================================================================
[Strings]
MRVL = "D-Link"

TxAntennaStr = "Tx Antenna Select"
RxAntennaStr = "Rx Antenna Select" 
Channel = "Channel"
FragThsds = "Fragamentation Threshold"
DataRate = "Data Rate"
RTSThsds = "RTS Threshold"
AuthMode = "Authentication Mode"
;WirelessM = "Wireless Mode"
NetworkMode = "Operation Mode"
WepStatus = "WEP Status"
SSID = "SSID"
PreambleStr = "Preamble Select"
;PowerMode = "Power Save Mode"

W8100PCIXPCB.DeviceDesc1     = "D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter"
W8100PCIXPCB.DeviceDesc2     = "D-Link AirPlus G DWL-G510 Wireless PCI Card"
W8100PCIXP.Service.DispName  = "D-Link AirPlus G Wireless Driver"








 

