;***********************************************************************
; bnkUSB.inf
;
;
;   This installation script supports Windows 2000,XP  for the
;   Belkin 54Mbps Wireless USB Network Adapter.
;
;   
;***********************************************************************

[Version]
 DriverVer = 11/11/2003, 1.00.5.0
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%


[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = *

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]
 %A021_DESC_STR%     = USB20,        USB\VID_050d&PID_7050
 %A021_DESC_STR%     = USB20,        USB\VID_09aa&PID_1000
  
;==========
[USB20]       ; Win9x
 AddReg         = USB20.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = USB_DRIVER


[USB20.NT]    ; Win2k
 AddReg         = USB20.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = USB_DRIVER.NT
 BusType        = 15
 Characteristics= 0x84

[USB20.NT.Services]
 AddService= PRISM_A02, 2, USB_DRIVER_A02.Service, USB_DRIVER.EventLog

[USB20.NT.CoInstallers]
 CopyFiles      = USB_COINSTALL.copy.NT
 AddReg         = USB20.reg.NT
 
[USB20.reg.NT]
; HKR,           ,CoInstallers32         ,0x00010000     ,"PRISMNDI.dll,NdiProc"

[USB20.reg]
 HKR,Ndi,DeviceID,0,"USB\VID_09aa&PID_1000"
; 0x3890 = 14480
 HKR,,PlatformID,0,"14480"
 HKR,,VendorDesc,0,%A021_DESC_STR%
 HKR,,FWFileName,0,"PRISMA02.arm"

;###############################################################################

[USB_DRIVER_A02.Service]
 DisplayName    = %A02_SERVICE_STR%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\PRISMAXP.sys
 LoadOrderGroup = NDIS

[USB_DRIVER.EventLog]
 AddReg         = USB_DRIVER.EventLog.reg

[USB_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################

[COMMON_A02.reg]
 HKR,NDI                ,Service                ,0      ,"PRISM_A02"
 HKR,NDI                ,CardType               ,0      ,"USB"
 HKR,                   ,BusType                ,0      ,"0"
 HKR,                   ,DeviceVxDs             ,0      ,"PRISMA9X.sys"


[COMMON_NDIS.reg]
; Win9X
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
; HKR,NDI                ,NdiInstaller           ,0      ,"USBCoI9x.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a


[COMMON_NDIS.reg.NT]
; HKR,                   ,EnumPropPages32        ,0      ,"PRISMNDI.dll,NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

[COMMON.reg]
 HKR,                   ,AntennaDiversity        ,0      ,"0" 
 HKR,                   ,FWFileName             ,0      ,"PRISMA02.arm"
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 
 HKR,NDI\params\RTSThresh,default,0,"2347"
 HKR,Ndi\params\RTSThresh,default,0,"2347"
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,"int"
; HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,"0"
 HKR,NDI\params\RTSThresh,max,0,"2347"
 HKR,NDI\params\RTSThresh,step,0,"1"
 HKR,NDI\params\RTSThresh,optional,0,"1"

 HKR,NDI\params\ShortRetryLimit,default,0,"7"
 HKR,NDI\params\ShortRetryLimit,default,0,"7"
 HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
 HKR,NDI\params\ShortRetryLimit,type,,"int"
 HKR,NDI\params\ShortRetryLimit,min,0,"1"
 HKR,NDI\params\ShortRetryLimit,max,0,"255"
 HKR,NDI\params\ShortRetryLimit,step,0,"1"
 HKR,NDI\params\ShortRetryLimit,optional,0,"1"      

 HKR,NDI\params\LongRetryLimit,default,0,"4"
 HKR,NDI\params\LongRetryLimit,default,0,"4"
 HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
 HKR,NDI\params\LongRetryLimit,type,0,"int"
 HKR,NDI\params\LongRetryLimit,min,0,"1"
 HKR,NDI\params\LongRetryLimit,max,0,"255"
 HKR,NDI\params\LongRetryLimit,step,0,"1"
 HKR,NDI\params\LongRetryLimit,optional,0,"1"

 HKR,NDI\params\ConfigProfile,default,0,"256"
 HKR,NDI\params\ConfigProfile,default,0,"256"
 HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
 HKR,NDI\params\ConfigProfile,type,,"enum"
; HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
 HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
 HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
 HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
 HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
 HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
 HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
 HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
 HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
 HKR,NDI\params\ConfigProfile,optional,0,"1"

 HKR,,NitroMode,0,"1"
 HKR,NDI\params\NitroMode,default,0,"1"
 HKR,NDI\params\NitroMode,default,0,"1"
 HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
 HKR,NDI\params\NitroMode,type,,"enum"
; HKR,NDI\params\NitroMode,flag,1,30,00,00,00
 HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
 HKR,NDI\params\NitroMode\enum,1,,%ON_STR%
 HKR,NDI\params\NitroMode,optional,0,"1"

 HKR,,PSMode,0,"1"
 HKR,NDI\params\PSMode,default,0,"1"
 HKR,Ndi\params\PSMode,default,0,"1"
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,"enum"
; HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
 HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
 HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
 HKR,NDI\params\PSMode,optional,0,"1"

;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 USB_DRIVER      = 11 ; Win9x=%windir%\system
 USB_DRIVER.NT   = 12 ; Win2k=%windir%\system32\drivers

[USB_DRIVER]
; PRISMA9X.sys

[USB_COINSTALL.copy.NT]

[USB_DRIVER.NT]
 PRISMAXP.SYS

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %Disk%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
; PRISMA9X.sys           = 1

[SourceDisksFiles.X86]  ; Win2k/Xp
 PRISMAXP.SYS           = 1

;###############################################################################
[Strings]
;String ID               = String Text
;---------                 -----------
 VER_VENDOR_STR          = "BELKIN"
 VER_VENDOR_NAME_STR     = "BELKIN Inc."
 Disk			 = "Belkin 54Mbps Wireless USB Network Adapter Install Disk"

 A021_DESC_STR           = "Belkin 54Mbps Wireless USB Network Adapter"
 A02_SERVICE_STR         = "Belkin 54Mbps Wireless USB Network Adapter"

 ON_STR                  = "On"
 OFF_STR                 = "Off"
 RTSTHRESH_STR           = "RTS Threshold"
 AUTHENT_TYPE_STR        = "Authentication Algorithm"
 POWER_SAVE_STR          = "Power Save Mode"
 POWER_SAVE_OFF_STR      = "Disabled"
 POWER_SAVE_DYN_STR      = "Dynamic"
 POWER_SAVE_MAX_STR      = "Maximum"
 SHORT_RETRY_STR         = "Short Retry Limit"
 LONG_RETRY_STR          = "Long Retry Limit"
 CONFIG_PROFILE          = "Configuration Profile"
 CONFIG_PROF_B_ONLY      = "B only"
 CONFIG_PROF_MIXED       = "Mixed"
 CONFIG_PROF_MIXED_LONG  = "Mixed Long"
 CONFIG_PROF_G_ONLY      = "G only"
 CONFIG_PROF_TEST        = "Test"
 CONFIG_PROF_B_WIFI      = "B WiFi"
 CONFIG_PROF_MIXED_SHORT = "Mixed Short"
 CONFIG_PROF_WIFI_SPEC   = "WiFi Spec"
 NITRO_MODE              = "Nitro Mode"

