;***********************************************************************
;
; WLANNIC.INF
;
;   This installation script supports Windows 98,Me,2000&XP for the
;   EagleTec WG-2000 CardBus Wireless LAN Adapters.
;
;   Copyright (c) EagleTec (Asia) Ltd, 2003 
;   All Rights Reserved.
;
;***********************************************************************

[Version]
 DriverVer = 09/10/2003, 1.0.17
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
;CatalogFile         = WlanNIC.cat
 MillenniumPreferred = .ME

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = *

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]
 %DCB_DESC_STR%     = WLAN_DCB1,        PCI\VEN_1260&DEV_3890&SUBSYS_00001260
 %DCB_DESC_STR%		= WLAN_DCB2,        PCI\VEN_1260&DEV_3890&SUBSYS_001417CF
 %DCB_DESC_STR%		= WLAN_DCB3,        PCI\VEN_1260&DEV_3890&SUBSYS_001517CF
 %DCB_DESC_STR%		= WLAN_DCB4,        PCI\VEN_1260&DEV_3890&SUBSYS_002017CF 
 
 

;==========================================
[WLAN_DCB1]       ; Win9x
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB1.reg, COMMON_DCB.reg, COMMON_NDIS.reg, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy, WLAN_FWDCB.copy, WLAN_APPLET.copy, WLAN_NDI.copy, WLAN_DOM.copy

[WLAN_DCB1.ME]    ; WinMe
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB1.reg, COMMON_DCB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy.ME, WLAN_FWDCB.copy.ME, WLAN_APPLET.copy.ME, WLAN_NDI.copy.ME, WLAN_DOM.copy

[WLAN_DCB1.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB1.reg, COMMON_DCB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PS_MODE.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy.ME, WLAN_FWDCB.copy.ME, WLAN_APPLET.copy.ME, WLAN_NDI.copy.ME, WLAN_DOM.copy

[WLAN_DCB1.NT]    ; Win2k
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB1.reg, COMMON_DCB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy.NT, WLAN_FWDCB.copy.NT, WLAN_APPLET.copy.NT, WLAN_DOM.copy
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB1.NT.Services]
 AddService     = "WLAN_DCB", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB1.NT.CoInstallers]
 CopyFiles      = WLAN_COINSTALL.copy.NT
 AddReg         = WLAN_COINSTALL.reg.NT

[WLAN_DCB1.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_00001260"
; 0x3890 = 14480
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR%
 HKR,,FWFileName,0,"WLANDCB.arm"
 
;==========================================
[WLAN_DCB2]       ; Win9x
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB2.reg, COMMON_DCB.reg, COMMON_NDIS.reg, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy, WLAN_FWDCB.copy, WLAN_APPLET.copy, WLAN_NDI.copy, WLAN_DOM.copy

[WLAN_DCB2.ME]    ; WinMe
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB2.reg, COMMON_DCB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy.ME, WLAN_FWDCB.copy.ME, WLAN_APPLET.copy.ME, WLAN_NDI.copy.ME, WLAN_DOM.copy

[WLAN_DCB2.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB2.reg, COMMON_DCB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PS_MODE.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy.ME, WLAN_FWDCB.copy.ME, WLAN_APPLET.copy.ME, WLAN_NDI.copy.ME, WLAN_DOM.copy

[WLAN_DCB2.NT]    ; Win2k
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB2.reg, COMMON_DCB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy.NT, WLAN_FWDCB.copy.NT, WLAN_APPLET.copy.NT, WLAN_DOM.copy
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB2.NT.Services]
 AddService     = "WLAN_DCB", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB2.NT.CoInstallers]
 CopyFiles      = WLAN_COINSTALL.copy.NT
 AddReg         = WLAN_COINSTALL.reg.NT

[WLAN_DCB2.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_001417CF"
; 0x3890 = 14480
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR%
 HKR,,FWFileName,0,"WLANDCB.arm"
 
;==========================================
[WLAN_DCB3]       ; Win9x
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB3.reg, COMMON_DCB.reg, COMMON_NDIS.reg, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy, WLAN_FWDCB.copy, WLAN_APPLET.copy, WLAN_NDI.copy, WLAN_DOM.copy

[WLAN_DCB3.ME]    ; WinMe
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB3.reg, COMMON_DCB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy.ME, WLAN_FWDCB.copy.ME, WLAN_APPLET.copy.ME, WLAN_NDI.copy.ME, WLAN_DOM.copy

[WLAN_DCB3.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB3.reg, COMMON_DCB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PS_MODE.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy.ME, WLAN_FWDCB.copy.ME, WLAN_APPLET.copy.ME, WLAN_NDI.copy.ME, WLAN_DOM.copy

[WLAN_DCB3.NT]    ; Win2k
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB3.reg, COMMON_DCB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy.NT, WLAN_FWDCB.copy.NT, WLAN_APPLET.copy.NT, WLAN_DOM.copy
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB3.NT.Services]
 AddService     = "WLAN_DCB", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB3.NT.CoInstallers]
 CopyFiles      = WLAN_COINSTALL.copy.NT
 AddReg         = WLAN_COINSTALL.reg.NT

[WLAN_DCB3.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_001517CF"
; 0x3890 = 14480
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR%
 HKR,,FWFileName,0,"WLANDCB.arm"   
 
 
;==========================================
[WLAN_DCB4]       ; Win9x
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB4.reg, COMMON_DCB.reg, COMMON_NDIS.reg, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy, WLAN_FWDCB.copy, WLAN_APPLET.copy, WLAN_NDI.copy, WLAN_DOM.copy

[WLAN_DCB4.ME]    ; WinMe
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB4.reg, COMMON_DCB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy.ME, WLAN_FWDCB.copy.ME, WLAN_APPLET.copy.ME, WLAN_NDI.copy.ME, WLAN_DOM.copy

[WLAN_DCB4.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB4.reg, COMMON_DCB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PS_MODE.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy.ME, WLAN_FWDCB.copy.ME, WLAN_APPLET.copy.ME, WLAN_NDI.copy.ME, WLAN_DOM.copy

[WLAN_DCB4.NT]    ; Win2k
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = WLAN_DCB4.reg, COMMON_DCB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
 CopyFiles      = WLAN_DRIVER.copy.NT, WLAN_FWDCB.copy.NT, WLAN_APPLET.copy.NT, WLAN_DOM.copy
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB4.NT.Services]
 AddService     = "WLAN_DCB", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB4.NT.CoInstallers]
 CopyFiles      = WLAN_COINSTALL.copy.NT
 AddReg         = WLAN_COINSTALL.reg.NT

[WLAN_DCB4.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_002017CF"
; 0x3890 = 14480
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR%
 HKR,,FWFileName,0,"WLANDCB.arm" 
;###############################################################################

[WLAN_COINSTALL.reg.NT]
 
[WLAN_DRIVER_DCB.Service]
 DisplayName    = %WLAN_SERVICE_DISPLAY_DCB%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\WLANDCB.sys
 LoadOrderGroup = NDIS
 
[WLAN_DRIVER.EventLog]
 AddReg         = WLAN_DRIVER.EventLog.reg

[WLAN_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################

[COMMON_DCB.reg]
 HKR,NDI                ,Service                ,0      ,"WLAN_DCB"
 HKR,                   ,BusType                ,0      ,"5"
 HKR,                   ,DeviceVxDs             ,0      ,"WLANDCB.sys"
 HKR,                   ,EnableIRQSharing       ,1      ,01,00,00,00
 HKR,                   ,IOBaseAddress          ,1      ,02,00,00,00
 HKR,                   ,InterruptNumber        ,1      ,04,00,00,00

[COMMON_NDIS.reg]
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"WLAN"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.ME]
;HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
;HKR,NDI                ,NdiInstaller           ,0      ,"PRISMCFG.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"WLAN"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.NT]
; HKR,                   ,EnumPropPages32        ,0      ,"PRISMCFG.cpl,NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

[COMMON.reg]
;HKR,                   ,PRISMIOC				,0      ,"1"
 HKR,                   ,WLANIOC				,0      ,"XG-300"
;Always specify Band 2.4GHz
 HKR,                   ,Band				    ,0      ,"1"
;Specify RegulatorDomain, used by utility
;Domain	HexCode	KeyValue	Channel	Description
;======	======= ========	=======	===========
;FCC	0x10	"16"		1-11	USA
;DOC	0x20	"32"		1-11	Canada
;ETSI	0x30	"48"		1-13	most of Europe
;Spain	0x31	"49"		10-11
;France	0x32	"50"		10-13
;MKK	0x40	"64"		1-14	Japan
;ARIB	0x41	"65"		1-14	(Default)
;======	=======	========	=======	============
 HKR,                   ,RegulatorDomain		,0      ,"48"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,         ,RTSThresh,0,2347
 HKR, defaults,RTSThresh,0,2347
 HKR,NDI\params\RTSThresh,,0,2347
 HKR,Ndi\params\RTSThresh,default,0,2347
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2347
 HKR,NDI\params\RTSThresh,step,0,1
 HKR,NDI\params\RTSThresh,optional,0,1

 HKR,         ,FragThresh,0,2346
 HKR,defaults,FragThresh,0,2346
 HKR,NDI\params\FragThresh,,0,2346
 HKR,Ndi\params\FragThresh,default,0,2346
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2346
 HKR,NDI\params\FragThresh,step,0,2
 HKR,NDI\params\FragThresh,optional,0,1
 
;;SSID 
 HKR,         ,SSID,0,"ANY"
 HKR, defaults,SSID,0,"ANY" ;Default value is "any"
 HKR, NDI\params\SSID,,0,"ANY"       
 HKR, Ndi\params\SSID,default,	0, "ANY"
 HKR, Ndi\params\SSID,ParamDesc,0, %ESSID_Str%
 HKR, Ndi\params\SSID,type,0, "edit"
 HKR, Ndi\params\SSID,default,0, "ANY"
 HKR, Ndi\params\SSID,LimitText,0, "32"
 HKR, Ndi\params\SSID,UpperCase,0, "0"
 HKR, NDI\params\SSID,optional,0,1

;NetworkType
 HKR,         ,NetworkType,0,1
 HKR, defaults,NetworkType,0,1   ;Infrasturcture
 HKR, NDI\params\NetworkType,,0,1
 HKR, Ndi\params\NetworkType,default,0,1 
 HKR, Ndi\params\NetworkType,ParamDesc,0, %NET_WORK_TYPE%
 HKR, Ndi\params\NetworkType,type,0, "enum"
 HKR, Ndi\params\NetworkType,default,0, "1"
 HKR, Ndi\params\NetworkType\enum,1,0, "Infrastructure"
 HKR, Ndi\params\NetworkType\enum,0,0, "802.11 AdHoc"
 HKR, NDI\params\NetworkType,optional,0,1

 HKR,         ,LongPreamble,0,0
 HKR, defaults,LongPreamble,0,0   ;Infrasturcture
 HKR, NDI\params\LongPreamble,,0,0
 HKR, Ndi\params\LongPreamble,default,0,0 
 HKR, Ndi\params\LongPreamble,ParamDesc,0, %SHORT_PREAM_STR%
 HKR, Ndi\params\LongPreamble,type,0, "enum"
 HKR, Ndi\params\LongPreamble,default,0, "1"
 HKR, Ndi\params\LongPreamble\enum,1,0, "Long"
 HKR, Ndi\params\LongPreamble\enum,0,0, "Short"
 HKR, NDI\params\LongPreamble,optional,0,1  
 
;11d Mode.
 HKR,         ,11dMode,0,0
 HKR, defaults,11dMode,0,0   ;Disalbed
 HKR, NDI\params\11dMode,,0,0
 HKR, Ndi\params\11dMode,default,0,0 
 HKR, Ndi\params\11dMode,ParamDesc,0, %11D_MODE%
 HKR, Ndi\params\11dMode,type,0, "enum"
 HKR, Ndi\params\11dMode,default,0, "0"
 HKR, Ndi\params\11dMode\enum,0,0, "Disabled"
 HKR, Ndi\params\11dMode\enum,1,0, "Strict"
 HKR, Ndi\params\11dMode\enum,2,0, "Flexible"
 HKR, NDI\params\11dMode,optional,0,1
 
 ;Nitro Mode
 HKR,		,NitroMode,0,1
 HKR,defaults,NitroMode,0,1
 HKR,NDI\params\NitroMode,,0,1
 HKR,NDI\params\NitroMode,default,0,1
 HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
 HKR,NDI\params\NitroMode,type,0,int
 HKR,NDI\params\NitroMode,min,0,0
 HKR,NDI\params\NitroMode,max,0,1
 HKR,NDI\params\NitroMode,step,0,1
 HKR,NDI\params\NitroMode,optional,0,1
 
 ;NitroTime
 
 HKR,		,NitroTime,0,650
 HKR,defaults,NitroTime,0,650
 HKR,NDI\params\NitroTime,,0,650
 HKR,NDI\params\NitroTime,default,0,650
 HKR,NDI\params\NitroTime,ParamDesc,,"NitroTime"
 HKR,NDI\params\NitroTime,type,0,int
 HKR,NDI\params\NitroTime,min,0,0
 HKR,NDI\params\NitroTime,max,0,5000
 HKR,NDI\params\NitroTime,step,0,10
 HKR,NDI\params\NitroTime,optional,0,1


[COMMON_AMAC_DEL.reg]
 HKR,defaults,DataRates
 HKR,NDI\params\DataRates
 HKR,NDI\params\DataRate
 HKR,DSChannel
 HKR,defaults,DSChannel
 HKR,NDI\params\DSChannel

[COMMON_AMAC.reg]
 
 HKR,		,ShortRetryLimit,0,7
 HKR,defaults,ShortRetryLimit,0,7
 HKR,NDI\params\ShortRetryLimit,,0,7
 HKR,NDI\params\ShortRetryLimit,default,0,7
 HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
 HKR,NDI\params\ShortRetryLimit,type,,int
 HKR,NDI\params\ShortRetryLimit,min,0,1
 HKR,NDI\params\ShortRetryLimit,max,0,255
 HKR,NDI\params\ShortRetryLimit,step,0,1
 HKR,NDI\params\ShortRetryLimit,optional,0,1


 HKR,		,LongRetryLimit,0,4
 HKR,defaults,LongRetryLimit,0,4
 HKR,NDI\params\LongRetryLimit,,0,4
 HKR,NDI\params\LongRetryLimit,default,0,4
 HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
 HKR,NDI\params\LongRetryLimit,type,0,int
 HKR,NDI\params\LongRetryLimit,min,0,1
 HKR,NDI\params\LongRetryLimit,max,0,255
 HKR,NDI\params\LongRetryLimit,step,0,1
 HKR,NDI\params\LongRetryLimit,optional,0,1

[COMMON_PSMODE.reg]
 HKR,		,PSMode,0,1
 HKR,		defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
 HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
 HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
 HKR,NDI\params\PSMode,optional,0,1

[COMMON_PS_MODE_XP.reg]

 HKR,,PSMode,0,1
 HKR,defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
 HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
 HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
 HKR,NDI\params\PSMode\enum,4,,%POWER_SAVE_AUTO_DYN_STR%
 HKR,NDI\params\PSMode\enum,5,,%POWER_SAVE_AUTO_MAX_STR%
 HKR,NDI\params\PSMode,optional,0,1
 
;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 WLAN_DRIVER.copy      = 11 ; Win9x=%windir%\system
 WLAN_DRIVER.copy.ME   = 11 ; Win9x=%windir%\system
 WLAN_DRIVER.copy.NT   = 12 ; Win2k=%windir%\system32\drivers
 WLAN_FWDCB.copy      	= 11 ; Win9x=%windir%\system
 WLAN_FWDCB.copy.ME   	= 11 ; Win9x=%windir%\system
 WLAN_FWDCB.copy.NT  	= 12 ; Win2k=%windir%\system32\drivers
 WLAN_DOM.copy		= 10 ; %windir% all OS

[WLAN_NDI.copy]

[WLAN_NDI.copy.ME]

[WLAN_COINSTALL.copy.NT]

[WLAN_DRIVER.copy]
 WLANDCB.sys

[WLAN_DRIVER.copy.ME]
 WLANDCB.sys

[WLAN_DRIVER.copy.NT]
 WLANDCB.sys

[WLAN_FWDCB.copy]
 WLANDCB.arm

[WLAN_FWDCB.copy.ME]
 WLANDCB.arm

[WLAN_FWDCB.copy.NT]
 WLANDCB.arm

[WLAN_APPLET.copy]

[WLAN_APPLET.copy.ME]

[WLAN_APPLET.copy.NT]


[WLAN_DOM.copy]
 WLANDOM.ini

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
 WLANDCB.sys           = 1
 WLANDCB.arm           = 1
 WLANDOM.ini           = 1

[SourceDisksFiles.ME]   ; WinMe
 WLANDCB.sys           = 1
 WLANDCB.arm           = 1
 WLANDOM.ini           = 1

[SourceDisksFiles.X86]  ; Win2k/Xp
 WLANDCB.sys           = 1
 WLANDCB.arm           = 1
 WLANDOM.ini           = 1


;###############################################################################
[Strings]
;String ID              = String Text
;---------                -----------
 VER_VENDOR_STR         = "EagleTec"
 VER_VENDOR_NAME_STR    = "EagleTec"

 
 WLAN_SERVICE_DISPLAY_DCB = "EagleTec WG-2000 IEEE 802.11g Wireless LAN CardBus Driver"
 
 INSTALL_DISK_STR       = "EagleTec WG-2000 IEEE 802.11g Wireless LAN Install Disk"

 ADHOC_DEMO_STR          = "Adhoc Demo Mode"
 SHORT_PREAM_STR         = "Preamble Mode"
 RTSTHRESH_STR           = "RTS Threshold"
 FRAGTHRESH_STR          = "Fragmentation Threshold"
 AUTHENT_TYPE_STR        = "Authentication Algorithm"
 LISTENINTERVAL_STR      = "Listen Interval"
 POWER_SAVE_STR          = "Power Save Mode"
 POWER_SAVE_OFF_STR      = "Disabled"
 POWER_SAVE_DYN_STR      = "Dynamic"
 POWER_SAVE_MAX_STR      = "Maximum"
 POWER_SAVE_AUTO_DYN_STR = "Auto Dynamic"
 POWER_SAVE_AUTO_MAX_STR = "Auto Maximum"
 LOAD_FIRMWARE_STR       = "Firmware Download"
 SHORT_RETRY_STR         = "Short Retry Limit"
 LONG_RETRY_STR          = "Long Retry Limit"
 CHANNEL_STR             = "Channel"
 DATARATES_STR           = "Data Rate"
 DATARATES_AUTO          = "Fully Automatic"
 ALSR_STR                = "Auto Long Slot Reassociation"
 11D_MODE				 = "11D Mode"	
 NITRO_MODE              = "Nitro Mode"
 ESSID_Str				= "ssid"
 NET_WORK_TYPE			= "Network Type"

 DCB_DESC_STR            = "EagleTec WG-2000 IEEE 802.11g Wireless LAN CardBus Adapter"



