
[netcard]
;   key = description, MSID, type, media, mode, install, protini, style

ATNIC="Allied Telesis AT-2450/270x Series",000,ndis,ethernet,real,ATNIC,ATNIC_NIF

[ATNIC]
devdir=?:atinic.dos
device=atinic.dos,@devdir\atinic.dos

[ATNIC_NIF]
DRIVERNAME=ATINIC$
param=SPEED_DUPLEX,"Speed/Duplex",text,"0,1,2,3,4,5",5,0x30
;0=Auto, 1=100H, 2=100F, 3=10H, 4=10F, 5=Hardware
param=PORTIO,"I/O ACCESS",text,"0,1",0,0x30
;0=Memory Mapped I/O, 1=Port I/O