
[version]
Signature="$WINDOWS NT$"
Class=hdc
ClassGuid={4D36E96A-E325-11CE-BFC1-08002BE10318}
Provider=%AMD%

DriverVer=10/11/2007,5.1.0.8

;32x86
[SourceDisksNames]
1 = %DiskDesc%
[SourceDisksFiles]
amdide.sys  = 1

[DestinationDirs]
DefaultDestDir = 12

[Manufacturer]
%AMD%=AMD_HDC

[AMD_HDC]
;SB700
;%SATA_TO_IDE% = amdide_Inst,PCI\VEN_1002&DEV_4390   
;SB600
%SATA_TO_IDE% = amdide_Inst,PCI\VEN_1002&DEV_4380   
;SB450/SB460
;%SATA_TO_IDE% = amdide_Inst,PCI\VEN_1002&DEV_437A   
;SB450/SB460
;%SATA_TO_IDE% = amdide_Inst,PCI\VEN_1002&DEV_4379   
;SB700
;%PCI_IDE% = amdide_Inst,PCI\VEN_1002&DEV_439C     
;SB600  
;%PCI_IDE% = amdide_Inst,PCI\VEN_1002&DEV_438C       
 ;SB450/SB460
;%PCI_IDE% = amdide_Inst,PCI\VEN_1002&DEV_4376      

[amdide_Inst]
CopyFiles = @amdide.sys

[amdide_Inst.Services]
AddService = amdide, %SPSVCINST_ASSOCSERVICE%, amdide_Service_Inst

[amdide_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
LoadOrderGroup = System Bus Extender
ServiceBinary  = %12%\amdide.sys

[ControlFlags]
ExcludeFromSelect=*

[Strings]
AMD         = "Advanced Micro Devices"
SATA_TO_IDE = "AMD SATA Controller(Native IDE Mode)"
PCI_IDE     = "AMD PCI IDE Controller"
DiskDesc    = "Installation Disk for AMD PCI SATA/IDE Controller"


;*******************************************
;Handy macro substitutions (non-localizable)
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1


