;/*++
;
;Copyright (c) 2007 NETGEAR Communications, Incorporated All Rights Reserved
;
;Module Name:
;
;   wn311b.inf
;
;Abstract:
;    INF file for installing NETGEAR RangeMax(tm) Next Wireless Notebook Adapter
;
;--*/

[version]
	Signature	= "$Windows NT$"		; Combined Win9x/Win2k inf
	Class=Net
	ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
	Provider	= %NetGear%
	Compatible	= 1
DriverVer=02/20/2008, 4.170.75.0
	CatalogFile=wn511b.CAT
	

[Manufacturer]
	%NetGear% = NETGEAR

[ControlFlags] 
	ExcludeFromSelect = *

[NETGEAR]
	
        %NTGR_DeviceDesc% = NTGR,  PCI\VEN_14E4&DEV_4329&SUBSYS_F03014E4
        %NTGR_Devicespec% = NTGR,  PCI\VEN_14E4&DEV_4329&SUBSYS_7B001385

;-----------------------------------------------------------------
; Win2k specific
;


[NTGR.NT]
	
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX.reg, BCM43XX.brcm.reg, common.reg, g.options.reg
	DelReg          = common.delreg, rate.delreg
	CopyFiles	= BCM43XX.files.NT


[NTGR.NT.Services]
	AddService = BCM43XX, 2, BCM43XX.Service, common.EventLog


[BCM43XX.reg]
	; Ndis Info
	; Interfaces
	HKR,	Ndi\Interfaces,	UpperRange,	,	"ndis5"
	HKR,	Ndi\Interfaces,	LowerRange,	,	"ethernet"

[BCM43XX.brcm.reg]
	HKR,	Ndi,	HelpText,		,	%BCM43XX_HELP%
	HKR,	Ndi,	Service,		0,	"BCM43XX"

[BCM43XX.Service]
	DisplayName	= %BCM43XX_Service_DispName%
	ServiceType	= 1			; %SERVICE_KERNEL_DRIVER%
	StartType	= 3			; %SERVICE_DEMAND_START%
	ErrorControl	= 1			; %SERVICE_ERROR_NORMAL%
	ServiceBinary	= %12%\wn511b.sys
	LoadOrderGroup	= NDIS

[common.EventLog]
	AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
	HKR,	,	EventMessageFile,	0x00020000,	"%%SystemRoot%%\System32\netevent.dll"
	HKR,	,	TypesSupported,		0x00010001,	7

[BCM43XX.files.NT]
	wn511b.sys,,,6

;-----------------------------------------------------------------
; Both Win9x & Win2k
;

[common.delreg]
	HKR, Ndi\params\IBSSGMode\enum, "1"
	HKR, Ndi\params\RoamPref
        HKR, Ndi\params\AssocPref
	HKR, Ndi\params\Locale
	HKR,,Locale
	HKR, Ndi\params\RoamTrigger
	HKR,,RoamTrigger
	HKR, Ndi\params\MixedCell
	HKR,,WME

[rate.delreg]
	HKR, Ndi\params\Rate
	HKR, Ndi\params\RateA

[common.reg]
             
	HKR, ,"EnableSoftAP", 0, "0"
	HKR, ,"EnableAutoConnect", 0, "0"
	HKR,	Ndi\params\Country, ParamDesc,	0,	%Location%
	HKR,	Ndi\params\Country, type,		0,	"enum"

	HKR,	Ndi\params\Country\enum, "AU",	0,	%Australia%

	HKR,	Ndi\params\Country\enum, "BR",	0,	%Brazil%

	HKR,	Ndi\params\Country\enum, "CA",	0,	%Canada%

	HKR,	Ndi\params\Country\enum, "CN",	0,	%China%

	HKR,	Ndi\params\Country\enum, "FR",	0,	%France%

	HKR,	Ndi\params\Country\enum, "IL",	0,	%Israel%

	HKR,	Ndi\params\Country\enum, "JP",	0,	%Japan%

	HKR,	Ndi\params\Country\enum, "MX",	0,	%Mexico%

	HKR,	Ndi\params\Country\enum, "ZA",	0,	%SouthAfrica%

	HKR,	Ndi\params\Country\enum, "GB",	0,	%UnitedKingdom%

	HKR,	Ndi\params\Country\enum, "US",	0,	%UnitedStates%

	HKR,	Ndi\params\Country,	default,, 	"US"


	HKR,	Ndi\params\RadioState, ParamDesc,	0,	%RadioEnableDisable%
	HKR,	Ndi\params\RadioState, type,		0,	"enum"
	HKR,	Ndi\params\RadioState\enum, "1",		0,	%Disabled%
	HKR,	Ndi\params\RadioState\enum, "0",		0,	%Enabled%
	HKR,    Ndi\params\RadioState,default,,"0"	

	HKR,	Ndi\params\PwrOut, ParamDesc,	0,	%PowerOutput%
	HKR,	Ndi\params\PwrOut, type,		0,	"enum"
	HKR,	Ndi\params\PwrOut\enum, "100",	0,	%P100%
	HKR,	Ndi\params\PwrOut\enum, "50",	0,	%P50%
	HKR,	Ndi\params\PwrOut\enum, "25",	0,	%P25%
        HKR,	Ndi\params\PwrOut\enum, "12",	0,	%P125%
        HKR,	Ndi\params\PwrOut\enum, "5",	0,	%PLowest%
	HKR,	Ndi\params\PwrOut,default,,"100"


               HKR,					,"FrameBursting",	0,	"1"
   ;            HKR,	                                                                ,"Country",	0, 	"US"
                HKR,					,"LanExpress",	0,	"BR00"
	HKR,					,"WEP",	0,	""
	HKR,					,"NetworkType",	0,	"-1"
	HKR,					,"SSID",	0,	""

	;HKR,					,"gpio0",	0,	"-1"
	;HKR,					,"gpio1",	0,	"-1"
	;HKR,					,"gpio2",	0,	"-1"
	;HKR,					,"gpio3",	0,	"-1"
                HKR,					,"ledbh0",	0,	"10"
                HKR,					,"ledbh1",	0,	"-1"
                HKR,					,"ledbh2",	0,	"-1"
                HKR,					,"ledbh3",	0,	"-1"
                HKR,					,"leddc",	0,	"0"               




        HKR,					,"EFCEnable",		0,	"0"

	HKR,					,"ledblinkslow",	0,	"-1"
	HKR,					,"ledblinkmed",	0,	"-1"
	HKR,					,"ledblinkfast",	0,	"-1"
                
	HKR,					,"LegacyProbe",	0,	"0"

	;HKR,					,"gpiotimerval",	0,	"0"

	HKR,					,"scan_channel_time",	0,	"-1"
	HKR,					,"scan_unassoc_time",	0,	"-1"
	HKR,					,"scan_home_time",		0,	"-1"
	HKR,					,"scan_passes",			0,	"-1"

	HKR,					,"BadFramePreempt",		0,	"0"

	HKR,					,"Interference_Mode",		0,	"3"

	HKR,					,"ccx_rm",			0,	"1"
	HKR,					,"ccx_rm_limit",		0,	"300"


              HKR,					,"Afterburner",	0,	"0"
             HKR,					,"antdiv",	0,	"-1"
 HKR,					,"ApCompatMode",	0,	"0"
 HKR,					,"BTCoexist",	0,	"0"
 HKR,					,"Chanspec",	0,	"11"
 HKR,					,"frag",	0,	"2346"
 HKR,					,"IBSSAllowed",	0,	"1"
 HKR,					,"IBSSMode",	0,	"0"
 HKR,					,"IBSSGProtection",	0,	"2"
 HKR,					,"IBSSLink",	0,	"1"
 HKR,					,"LOM",	0,	"0"
 HKR,					,"Managed",	0,	"1"
 HKR,					,"MixedCell",	0,	"0"
 HKR,					,"MPC",	0,	"1"
 HKR,					,"PowerSaveMode",	0,	"2"
 HKR,					,"Rate",	0,	"0"
 HKR,					,"RoamDelta",	0,	"1"
 HKR,					,"rts",	0,	"2347"
 HKR,					,"ssid_auto_promote",	0,	"0"
 HKR,					,"vlan_mode",	0,	"-1"
 HKR,					,"WZCCoexist",	0,	"0"
 HKR,					,"RoamTrigger",	0,	"0"
 HKR,					,"mimo_antsel",	0,	"0"


; add for netgear to upgrade the software
 HKR,					,"SoftwareDate",	0,	"00-00-0000"
 HKR,					,"SoftwareVersion",	0,	"00.00.00.00"


[g.options.reg]

	HKR,	Ndi\params\PLCPHeader, ParamDesc,	0,	%BSSPLCPHeader%
	HKR,	Ndi\params\PLCPHeader, type,		0,	"enum"
	HKR,	Ndi\params\PLCPHeader\enum, "-1",	0,	%Long%
	HKR,	Ndi\params\PLCPHeader\enum, "0",	0,	%AutoShortLong%
	HKR,	Ndi\params\PLCPHeader,default,,"0"


[DestinationDirs]
	DefaultDestDir=11
	BCM43XX.files.NT = 12


[SourceDisksNames]
	1=%BCM43XX_DiskName%,,

[SourceDisksFiles]
	wn511b.SYS=1
	

[strings]
NTGR_Devicespec="RangeMax(tm) NEXT Wireless Notebook Adapter WN511B"
NetGear="NETGEAR"
BCM430B_DeviceDesc="RangeMax(tm) NEXT Wireless Notebook Adapter WN511B"
NTGR_DeviceDesc="RangeMax(tm) NEXT Wireless Notebook Adapter WN511B"
BCM430A_DeviceDesc="RangeMax(tm) NEXT Wireless Notebook Adapter WN511B"
BCM430M_DeviceDesc="RangeMax(tm) NEXT Wireless Notebook Adapter WN511B"
BCM43XX_HELP="The NETGEAR 802.11 Network Adapter provides wireless local area networking."
BCM43XX_Service_DispName="NETGEAR WN511B Wireless Adapter Service"
BCM43XX_DiskName="NETGEAR Wireless Adapter Driver Disk"
54gAuto="54g - Auto"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="802.11b Preamble"
BlueToothCollaboration="Bluetooth Collaboration"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g(tm) Mode"
IBSS54gtmProtectionMode="IBSS 54g(tm) Protection Mode"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Transmit Power"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio On/Off"
Rate="Rate"
RoamingDecision="Roaming Decision"
Usebestrate="Use best rate"
XPress_Technology="XPress (TM) Technology"
Location="Regional Domain"
Fast="Fast"
MiminumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WMM"
Afterburner="Afterburner"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"
Manage_Wireless_Settings="Manage Wireless Settings"
DisableRadioUponWiredConnection="Disable Upon Wired Connect"
SSIDAutoPromote="SSID Autopromote"
IBSSChannelNumber="WZC IBSS Channel Number"
IbssAllowed="IBSS Allowed"
Loose_11h_and_11d="Loose 11h+d"
Loose_11h="Loose 11h"
Strict_11h="Strict 11h"
MixedCell="Mixed Cell Support"
vlan_mode="VLAN Priority Support"
Default              = "Default"
UnitedStates         = "United States"
SouthAfrica	     = "Africa"
Australia  	     = "Australia"
China                = "Asia"
Canada		     = "Canada"
UnitedKingdom	     = "Europe"
France		     = "France"
Israel		     = "Israel"
Mexico		     = "Mexico"
Japan		     = "Japan"
Brazil       	     = "Sourth America"
P100 = "100%"
P50  ="50%"
P25  ="25%"
P125 ="12.5%"
PLowest ="Lowest"