;------------------------------------------------------------------------
;
;   Copyright and Disclaimer:
;
;       ---------------------------------------------------------------
;       This software is provided "as is" without warranty of any kind,
;       either expressed or implied, including but not limited to the
;       implied warranties of merchantability and/or fitness for a
;       particular purpose.
;
;       Copyright (c) 1999-2000 Conexant Systems, Inc.
;       All Rights Reserved.
;       ---------------------------------------------------------------
;
;
;   Abstract:
;
;       This is the tuner driver inf file.
;
;------------------------------------------------------------------------

[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider="Conexant"
DriverVer=05/10/2005,4.0.102.0
CatalogFile.ntx86=cx88tune.cat

[Manufacturer]
"Conexant"=Conexant

[SourceDisksNames]
1="Conexant Cx23880 Drivers",,,""

[SourceDisksFiles]
cx88tune.sys=1

[Conexant]
;Philips NTSC
%CXTUNE.DeviceDescP%     = CXTUNE.Philips,	STREAM\CXTUNE.VEN_14F1.Philips
%CXTUNE.DeviceDescP%	 = CXTUNE.Philips,   	STREAM\CXTUNE.VEN_14F1.Philips#PCI#VEN_14F1&DEV_8800&SUBSYS_FF7F1642

;TCL2002 MI-3 PAL D/K & I
%CXTUNE.DeviceDescTCLMI3% = CXTUNE.TCL2002MI3, 	STREAM\CXTUNE.VEN_14F1.TCL2002MI3
%CXTUNE.DeviceDescTCLMI3% = CXTUNE.TCL2002MI3, 	STREAM\CXTUNE.VEN_14F1.TCL2002MI3#PCI#VEN_14F1&DEV_8800&SUBSYS_43561642


[CXTUNE.Philips]
Include  =  ks.inf, kscaptur.inf
Needs    =  KS.Registration,KSCAPTUR.Registration.NT
AddReg   =  CXTUNE.addreg,philips.addreg
CopyFiles=  CXTUNE.CopyDrivers


[CXTUNE.TCL2002MI3]
Include  =  ks.inf, kscaptur.inf
Needs    =  KS.Registration,KSCAPTUR.Registration.NT
AddReg   =  CXTUNE.addreg,TCL2002MI3.addreg
CopyFiles=  CXTUNE.CopyDrivers

[DestinationDirs]
CXTUNE.CopyDrivers=10,system32\drivers

[CXTUNE.CopyDrivers]
cx88tune.sys

[CXTUNE.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,CX88TUNE.sys
HKR,,OkToHibernate,3,01
HKR,,PageOutWhenUnopened,3,00


[Philips.AddReg]
HKR,"DriverData","TunerBrand",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xc0, 0x00, 0x00, 0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","TunerMode",0x0010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","TunerInput",0x00010001, 0x00, 0x00, 0x00, 0x00

[TCL2002MI3.AddReg]
HKR,"DriverData","TunerBrand",0x00010001, 0x08, 0x00, 0x00, 0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xc0, 0x00, 0x00, 0x00
HKR,"DriverData","TunerType",0x00010001, 0x12, 0x00, 0x00, 0x00
HKR,"DriverData","TunerMode",0x0010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","TunerInput",0x00010001, 0x00, 0x00, 0x00, 0x00

[TvTuner]
AddReg=TvTuner.AddReg

[TvTuner.AddReg]
HKR,,CLSID,,{266EEE40-6C63-11cf-8A03-00AA006ECB65}
HKR,,FriendlyName,,%CXTUNE.TUNER%

[CXTUNE.Philips.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[CXTUNE.TCL2002MI3.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[CXTUNE.Philips.Services]
AddService = CXTUNE,0x00000002,CXTUNE.ServiceInstall

[CXTUNE.TCL2002MI3.Services]
AddService = CXTUNE,0x00000002,CXTUNE.ServiceInstall


[CXTUNE.ServiceInstall]
DisplayName   = %CXTUNE.DeviceDesc%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_AUTO_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %10%\system32\drivers\CX88TUNE.sys

[Strings]
CXTUNE.DeviceDesc         = "Conexant 2388x Tuner"
CXTUNE.DeviceDescP        = "Conexant 2388x Tuner (FM1236 NTSC)"
CXTUNE.DeviceDescTCLMI3   = "Conexant 2388x Tuner (PAL D/K&I)"

CXTUNE.Tuner              = "Conexant 2388x Tuner"

SERVICE_KERNEL_DRIVER=1
SERVICE_AUTO_START=2
SERVICE_ERROR_NORMAL=1
