;*****************************************************************************
;
;                    Copyright 2000 - 2006
;
;  Supported Platform: 32 bit, 64 bit (except IA64)
;  Supported OS:       Windows XP, Windows Vista
; 
;*****************************************************************************

[Version]
signature           = "$CHICAGO$" ;All Windows OS
Class               = MEDIA
ClassGUID           = {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider            = %PROVIDER%
CatalogFile.NTx86   = LVHybrid.cat
CatalogFile.NTAMD64 = LVHybr64.cat

;---------------------mm/dd/yyyy,version--------------------
DriverVer           = 03/22/2007,23.35.01.002
;                   -> Release
;-----------------------------------------------------------



[Manufacturer]
%PROVIDER%  = Lifeview, NTx86, NTAMD64

;---> 32 BIT SUPPORT <---
[Lifeview.NTx86]
;*****************************LVBOARD********************************
;******** CR002A ***  NO FM
%CR002A_30.DeviceDesc% = CR002A_30.NTx86,PCI\VEN_1131&DEV_7130&SUBSYS_002a5168
%CR002A_33.DeviceDesc% = CR002A_33.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_002a5168
%CR002A_34.DeviceDesc% = CR002A_34.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_002a5168
;******** CR002B ***
%CR002B_30.DeviceDesc% = CR002B_30.NTx86,PCI\VEN_1131&DEV_7130&SUBSYS_002b19d3
%CR002B_33.DeviceDesc% = CR002B_33.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_002b19d3
%CR002B_34.DeviceDesc% = CR002B_34.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_002b19d3
;******** CR002C ***
%CR002c_30.DeviceDesc% = CR002c_30.NTx86,PCI\VEN_1131&DEV_7130&SUBSYS_002c19d3
%CR002c_33.DeviceDesc% = CR002c_33.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_002c19d3
%CR002c_34.DeviceDesc% = CR002c_34.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_002c19d3

;******** CR0138 *** NO FM
%P30_30.DeviceDesc% = P30_30.NTx86,PCI\VEN_1131&DEV_7130&SUBSYS_01385168
%P34_34.DeviceDesc% = P34_34.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_01385168

;******** CR0016 ***
%CR0016_33.DeviceDesc% = CR0016_33.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_001619d3
%P35PRO_33.DeviceDesc% = CR0016_33.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_03145168
;******** P35_33 *** NO FM
%P35_33.DeviceDesc% = P35_33.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_13145168



;---> 64 BIT SUPPORT <---
[Lifeview.NTAMD64]
;******** CR002A ***  NO FM
%CR002A_30.DeviceDesc% = CR002A_30.NTAMD64,PCI\VEN_1131&DEV_7130&SUBSYS_002a5168
%CR002A_33.DeviceDesc% = CR002A_33.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_002a5168
%CR002A_34.DeviceDesc% = CR002A_34.NTAMD64,PCI\VEN_1131&DEV_7134&SUBSYS_002a5168
;******** CR002B ***
%CR002B_30.DeviceDesc% = CR002B_30.NTAMD64,PCI\VEN_1131&DEV_7130&SUBSYS_002b19d3
%CR002B_33.DeviceDesc% = CR002B_33.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_002b19d3
%CR002B_34.DeviceDesc% = CR002B_34.NTAMD64,PCI\VEN_1131&DEV_7134&SUBSYS_002b19d3
;******** CR002C ***
%CR002c_30.DeviceDesc% = CR002c_30.NTAMD64,PCI\VEN_1131&DEV_7130&SUBSYS_002c19d3
%CR002c_33.DeviceDesc% = CR002c_33.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_002c19d3
%CR002c_34.DeviceDesc% = CR002c_34.NTAMD64,PCI\VEN_1131&DEV_7134&SUBSYS_002c19d3

;******** CR0138 *** NO FM
%P30_30.DeviceDesc% = P30_30.NTAMD64,PCI\VEN_1131&DEV_7130&SUBSYS_01385168
%P34_34.DeviceDesc% = P34_34.NTAMD64,PCI\VEN_1131&DEV_7134&SUBSYS_01385168

;******** CR0016 ***
%CR0016_33.DeviceDesc% = CR0016_33.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_001619d3
%P35PRO_33.DeviceDesc% = CR0016_33.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_03145168
;******** P35_33 *** NO FM
%P35_33.DeviceDesc% = P35_33.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_13145168


[SourceDisksNames]
1 = %INSTALLATION_DISK%,,


[SourceDisksFiles]
LVHybrid.sys           = 1
LVHybr64.sys           = 1
34CoInstaller.dll      = 1


[DestinationDirs]
SectionX32.CopyDll.NTx86      = 11
SectionX64.CopyDll.NTAMD64    = 11
SectionX32.CopyDriver.NTx86   = 10,system32\drivers
SectionX64.CopyDriver.NTAMD64 = 10,system32\drivers


[SectionX32.CopyDll.NTx86]
34CoInstaller.dll


[SectionX64.CopyDll.NTAMD64]


[SectionX32.CopyDriver.NTx86]
LVHybrid.sys


[SectionX64.CopyDriver.NTAMD64]
LVHybr64.sys


;=======================================================-------------------------------------------------------
;======================================
;
;       Initialization Entries
;
;======================================
;=====LV=====
;********  x32bit ***
;******** CR002A PROTEUS x32 ***
;-------------30----------
[CR002A_30.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[CR002A_30.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, CR002A_34.AddReg

[CR002A_30.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86
;------------33----------CR002A_34.AddReg??-
[CR002A_33.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[CR002A_33.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, CR002A_34.AddReg

[CR002A_33.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86
;-----------34------------
[CR002A_34.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[CR002A_34.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, CR002A_34.AddReg

[CR002A_34.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86
;******** CR002B PROTEUS x32 ***
;-------------30----------
[CR002B_30.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[CR002B_30.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, CR002B_34.AddReg

[CR002B_30.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86
;------------33----------CR002B_34.AddReg??-
[CR002B_33.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[CR002B_33.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, CR002B_34.AddReg

[CR002B_33.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86
;-----------34------------
[CR002B_34.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[CR002B_34.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, CR002B_34.AddReg

[CR002B_34.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86

;******** CR002C_PROTEUS x32 ***************
;-----------30------------
[CR002C_30.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[CR002C_30.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, CR002C_34.AddReg

[CR002C_30.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86

;-----------33------------
[CR002C_33.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[CR002C_33.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, CR002C_34.AddReg

[CR002C_33.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86

;-----------34------------
[CR002C_34.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[CR002C_34.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, CR002C_34.AddReg

[CR002C_34.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86

;******** P34_34+***************

;-----------30------------
[P30_30.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[P30_30.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, P30_30.AddReg 

[P30_30.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86

;-----------34------------
[P34_34.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[P34_34.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, P34_34.AddReg 

[P34_34.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86




;******** P35_33***************
;-----------34------------
[P35_33.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[P35_33.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, P35_33.AddReg

[P35_33.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86

;******** CR0016_33***************
[CR0016_33.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[CR0016_33.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, CR0016_33.AddReg

[CR0016_33.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86






;=====LV=============================================================
;********  x64bit ***
;******** CR002A PROTEUS x64 ***
;-------------30----------
[CR002A_30.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[CR002A_30.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, CR002A_34.AddReg

[CR002A_30.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64
;------------33----------CR002A_34.AddReg??-
[CR002A_33.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[CR002A_33.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, CR002A_34.AddReg

[CR002A_33.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64
;-----------34------------
[CR002A_34.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[CR002A_34.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, CR002A_34.AddReg

[CR002A_34.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64
;******** CR002B PROTEUS x64 ***
;-------------30----------
[CR002B_30.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[CR002B_30.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, CR002B_34.AddReg

[CR002B_30.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64
;------------33----------CR002B_34.AddReg??-
[CR002B_33.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[CR002B_33.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, CR002B_34.AddReg

[CR002B_33.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64
;-----------34------------
[CR002B_34.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[CR002B_34.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, CR002B_34.AddReg

[CR002B_34.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64

;******** CR002C_PROTEUS x32 ***************
;-----------30------------
[CR002C_30.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[CR002C_30.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, CR002C_34.AddReg

[CR002C_30.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64

;-----------33------------
[CR002C_33.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[CR002C_33.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, CR002C_34.AddReg

[CR002C_33.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64

;-----------34------------
[CR002C_34.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[CR002C_34.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, CR002C_34.AddReg

[CR002C_34.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64

;******** P34_34+***************

;-----------30------------
[P30_30.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[P30_30.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, P30_30.AddReg 

[P30_30.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64
;-----------34------------
[P34_34.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[P34_34.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, P34_34.AddReg 

[P34_34.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64




;******** P35_33***************
;-----------34------------
[P35_33.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[P35_33.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, P35_33.AddReg

[P35_33.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64

;******** CR0016_33***************
[CR0016_33.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[CR0016_33.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, CR0016_33.AddReg

[CR0016_33.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64



;=======================================================-------------------------------------------------------
;******** GENERAL x32 ***
[SectionX32.ServiceInstall.NTx86]
DisplayName   = %DISPLAY_NAME%
Description   = %SERVICE_DESCRIPTION%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_IGNORE%
ServiceBinary = %12%\LVHybrid.sys


;******** GENERAL x64 ***
[SectionX64.ServiceInstall.NTAMD64]
DisplayName   = %DISPLAY_NAME%
Description   = %SERVICE_DESCRIPTION%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_IGNORE%
ServiceBinary = %12%\LVHybr64.sys

;=======================================================-------------------------------------------------------

;======================================
;
;           Registry Entries
;
;======================================
; [StartName=driver-object-name]
; [AddReg=add-registry-section[, add-registry-section] ...]
; [DelReg=del-registry-section[, del-registry-section] ...]
; [BitReg=bit-registry-section[,bit-registry-section] ...]
; [LoadOrderGroup=load-order-group-name]
; [Dependencies=depend-on-item-name[,depend-on-item-name]...]

;
;******** General DLL Registry Entries ***
;

[SectionX32.DllAddReg.NTx86]
HKR,,CoInstallers32,0x00010000,"34CoInstaller.dll, CoInstallerEntry"


[SectionX64.DllAddReg.NTAMD64]


;
;******** General Driver Registry Entries ***
;

[SectionX32.AddReg.NTx86]

HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,LVHybrid.sys

; --- Registry Entries For Audio Capture ---
HKR,,Driver,,LVHybrid.sys
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"

HKR,Drivers,SubClasses,,"wave,mixer"
HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\wave\wdmaud.drv,Description,,%LVHybrid.AudioDeviceDesc%
HKR,Drivers\mixer\wdmaud.drv,Description,,%LVHybrid.AudioDeviceDesc%

; add audio input and output pinnames
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audioinput"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_ITU_PIN%,"Name",,"Analog ITU Video"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_I2S_PIN%,"Name",,"I2S Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_CAP_PIN%,"Name",,"~Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_CAP_PIN%,"Name",,"~Capture"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_PRE_PIN%,"Name",,"~Preview"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_AES_PIN%,"Name",,"MPEG Audio ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_VES_PIN%,"Name",,"MPEG Video ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_PS_PIN%,"Name",, "MPEG2 Program"

;===AMD64===============
[SectionX64.AddReg.NTAMD64]

HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,LVHybr64.sys

; --- Registry Entries For Audio Capture ---

HKR,,Driver,,LVHybr64.sys
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"

HKR,Drivers,SubClasses,,"wave,mixer"
HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\wave\wdmaud.drv,Description,,"LVHybrid Audio Capture Device"
HKR,Drivers\mixer\wdmaud.drv,Description,,"LVHybrid Audio Capture Device"


; add audio input and output pinnames
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audioinput"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_ITU_PIN%,"Name",,"Analog ITU Video"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_I2S_PIN%,"Name",,"I2S Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_CAP_PIN%,"Name",,"~Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_CAP_PIN%,"Name",,"~Capture"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_PRE_PIN%,"Name",,"~Preview"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_AES_PIN%,"Name",,"MPEG Audio ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_VES_PIN%,"Name",,"MPEG Video ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_PS_PIN%,"Name",, "MPEG2 Program"


;
;******** Board - Specific Registry Entries ***
;
;=======================================================-------------------------------------------------------
;---- CR002A ----
[CR002A_34.AddReg]
; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%LVHYBRID_CUSTOM_TUNERNAME%

; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters", "SmallXBar",0x00010001,0x01

;EEROM
HKR, "I2C Devices", "Force Registry Settings",0x00010001,0x01

;video mappings 
HKR, "VideoDecoder", "Tuner Channel",0x00010001,0x01
HKR, "VideoDecoder", "CVBS Channel",0x00010001,0x03
HKR, "VideoDecoder", "SVHS Channel",0x00010001,0x08
HKR, "VideoDecoder", "FM Radio Channel",0x00010001,0xFF

;audio mappings
HKR, "AudioDecoder", "Tuner Channel",0x00010001,0x01
HKR, "AudioDecoder", "CVBS Channel",0x00010001,0x03
HKR, "AudioDecoder", "SVHS Channel",0x00010001,0x03
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,0x03

;XTAL setting
HKR, "AudioDecoder", "XTAL",0x00010001,0x01               ;Default = 32MHz
;9935 B/DFF DIFF
;gpio mappings
HKR, "GPIO", "Config",0x00010001,0x0000E000
HKR, "Audio", "GPIOAudioSwitch",0x00010001,0x01

;tuner settings
HKR, "I2C Devices", "Number of I2C Devices",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x39
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x86
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0xFF
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x20
;HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x0   ; Add. data #2
;HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x0   ; Add. data #3
;---- CR002B ----
[CR002B_34.AddReg]
; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%LVHYBRID_CUSTOM_TUNERNAME%

; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters", "SmallXBar",0x00010001,0x01

;EEROM
HKR, "I2C Devices", "Force Registry Settings",0x00010001,0x01

;video mappings 
HKR, "VideoDecoder", "Tuner Channel",0x00010001,0x01
HKR, "VideoDecoder", "CVBS Channel",0x00010001,0x03
HKR, "VideoDecoder", "SVHS Channel",0x00010001,0x08
HKR, "VideoDecoder", "FM Radio Channel",0x00010001,0xFF

;audio mappings
HKR, "AudioDecoder", "Tuner Channel",0x00010001,0x01
HKR, "AudioDecoder", "CVBS Channel",0x00010001,0x03
HKR, "AudioDecoder", "SVHS Channel",0x00010001,0x03
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,0x03

;XTAL setting
HKR, "AudioDecoder", "XTAL",0x00010001,0x01               ;Default = 32MHz
;9935 B/DFF DIFF
;gpio mappings
HKR, "GPIO", "Config",0x00010001,0x0000E000
HKR, "Audio", "GPIOAudioSwitch",0x00010001,0x01

;tuner settings
HKR, "I2C Devices", "Number of I2C Devices",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x36
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x86
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0xFF
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x30
;HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x0   ; Add. data #2
;HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x0   ; Add. data #3



;---- CR002C ----
[CR002C_34.AddReg]
; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%LVHYBRID_CUSTOM_TUNERNAME%

; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters", "SmallXBar",0x00010001,0x01

;EEROM
HKR, "I2C Devices", "Force Registry Settings",0x00010001,0x01

;video mappings 
HKR, "VideoDecoder", "Tuner Channel",0x00010001,0x01
HKR, "VideoDecoder", "CVBS Channel",0x00010001,0x03
HKR, "VideoDecoder", "SVHS Channel",0x00010001,0x08
HKR, "VideoDecoder", "FM Radio Channel",0x00010001,0xFF

;audio mappings
HKR, "AudioDecoder", "Tuner Channel",0x00010001,0x01
HKR, "AudioDecoder", "CVBS Channel",0x00010001,0x03
HKR, "AudioDecoder", "SVHS Channel",0x00010001,0x03
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,0x03

;XTAL setting
HKR, "AudioDecoder", "XTAL",0x00010001,0x01               ;Default = 32MHz
;9935 B/DFF DIFF
;gpio mappings
HKR, "GPIO", "Config",0x00010001,0x0000E000
HKR, "Audio", "GPIOAudioSwitch",0x00010001,0x01

;tuner settings
HKR, "I2C Devices", "Number of I2C Devices",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x37
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x86
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0xFF
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x30
;HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x0   ; Add. data #2
;HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x0   ; Add. data #3

;---- P30_30. ----
[P30_30.AddReg]
; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%LVHYBRID_CUSTOM_TUNERNAME%

; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters", "SmallXBar",0x00010001,0x01

;EEROM
HKR, "I2C Devices", "Force Registry Settings",0x00010001,0x01

;video mappings 
HKR, "VideoDecoder", "Tuner Channel",0x00010001,0x01
HKR, "VideoDecoder", "CVBS Channel",0x00010001,0x03
HKR, "VideoDecoder", "SVHS Channel",0x00010001,0x08
HKR, "VideoDecoder", "FM Radio Channel",0x00010001,0xFF

;audio mappings
HKR, "AudioDecoder", "Tuner Channel",0x00010001,0x03
HKR, "AudioDecoder", "CVBS Channel",0x00010001,0x03
HKR, "AudioDecoder", "SVHS Channel",0x00010001,0x03
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,0x03

;XTAL setting
HKR, "AudioDecoder", "XTAL",0x00010001,0x01               ;Default = 32MHz
;9935 B/DFF DIFF
;gpio mappings
HKR, "GPIO", "Config",0x00010001,0x0000E000
HKR, "Audio", "GPIOAudioSwitch",0x00010001,0x01

;tuner settings
HKR, "I2C Devices", "Number of I2C Devices",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x38
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x86
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0xFF
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x20
;HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x0   ; Add. data #2
;HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x0   ; Add. data #3


;---- P34_34. ----
[P34_34.AddReg]
; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%LVHYBRID_CUSTOM_TUNERNAME%

; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters", "SmallXBar",0x00010001,0x01

;EEROM
HKR, "I2C Devices", "Force Registry Settings",0x00010001,0x01

;video mappings 
HKR, "VideoDecoder", "Tuner Channel",0x00010001,0x01
HKR, "VideoDecoder", "CVBS Channel",0x00010001,0x03
HKR, "VideoDecoder", "SVHS Channel",0x00010001,0x08
HKR, "VideoDecoder", "FM Radio Channel",0x00010001,0xFF

;audio mappings
HKR, "AudioDecoder", "Tuner Channel",0x00010001,0x01
HKR, "AudioDecoder", "CVBS Channel",0x00010001,0x03
HKR, "AudioDecoder", "SVHS Channel",0x00010001,0x03
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,0x01

;XTAL setting
HKR, "AudioDecoder", "XTAL",0x00010001,0x01               ;Default = 32MHz
;9935 B/DFF DIFF
;gpio mappings
HKR, "GPIO", "Config",0x00010001,0x0000E000
HKR, "Audio", "GPIOAudioSwitch",0x00010001,0x01


;tuner settings
HKR, "I2C Devices", "Number of I2C Devices",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x38
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x86
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0xFF
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x20
;HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x0   ; Add. data #2
;HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x0   ; Add. data #3



;---- P35_33 ----
[P35_33.AddReg]
; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%LVHYBRID_CUSTOM_TUNERNAME%

; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters", "SmallXBar",0x00010001,0x01

;EEROM
HKR, "I2C Devices", "Force Registry Settings",0x00010001,0x01

;video mappings 
HKR, "VideoDecoder", "Tuner Channel",0x00010001,0x01
HKR, "VideoDecoder", "CVBS Channel",0x00010001,0x03
HKR, "VideoDecoder", "SVHS Channel",0x00010001,0x08
HKR, "VideoDecoder", "FM Radio Channel",0x00010001,0xFF

;audio mappings
HKR, "AudioDecoder", "Tuner Channel",0x00010001,0x01
HKR, "AudioDecoder", "CVBS Channel",0x00010001,0x03
HKR, "AudioDecoder", "SVHS Channel",0x00010001,0x03
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,0x01

;XTAL setting
HKR, "AudioDecoder", "XTAL",0x00010001,0x01               ;Default = 32MHz
;9935 B/DFF DIFF
;gpio mappings
HKR, "GPIO", "Config",0x00010001,0x0000E000

HKR, "Audio", "I2S Output",0x00010001,0x00

HKR, "Audio", "I2S2 Output",0x00010001,0x00
HKR, "Audio", "GPIOAudioSwitch",0x00010001,0x01

;tuner settings
HKR, "I2C Devices", "Number of I2C Devices",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x22
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0xFF
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x02
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x20
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x10   ; Add. data #2
;HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x0   ; Add. data #3


;---- CR0016_33 ----
[CR0016_33.AddReg]
; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%LVHYBRID_CUSTOM_TUNERNAME%

; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters", "SmallXBar",0x00010001,0x01

;EEROM
HKR, "I2C Devices", "Force Registry Settings",0x00010001,0x01

;video mappings 
HKR, "VideoDecoder", "Tuner Channel",0x00010001,0x01
HKR, "VideoDecoder", "CVBS Channel",0x00010001,0x03
HKR, "VideoDecoder", "SVHS Channel",0x00010001,0x08
HKR, "VideoDecoder", "FM Radio Channel",0x00010001,0xFF

;audio mappings
HKR, "AudioDecoder", "Tuner Channel",0x00010001,0x01
HKR, "AudioDecoder", "CVBS Channel",0x00010001,0x03
HKR, "AudioDecoder", "SVHS Channel",0x00010001,0x03
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,0x01

;XTAL setting
HKR, "AudioDecoder", "XTAL",0x00010001,0x01               ;Default = 32MHz
;9935 B/DFF DIFF
;gpio mappings
HKR, "GPIO", "Config",0x00010001,0x0000E000

HKR, "Audio", "I2S Output",0x00010001,0x00

HKR, "Audio", "I2S2 Output",0x00010001,0x00
HKR, "Audio", "GPIOAudioSwitch",0x00010001,0x01

;tuner settings
HKR, "I2C Devices", "Number of I2C Devices",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x22
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0xFF
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x02
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x30
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x10   ; Add. data #2
;HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x0   ; Add. data #3

;======================================
;
;           Strings Defines
;
;======================================

[Strings]
;-------------------------------
; Capture Filter Pin Name GUIDs
;-------------------------------
AVSTREAM_ANLG_AUDIO_IN_PIN   = "{7BB284B9-714D-493d-A101-B1B028E782BD}"
AVSTREAM_ANLG_AUDIO_OUT_PIN  = "{5582E657-E596-42b5-9DB3-541B27A2355F}"
AVSTREAM_ANLG_VIDEO_ITU_PIN  = "{82631A2E-403C-4581-A4B0-EC173D004410}"
AVSTREAM_ANLG_AUDIO_I2S_PIN  = "{C2E46358-F032-4d88-B802-06B59D162730}"
AVSTREAM_ANLG_VIDEO_CAP_PIN  = "{16FFBD0A-F770-4692-A2FF-DD394DFE9564}"
AVSTREAM_ANLG_VIDEO_PRE_PIN  = "{A19F6121-9CF7-4081-8053-256668FCBE1F}"
AVSTREAM_ANLG_AUDIO_CAP_PIN  = "{BA9E27B1-CF44-490e-8EAB-5F662E5FFE74}"
AVSTREAM_MPEG_AES_PIN        = "{9DEC84B9-BCEF-4aac-997E-43EDD0A2D6C7}"
AVSTREAM_MPEG_VES_PIN        = "{181CF87E-7741-47ba-8629-22347E03C64C}"
AVSTREAM_MPEG_PS_PIN         = "{DDA87B83-65DB-4aec-82D0-79FBE67D2BB6}"


;--------------------
; System Defines
;--------------------
SERVICE_BOOT_START       = 0x0
SERVICE_SYSTEM_START     = 0x1
SERVICE_AUTO_START       = 0x2
SERVICE_DEMAND_START     = 0x3
SERVICE_DISABLED         = 0x4

SERVICE_KERNEL_DRIVER    = 0x1
SERVICE_ERROR_IGNORE     = 0x0
SERVICE_ERROR_NORMAL     = 0x1
SERVICE_ERROR_SEVERE     = 0x2
SERVICE_ERROR_CRITICAL   = 0x3
FLG_REGSVR_DLLREGISTER   = 0x00000001


;***********************************************************
;                      !!! ATTENTION !!!
; Customer Strings:
;   The following strings MUST be changed, if the driver has
;   been customized, to not interfere with the original one.
;
;************************************************************

;--- Driver names for 32/64 bit OS ---
DRIVER_NAME_X32               = "LVHybrid.sys"
DRIVER_NAME_X64               = "LVHybr64.sys"

;--- Catalog file (signature) names for 32/64 bit OS ---
SIGNATURE_NAME_X32            = "LVHybrid.cat"
SIGNATURE_NAME_X64            = "LVHybr64.cat"

;--- Coinstaller DLL name for 32/64 bit OS ---
COINSTALLER_NAME_X32          = "34CoInstaller.dll"
;COINSTALLER_NAME_X64          = "3xCoInstX64.dll"

;--- Service names linked to the driver binary ---
SERVICE_NAME_X32              = "LVHybrid"
SERVICE_NAME_X64              = "LVHybr64"
SERVICE_DESCRIPTION           = "Lifeview 713x capture driver"

;--- Name displayed in the device manager ---
DISPLAY_NAME                  = "LVHybrid service"

;--- General names ---
PROVIDER                      = "Lifeview "
INSTALLATION_DISK             = "Lifeview Installation Disk"


;***********************************************************
;
; Generic Strings:
;   Board Description (-> Displayed within e.g. Graphedit)
;
;***********************************************************

;*** Specific Names ***
;-----------------
LVHybrid.AudioDeviceDesc       = "Lifeview SAA713x Audio Capture Device"

LVHYBRID_CUSTOM_TUNERNAME     = "713x"
;=========LV=====32/64========================
CR002A_30.DeviceDesc         = "FlyTV P34+"
CR002A_33.DeviceDesc         = "FlyTV P34+"
CR002A_34.DeviceDesc         = "FlyTV P34+"

CR002B_30.DeviceDesc         = "FlyTV Prime SPO 30"
CR002B_33.DeviceDesc         = "FlyTV Prime SPO 33"
CR002B_34.DeviceDesc         = "FlyTV Prime SPO 34"

CR002c_30.DeviceDesc         = "FlyTV Prime SPO 30"
CR002c_33.DeviceDesc         = "FlyTV Prime SPO 33"
CR002c_34.DeviceDesc         = "FlyTV Prime SPO 34"

P34_34.DeviceDesc             = "FlyTV P34+"
P30_30.DeviceDesc             = "FlyTV P30+"


CR0016_33.DeviceDesc         = "FlyTV P35 PRO SPO"

P35PRO_33.DeviceDesc         = "FlyTV P35 Pro"
P35_33.DeviceDesc            = "FlyTV P35"